Article: 46797 of rec.guns
From: amirza@bronze.ucs.indiana.edu (Anmar Caves)
Newsgroups: rec.guns
Subject: [RELOAD]FAQ:Beginning Reloading
Message-ID: <9308301656.AA22922@rutgers.edu>
Date: 31 Aug 93 00:11:20 GMT
Sender: magnum@mimsy.umd.edu
Organization: Indiana University
Lines: 540
Approved: gun-control@cs.umd.edu


My Adventures in Reloading

[Written a year after I started, and updated considerably since then.]
Henry E. Shaffer

  Having become interested in reloading, and over the past year
having started and gained some experience, I thought that I would 
share my experiences and ideas with the list.  Perhaps someone 
will gain from this, and perhaps someone with more knowledge 
will set me straight(er) on something.  I'm going to emphasize 
the .38 Special load - as that is the bulk of the handgun
reloading I've been doing.  (I would also like to thank the people 
on the net who have shared their ideas with me.  I have incorporated 
many of their comments in revising my original story.  I've reloaded 
for a number of pistol calibers by buying new dies and using the rest 
of what I already had.  Also I've reloaded for the rifle, and have 
found that most of the equipment and experience carry over.  The 
percentage savings is often greater when reloading for the rifle.)

  Before we get started, it is worth discussing - Why Reload?
Most of the information on reloading shows the savings by
comparing your costs vs. the retail price of a box of name brand 
new ammo.  This is ridiculous!  If you have the money to reload,
you have the money to buy a case at a time - and are probably
willing to buy reloads.  One reference I have compares the price 
of home reloads (for .357 Magnum) vs. a retail price of over 
$20/box.  The last case of .38 Special wadcutter reloads I 
purchased (i.e., 1,000 rounds) cost me $75 plus trading in 1,000 
empties.  So my bought ammo cost me $3.75/box net of brass.  I 
buy cast lead bullets, and then can reload a box for $2.75-$3.00 
in supplies.  (The price of both bought ammo and supplies has 
gone up since then, but the relationship between the two still is 
roughly the same.)  There is not enough margin there to pay for 
my equipment and time.  Casting lead bullets can save more money, 
especially if you can scrounge wheel weights or other sources of 
lead - but it takes even more time and equipment so I'm going to 
ignore this aspect of reloading.  The economics of reloading 
improve somewhat if you reload more than one caliber, and 
especially for rifle reloading.  The savings can be great when you 
want match grade rifle ammo which is not hard to do by handloading,
but which is quite expensive to buy.  Also, each person has to decide 
how hard they are willing to work to save what amount of money.  For
many people, even a small savings is worth the effort to reload, and
if they are shooting a less popular caliber than the .38 Special the
cost advantage of reloading will be further increased because of the
higher price or unavailability of commercial reloads.

  However, not everything I want to shoot is available, and
even if it was, I may not want to buy in case quantities.
(If you shoot a caliber for which reloads aren't available 
then you must compare with new prices - in case lots.)  In 
particular, I went looking for suitable ammunition to use
in a speedloader, because I wanted to practice for IPSC 
competition.  (Why anyone would want to shoot IPSC with a
.38 Special revolver is a topic I'll leave for a later day!)
I couldn't find lead round nose (LRN) .38 Special ammo 
anywhere in town.  There wasn't any jacketed round nose
available either - semiwadcutter was available, but it
doesn't slip into the cylinder as nicely.  I could have
ordered RN quite easily, but then I would be paying
considerably more than I cared to pay - that would be up in 
the $15 - $25/box range.  But even if I ordered that, I would 
have to take what is manufactured, and I also was wondering 
about somewhat heavier bullets (say in the 160-180 gr range) 
which can be reloaded but are essentially unavailable in 
factory ammo.  Also the thought of experimenting with
different loads for accuracy and to fit my style and preferences
was appealing.  (Silhouette shooters also often want heavier
bullets than are generally available in factory ammo.)

  All together, there was enough to get me to want to try -
especially if it wasn't too expensive to fiddle around a
bit.  (That's where the Lee Reloader press offer attracted
me - but that's getting ahead of the story.)  So given that
you want to try - here's what I recommend.

  First - read up on reloading.  The Hornady Reloading Manual
set (2 volumes) 4th ed. is an excellent reference for a
beginner since it has such good illustrations and a glossary.
Lyman's Reloading Handbook is another good first reference.  
It contains history, theory, how-to-do-it, and a large reference 
section giving suggested loads and data on quite an array of rifle 
and handgun calibers (with outline drawings and dimensions of 
cartridges.)  It is not very expensive, and it is a useful reference 
even if you are not going to reload.  RCBS has a less expensive 
brochure which is worth reading but it is much smaller.  (It is also
somewhat old and may not be easily available.)  The Sierra handbooks 
are excellent, but more advanced.  Most of the powder companies give 
free small handbooks which mostly have loading data - fine - but not 
much discussion and so not very good for beginners.  The Speer manual 
is also on a somewhat advanced advanced level.  The Nosler is oriented
towards hunting.

  There also are books which have much more discussion, lots of
photos, etc.  I particularly enjoyed The ABC's of Reloading by
Dean Grennell, 4th ed. (DBI Books).  Reading that would be worthwhile,
and I strongly recommend it for a beginner.  I especially like the 
author's emphasis on safety and practicality.  

  SAFETY NOTE - This can't be over emphasized!  Be careful, and set 
up everything, including your routines, so that the chances of an 
accident are minimized.  Wear safety glasses, don't have distractions 
such as a TV around, don't eat or smoke when reloading, don't reload 
when affected by alcohol, drugs or when over-tired, ...  

  It wouldn't hurt to find a local gunshop which carries reloading 
equipment and supplies, and spend a little time looking around, 
seeing what they carry, and perhaps go ahead and buy some books 
and manuals.  See if you can identify someone there who is 
technically knowledgeable, and maybe even buy some supplies at 
this time.  I like to buy from local stores, but I also like to 
pay low prices, and these two may conflict.  Still, you can buy 
many of the items locally and so support your local people, and
also have a local source of expertise.  This is likely to save you
money, time and effort in the long run.  But note that there are 
substantial savings available through mail order.  (At the very 
least, get catalogs from: Gander Mountain, Midway, Wiley Outdoor, 
Mid-South Shooters Supply, and Natchez.  Also get catalogs from the 
major manufacturers of reloading equipment, and pay the $1 - $2 
charge if they have one.  Certainly include Hornady, Lee, Lyman, 
Omark/RCBS and Dillon.)  (Sometimes Midway sells a package of
assorted catalogs which is an easy way of getting a bunch.  If you
need addresses, look at the ads in any technically oriented firearms 
magazine, such as Handloader, or in the addresses section of Gun
Digest or Shooters Bible which are two valuable firearms reference
annuals.)

  OK, now that you feel comfortable with what is involved, and 
are confident that you want to get started - let's go.

  Buy a reloading press and a set of dies.  I strongly 
suggest starting with one caliber preferably a straight
sided pistol caliber (such as the .38 Special :-) so that
you can get a carbide resizing die and skip the case lube
and clean-off-lube steps.  (These steps are really not so
much effort and the .38 Special has other disadvantages
discussed below.  Basically, you'll want to start with
whatever it is that you shoot.)  I strongly suggest a simple,
single-die-at-a-time press.  It is cheap, it lets you
do everything (just not as fast) and right now you
are trying to learn everything about reloading, rather
than to turn out bulk ammo.  The simple press lets you
concentrate on technique and the meaning of what you are
doing, rather than on complicated machinery.  I even
suggest that you get a separate priming thing (tool), rather
than priming with the press - to further uncomplicate things.
(I keep talking with beginners who are attracted to the
progressive presses because of the allure of turning out large 
volumes of ammo quickly.  I try hard to discourage them from 
starting that way.  Mainly because I want them to learn how 
to do it well and safely.  Also because of the possible 
discouragement factors of price and complication - they might 
never get started if they have to buy this relatively expensive 
thing.  Even if they spend the money then they have to get it 
working just right - before they have experience - and so might 
get discouraged before everything gets going satisfactorily.  On 
the other hand maybe they might get bored working more slowly.)

  I've talked with many reloaders who have started with a
progressive press and who are very satisfied.  One common element
is that they all did it slowly and carefully at first.  They read
up on what they needed to do, and they carefully ran cases through
until they understood what was going on and how to reload safely.
A progressive press can also have some benefits, such as it being
much harder to double charge a case because a case will only stay in
the charging station for one handle cycle.  So I'm not saying that it 
is wrong to start this way, just that it is simpler and less expensive 
to start with a single stage press.

  The simple presses (called single stage presses) come in
two varieties - hand held and bench mount.  The hand held type
is the ultimate in small, portable and easily stored, but it 
is less convenient to use.  The bench mounted type is 
much easier to use, since it is mounted to the bench and has
more leverage and can be operated with one hand, with the other
one free to move components, etc.  You can actually bolt it to
a reloading bench, if you have a dedicated area.  But it works
just as well, and is more convenient, to bolt it to a piece of 
wood, and then clamp the wood to your workbench with C-clamps
when you want to use it.  I used a piece of hardwood 1 x 4 long 
enough to have the press just in front of my bench, and the end 
of the board goes to the back edge of the bench.  I use one clamp 
at the rear, and one at the front edge.  It takes me less than a 
minute to mount or remove and it is very solid during operation.
I can do everything, including full length resizing of .30-'06 
cases with it.  So far I've been able to reload 4 handgun calibers 
and 3 rifle calibers with this equipment, so I don't feel limited 
by this simple setup.

  (It has been pointed out to me that the .38 Special case 
is very large compared to the typical amount of powder loaded 
- and this makes it dangerous compared to the usual rifle case 
in which a normal load fills it up or nearly so.  With the .38 
Special it is possible to double charge or worse - which may 
lead to blowing up the gun and serious injury.  Therefore it 
is *very* important to be careful when reloading.  I did 
start with the .38 Special so that is what I'm discussing.)

  (There are also dangers in reloading for the rifle.  The 
length of the cartridge and the neck thickness take on more 
importance, and inattention can lead to over-pressure
conditions.  There is no simple way to be safe.  You have
to learn about what you are doing, and then pay attention
all of the time.)

  I bought the Lee Reloader Press, in a bundled deal which made 
it very inexpensive when also buying a set of dies - I got the 
carbide dies - and a priming tool - I got the Auto-Prime with a 
shell holder.  Since the die set includes a powder scoop and a 
shell holder, it is possible to get started with nothing but this 
purchase!   (Well, I also bought a small powder funnel, a reloading 
tray, and a primer pocket cleaner.  Also one needs supplies - 
further discussed below.)  There are many presses which can be 
bought in some kind of bundled deal or "kit" with a set of dies, 
etc.  Sometimes this is a very good buy, so look over prices and 
equipment carefully.  Note that a vibrator/tumbler for cleaning 
cases is not an essential item, although it is nice, and you will 
probably buy (or make) one if you continue in reloading.  (Also there 
are many very high quality brands of equipment, and I don't feel that 
Lee is any better than the others.  It may even not be as good, but it 
was the best buy I could find, and it has worked very well.)

The steps in reloading are (briefly):  (Note this is with a carbide
resizing die which doesn't need case lubricant and with a second
die which flares the case mouth and which also allows dumping powder 
through it.)  Also this is with the use of a powder scoop which means
that the purchase of a mechanical "powder measure" isn't required.  
Lee includes a scoop in their die sets and also sells an inexpensive
set of scoops.  I wear eye protection for the entire process and also 
keep the case pointing away from my head when I'm priming it.

 1. Wipe off the old cases with a rag.  (Not necessary if you've
      cleaned them some other way.)
 2. Resize/deprime.  (first die)
 2a.(optional, but recommended) Clean out primer pocket with a 
      cleaner brush or scraper.
 3. Prime with the Auto-Prime.
 4. Expand/flare with second die, and also
 5. Dump in scoop of powder through this die.  (The scoop is
     on the conservative side regarding the charge, and so a
     scale/balance to weigh the charge is not necessary.)
 6. Place bullet on top of case and seat and crimp (third die.)
 7. Voila!

  Since this is a single die press, all the cases have to be run
first through the first die, then the second step is done, etc.
This is one reason why reloading trays/blocks (or pieces of wood with 
a bunch of holes drilled in them) are so nice.  You have to change 
dies, and do a little readjustment at each change - but so what - 
you are getting great experience and practice each time you do that!
There are some tricks which minimize the work of adjusting dies - 
I've included some discussion as a postscript on this essay.
(Also, even if you later buy a fancier press, there are lots of
things which a single stage press can be used for - such as
bullet sizing/lubricating, depriming and bullet extraction.  So
it won't be wasted later on.)  Depending on the die set there
may be a slightly different sequence of steps, but the same 
operations will still be done.  The Lee Speed Die Set costs only
about 60% of the usual 3-die carbide set, and actually is 
slightly easier/faster to use in a single station press.  There
is one body part, and then the other attachments just are put
on and off with relatively little adjustment.  However it can't
be used conveniently in a multi-station press (turret or progressive) 
because there is only one body.  Still, it might be worth starting 
with this, for a handgun, to minimize the initial cost and fuss.

  I very strongly urge using two loading trays, and keeping them on
opposite sides of the press.  Then you can transfer each round 
systematically as you work on it.  This helps assure that you 
don't skip any and don't double charge any.  Without this help
you are very likely to lose track, especially if ever interrupted,
and to end up making a dangerous mistake.

  Now, what supplies should one purchase?  Keep it simple!  Don't
buy anything exotic - and keep away from peoples' favorite oddball 
loads!  (I.e., shotgun powder in pistol, weird weights or two bullets 
in one case, etc.)  Not that there is anything wrong with these 
"favorites" but when you are gaining experience you should keep in 
the mainstream.  Your load should be chosen from a manual (*not* 
from someone's memory!) and preferably should be checked with 
another manual or two and be in the moderate power range.  In 
understanding what is "mainstream", a knowledgeable person at the 
gunshop can be a big help.  Buy one box of brass (whatever they 
carry new is fine) preferably unprimed, a single box of primers 
(the smallest box which usually is 100 primers) and a box of 
bullets (100 to a box) and *one pound* of powder.  (I don't care how 
much you might save by buying an 8 pound keg - just buy one pound.)  

  Why new brass? - so you have one thing less to worry about.
Unprimed so you get the experience of priming.  One box of bullets 
- you're just getting started and gaining experience, not trying to 
save money by buying in bulk.  One pound of powder because it is 
*safer*.  (Think safe and play safe - don't do anything to cut 
corners on safety - don't smoke around the reloading bench ...)  
With new brass, a chamfering tool (handheld - try not to pay over 
$5) is not a bad idea, but is not necessary.  (Although if the 
curved cuts on your fingertips bother you, you will prefer to 
lightly chamfer your new cases inside and outside.)

  I got a box of Winchester brass, a box of CCI 500 (standard small
pistol) primers, a box of Hornady 158 gr. LRN, and a pound of 
Bullseye.  I fiddled with the equipment, fussed around and loaded up 
a whole box (50) of ammo.  Went out to the range and every round went 
bang - very satisfactory.  But the loads felt kind of light, sort of 
closer to target wadcutter loads than to factory loads.  Reloading 
and shooting the same cases confirmed the feeling.  (I should note 
that the scoop which came with the dies was too large for Bullseye - 
so I bought the inexpensive set of Lee Powder scoops and used a smaller 
one.)  What to do to increase the power?  Well, I was an expert by now 
:-), and looking for new horizons to conquer.  The clear next step was 
to be able to handle heavier loads - that meant an adjustable powder 
measure and then a balance to be able to check for accuracy and 
consistency.  

  (It has been pointed out to me that Bullseye is one of the
most "energetic" powders used.  I.e., it takes the smallest
volume to get a given amount of energy.  That means that a
very small amount is used, and so it will be harder to
notice a double charge if you slip up and do that.  Even if
you peer at the cases in the loading tray from the top after
charging with powder it is not easy to see the small amount
extra of this powder.  However Bullseye is very popular, and
this is what I have been using.  It does make it even more
important to be very systematic and avoid overcharging any
of the rounds.  With a loading tray, the brass is held upright
and lined up - this makes it much easier to look in and make
sure that powder is in every case and gives you the best chance
of seeing a double charge, if one is present.)

  It is also important to make sure that every case is charged
with powder.  The energy in the primer alone is enough to drive
the bullet into the barrel, but not enough to have it surely leave 
the barrel.  (This is referred to as a "squib load".) If you fire 
one of these and don't notice the lighter than usual recoil and 
report, and then fire a fully loaded round - the second bullet 
will violently encounter the first one, and the result can be a 
bulged barrel or worse.  Sometimes much worse, with injury as 
well as equipment damage resulting.)  However, with the brass in 
the loading tray after powder charging, when looking in from the
top it is *very* easy to see an uncharged case.

  Since I only used Bullseye at the start I didn't have to worry
about the possibility of mixing powders or of confusing powders.
Such errors can easily lead to disaster.  With more than one
powder around, one should be very careful to avoid these
errors.  Now that I use several different powders, I take such
simple precautions as only taking out one container at a time.

  A less obvious danger, but one which is easy to avoid, is lead 
poisoning.  No kidding, the amount of lead you get on your hands 
when working with lead bullets and with fired casings is dangerous 
if it gets into your body.  Don't touch food or smoke until you have 
scrubbed your hands clean!  Assume that all of your reloading gear 
has lead on it, and then you'll be extra careful.

  Lead poisoning is slow and insidious.  The danger of working
with primers is more dramatic and sudden.  Primers can detonate
when crushed, and so it is important to avoid this, particularly
when priming cases.  If a primer is going in "hard", stop and
check - don't just push harder.  Keep primers in their original
boxes until use - these boxes are designed to protect the primers
from impact.  Don't keep primers in a glass jar - an explosion
would produce particularly unpleasant effects.  Most of the 
reloading guides discuss the need to keep primers clean and dry, 
and particularly to avoid getting oil on them - all of this is to 
ensure that they go off when needed.  The safety issue is to make 
sure that they don't go off any other time, and to limit the
dangerous effects if a primer does go off inadvertently.

  I got the Lee Auto-Disk Powder Measure (the Deluxe model,
I was on a roll) and a Hornady balance (hm, I bought mail order,
but asked the order taker if I could talk to someone who knew
a lot about reloading, and I asked that person about quality
of different brands of balances - and got steered to the
Hornady vs. the Lee.  I've been very happy with it.  Whatever
brand you buy, make sure that you get one with magnetic damping.
This is an important feature which makes the balance much easier
to use because it makes it settle to a stop much faster without
harming accuracy.)  A set of balance check weights is be a good
idea, or at least some known weight objects (such as a small
jacketed bullet) to check for gross problems in operation of the
balance.  The Disk Powder measure screws into the Lee die in 
place of the funnel, and is actuated by the press when expanding 
the case.  Works like a charm, and for a while I also weighed 
every charge - then I used to weigh every tenth charge - now I 
weigh every twenty-fifth charge - I've never found one as much 
as 0.1 gr off the usual.  (The charge runs consistently 0.05 gr 
less than the chart says it should be - but it is very consistent.)
However there can be changes in lots of powder or in conditions so
that there is a different density and therefore there will be a
different weight.  This is one of the important reasons to use a
balance to check.  Now my loads run as hot as factory ammo, which is 
where I want them.  There are digital electronic scales which are much 
faster and easier to use, but they are considerably more expensive 
than the traditional beam balance.  Most people don't weigh stuff 
enough to make it important to have the extra speed and a beginner 
certainly can save the money.

  One more tool is very handy - a dial micrometer caliper - to check 
the overall lengths (OAL) of stuff, and see if and when cases 
need to be trimmed, and lots of other uses.  I use my stainless
steel machinist's caliper, but an inexpensive plastic one would
work well enough.  A vernier caliper could be bought for a few 
dollars, but is a pain to use compared to a dial caliper.  A 
reasonable stainless steel dial caliper will last for many 
decades, and have many uses, and so should be considered to be an
investment.  Since I'm firing mild loads, I've not yet had to do any 
case trimming.  One reason why checking length is important is that 
the crimping die's action will vary if case length varies.  Variable 
crimping hurts accuracy, and excessive crimping can lead to over-
pressure conditions.  (Note that a roll crimp is fine for revolvers 
and single shot pistols.  Semi-automatics commonly head space on the 
mouth of the case, and so can't work with a rolled-in crimp.  A 
taper crimp is used in those cases, and taper crimp dies are 
available from several die manufacturers.)

  Another neat gadget is a loaded cartridge check gauge (available
for such sources as Wilson, Midway, Dillon, etc.)  This is usually a
steel cylinder (perhaps the size of a 35 mm film can for the handgun
cartridge sizes) with a hole bored in the center, with it sized just
so that a properly sized cartridge will be able to fit in, and not 
poke through the far end.  So it checks all the critical dimensions of
the cartridge just by putting in a cartridge.  This is not a necessary
gadget, but it can be very helpful, especially when you are first
getting started.

  I couldn't stop there - since I was reloading them over and
over, the cases were getting just a bit sooty and tarnished,
and cleaning them with a rag wasn't enough - so I needed a 
tumbler/cleaner.  It makes the cases so nice and bright! I also 
bought some more cases, primers and bullets (in quantity this 
time, and got a reasonably nice price break.  Price breaks 
usually start when you reach quantities of 500 or 1000.)  It
took quite a while to finish my first pound of Bullseye, but I
did that and have gone through a lot more powder since then.
What I'm doing has added up to a bit more money by now than my 
start-up costs - but I didn't spend the extra until I was sure 
that I wanted to go on to do the extra stuff in reloading.

  It has turned out to be a nice way to spend an occasional
evening.  It hasn't been too expensive, and I've had no problems.
Note that I've been *very* careful - check everything twice.  I'm 
never in a rush to get out more rounds, but rather very systematic 
and if in doubt I do it again. (Really the only very dangerous 
part in handgun reloading is double charging a case.  It is hard to 
spot by the usual recommended technique of shining a light down the 
cases and looking at the powder levels.  So I do that anyway, but 
first I am very careful to move cases from the uncharged tray to the 
charged tray as I charge them, and to only work the lever once, ...
Also, I turn over each case before charging it - so I check the 
primer and also verify that it is empty.

  All in all, it has been fun - I've learned a lot about the
technology, and I can make loads of the sort I want.  I still 
shoot more bought ammo than I reload - but I went into this for 
fun, not to replace the store.  But even this way, if I had bought 
all the ammo that I've loaded, it would have cost much more than 
I've paid for all the supplies and equipment I've bought.  So I 
can argue that it also has saved me money compared to what I would 
have had to spend to get this type of ammo.  For rifle shooting 
I've worked out loads which have given me match accuracy (< 1/2 MOA!) 
and not only has it been much less expensive than factory match ammo, 
it has been *very* satisfying.

  Where next?  If I buy another press, I think I want one with a 
turret disk so I can leave all my dies mounted and not have to do 
any readjustment.  I don't think I want a progressive press, 
because there is more which can go wrong.  I could change my mind 
if I ever wanted to reload larger quantities, but my interest is 
still going in different directions.  I'm still interested in 
accuracy, and possibly also in heavier bullets.  If I experiment in
these areas, I still will load relatively small quantities.  I've 
bought a few other inexpensive tools, a case trimmer, a few brushes, 
reloading trays and storage boxes, some more manuals, ... .  I've 
tried some other powders, - lots of interesting projects under way.  
(Safety note - to avoid the danger of mixing (or mixing up) powders, 
only take out one container at a time.  Then it is clear what powder 
you are using and you won't ever return powder to the wrong can.)

  I bought dies and supplies to load ammo for my rifle (.308 Win. 
bolt action) which has turned out to be a worthwhile effort.  Other 
than the set of dies, the only other equipment needed was a new guide 
for the case trimmer.  (It was good to get to use it - the .38 Spl 
cases don't seem to ever need trimming.  I have a group of cases I've 
reloaded 30 times and they are still too short to touch the trimmer
cutter.  Also note how the cost of the brass per shot goes down very
fast when it can be reloaded many times.)  I use the very inexpensive 
Lee Case trimmer which you rotate with your hands.  It is reasonably 
fast and works very well, but is tiring to use if a lot of trimming is 
necessary.  

  My rifle die set is the Lee Collet Die set - this is one of the types 
of dies sets which does neck sizing - rather than full length resizing.  
Neck sizing is much easier to do, is easier on the brass, and generally 
provides superior accuracy because it doesn't affect the body of the 
cartridge which has taken on the shape (and headspace) of the particular 
rifle in which it has been fired.  So this works if the cartridges are 
being reloaded for the same bolt action rifle in which they were fired.  
Neck sizing is not recommended for semi-automatics because they need a 
bit more clearance between the cartridge and chamber walls to function 
easily.

  I picked a powder which was recommended by a knowledgeable 
salesman at a local shop (IMR 4895) and the bullet he recommended 
(Sierra 168 grain HPBT Matchking) and tried a few charge weights.  I 
used once fired Federal brass from the American Eagle ammo I had fired, 
and CCI Standard Large Rifle primers.  With the original ammo, I was
getting about 3" groups (100 yards, sandbag on bench.)  My first (light)
reload gave me 2" groups.  A one grain increase in the charge reduced
the groups to under 1", and one more grain gave me a 6 shot group
of 0.7".  (One grain can make a big difference in accuracy!)  My best
5 shot group is now 0.4", and I consistently average well under 1".
Note the change from mediocre groups to excellent groups - that
alone made the whole reloading exercise worth it for me.  Also, this
is where there are reasonably big savings from reloading.  I don't
shoot the rifle enough to want to buy match grade ammo by the case,
so the savings per round are reasonably large, and there was very
little additional investment in equipment needed.  I also have done 
some reloading for the .222 Remington.  Again, only an additional
die set and a cutter guide was needed.  (Oh well, I might as well 
admit that there are always a few extra gadgets which do something
nice or necessary.  Things like extra primer pocket cleaners or 
reamers, various brushes, etc.  But they aren't big items, and you 
don't really need to buy them, especially not at first.)  I guess
I shouldn't mention the match grade powder measure that I just got -
but I'm sure that I can always find new things worth buying!

  OK - that's my story.  It would be nice to hear about others' 
ideas and experiences.  (It was help from others which got me 
going and helped me continue - so let's all keep this hobby going.)

--henry schaffer

-- 
Anmar Mirza   #Chief of Tranquility  # My Opinions! Not IU's!#CIANSAKGBFBI
EMT-D         #Base, Lawrence Co. IN # Don't think of it as  #ASSASINATEDEA
N9ISY (tech)  #Somewhere out on the  #gun control,think of it#NAZIPLUTONIUM
Networks Tech.#Mirza Ranch.C'mon over# as victim disarmament.#PRESIDENTFEMA



