             Full Auto Conversion Plans For The SKS



Tools needed:   Small drift punch
                Grinding wheel or dremel tool
                Small metal bar- approx 1/4" X 4"

Instructions:
1. Cock the hammer and put the safety ON. Close bolt
2. Turn the weapon upside down and push trigger guard latch with 
   drift punch.
3. Push latch all the way in, letting the trigger guard jump out slightly.
   The guard can now be pulled up and out.
4. Place the guard on padded vice and push down on the safety gear and
   then pull the trigger to release the hammer. Use the metal bar to force
   the hammer out.
5. The thin rounded cam surface at the bottom of the hammer must be ground 
   or milled away flush with the flat bottom surface of the hammer.
6. Remover short trigger spring between trigger bar and safery sear.
   Rotate sear up and out of the way.
7. Remover disconnector by squeezing it together at the forward end.
8. Reassemble the trigger group, leaving out the disconnector.
9. Replace lower reciever group into buttstock of the weapon.
10. To restore the SKS to semi-auto, disassemble and reinstall the 
    disconnector.

\/\/ARLORD

