
><><><><><><><><><><><><><><><><><><><><><><><><><><><><>
*********************************************************
*                                                       *
*            PcPursuit Outdialing System                *
*                 The Complete Guide                    *                                                                       
*                                                       *
*                                                       *
*           Another Modernz Presentation                *
*                                                       *
*                        by                             *
*                  Digital-demon                        *
*                                                       *
*            (C)opyright January 26, 1992               *
*                                                       *
*********************************************************




*********************************************************
The Modernz can be contacted at:
                                                                                                                                                  
MATRIX BBS
WOK-NOW!
World of Kaos NOW!
World of Knowledge NOW!
St. Dismis Institute -  Sysops: Wintermute & Digital-demon
             (908) 905-6691
             (908) WOK-NOW!
             (908) 458-xxxx
Home of Modernz Text Philez
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>
                                                                                                                                                                                                                                                                               
TANSTAAFL
The Church of Rodney - Sysop: Tal Meta
             (908) 830-7960
Home of TANJ Text Philez                                 
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>
*********************************************************             
Also can be reached at :

Hellfire BBS  - SANctuary World HQ
             Sysop: Red
             (908)495-3926

*********************************************************
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>
                                                                                                                                                                                                                                                               

    Well this file has been several months in the making,
most hackers/phreakers are looking for anything at all
on outdials...This is a compilation of everything I 
have ever gotten a hold of or learned as to pcpursuit
outdials...If you are looking for other types of outdials
I may get around to writting a phile on them as well, but don't hold your breath...if there is something you can't
find in this phile, feel free to get in touch with me and
I will help you if I can.

                           _-Demon

                                        
P.S. Salutations and Greetings to all that know me,
if yah don't...then I could care less.
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    
<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        

    PC PURSUIT
    ----------


    With PC PURSUIT, you can explore a wealth of free resources and even
    discover more uses for your PC.  In any of the locations accessible to
    PC PURSUIT, you have the ability to:

        * communicate with friends and associates on-line,

        * download and upload public domain software from
          thousands of Bulletin Board Systems in the 34 PC
          PURSUIT cities,

        * research professional projects and personal hobbies
          through free databases, and

        * shop and advertise in electronic catalogs.

    The features and benefits offered by PC PURSUIT SERVICE include:

    Portability:

    ------------
          Because the service is widely accessible, you can use
          PC PURSUIT at home, at the office, or traveling.

    Accessibility:
    --------------
          The service can be accessed from nearly 9000 local
          telephone exchanges via the Sprint network. You can
          dial thousands of free databases at 300, 1200, and 2400
	  bps in 34 major cities across the nation, 24 hours a day.

     Convenient Billing:
     ------------------
          All PC PURSUIT service charges are billed directly to
          your VISA, MASTERCARD, DISCOVER or AMERICAN EXPRESS account; 
	  or automatically debited from your checking account.

     Nonstop Support:
     ---------------
          As with all other Sprint services, The Sprint Network
          Control Center provides 24-hour management to ensure
          reliable data transmission.  Customer Service is available
          to handle problem system problem reports 24 hours a day
          at 1-800-336-0437.

    START SAVING TODAY AND JOIN THE THOUSANDS OF PC USERS FROM COAST TO
    COAST WHO ARE ALREADY ENJOYING THE COST-EFFECTIVE WORLD OF PC
    COMMUNICATIONS THROUGH PC PURSUIT.  CALL TO REGISTER AT 800-736-1130
    (voice) OR 800-877-2006 (modem).

-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                                                                                                             
                                                                                                                                                                                                                                                                                                                                                   
        4/12/89

	We have installed a new version of TPBBS which corrects some
	of the file transfer problems of the past.  In the instructions
	below, the only reason for using the SET commands is if you
	need to escape to the PAD to issue additional commands.  Downloads
	now appear to work at 8-N-1 w/o having to issue 2:0,4:1.  Uploads
	are still restricted to 7-E-1 Kermit.

	------------------------------------------------------------------

	Many of you have indicated that you have been having problems
	with file transfers to and from this BBS.  First, file uploads
	have been disabled pending resolution of a bug report submitted
	to Sun regarding problems with their X25 package.  File downloads
	on the other hand, are possible if you use the following 
	procedure:

	      - call SprintNet at 8-N-1 and use the correct hunt/confirm
		sequence to wake up the port (see hunt.txt in the pcp
		file area)

	      - use <cr> or D1 at the TERMINAL= prompt
	      - enter:     SET 0:0,57:1,63:0
	      - enter:     C PURSUIT
	      - when you get the CONNECTED message, immediately enter:

			   @<cr>

	      - you will see TELENET and the @
	      - enter:     SET 2:0,4:1
	      - enter:     CONT
	      - and the BBS will display (or finish displaying) the
		initial welcome message

	After you do your file transfer, you may find that you have lost
	your character echo.  If this happens, enter;

		<cr>@<cr>
		SET 4:1
		CONT
	
	If you are not going to be doing file transfers, you can call in
	using 7-E-1 and ignore all the SET commands.  We regret the 
	complexity of the logon procedures, but we're hoping that Sun 
	will be able to supply us with a version of the X25 package which
	will work better in our environment.

	PC Pursuit Technical Coordinator

-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 
                                                                                                                                                                                                                                                                                                                                            
                                                                                                                                                                                                                                                             
There are a number of questions that are asked repeatedly on
this BBS....here are the answers to some of them:                                                                                                                                                                                    
                                                                                                                                                                                                                                    
Q:  I used to be able to do file transfers at a reasonable speed.
    Now my file transfers go at a snail's pace or fail entirely.  What's
    going on?                                                                                  
A:  We have had a team of engineers looking into the file transfer problems.
    They have found and corrected a network problem which appears to have
    been affecting file transfers.  This change has been implemented 
    everywhere we have outdials.  In general, both uploads and downloads
    should go much more efficiently now.  If any additional problems are 
    found or the engineers have additional suggestions for how to improve
    your transfers, that information will be posted here.

Q:  This BBS is always busy...can I download the files in your PURSUIT
    file area and post them on *my* BBS so that other customers can
    get to them easier?
A:  Yes...If you decide to do that though, please try to make sure that
    the information you post is kept up to date.
 
Q:  I'm having problems with file transfers....what do I do?

A:  First, take a look at the file TIPS.TXT in the PURSUIT file
    area.  Also, if you're more technically oriented, there are
    other .TXT files in that file area (such as TELE_ITT.TXT and
    X3_ITI.TXT) which you may find useful.  
 
Q:  I've looked at TIPS.TXT and am still having problems...now what?
A:  Leave a public message in the GENERAL message area indicating your
    hardware and software configuration and a short but complete
    description of the problem.  There are many users on this BBS
    (both Sprint employees and other customers) who are very knowledgeable
    about the service who will be glad to assist.
 
Q:  I can't get through to the Net Exchange at night but I've been told
    this is where to go for help with the service.  What now?
A:  As long as you call the Net Exchange using "C PURSUIT",
    the call to this BBS is free 24 hours a day, 7 days a week.  The
    BBS may be down for short periods during the day for maintenance
    but it's available at most other times.

Q:  Occasionally, I have problem accessing an outdial during the weekend 
    for a short period of time, what could cause such an intermittent
    outage?

A:  You may be experiencing an outage due to reload.  Reloads
    occur in order to perform required maintenance and table changes 
    on the SprintNet network.
    There are three time periods when TP reloads are scheduled. 
	
	     Saturday  (00:00 - 08:00 local time)
             Sunday    (00:00 - 08:00 local time)
             Monday    (00:00 - 08:00 local time)
			 
Q:  Where do I request new in-dial and out-dial rotaries?
A:  If you have a request for a new in-dial site or a new speed in an
    existing site, leave a message to our product manager.  Requests for
    new outdial sites should be composed via questionnaire #6.
 
Q:  Where can I leave an ad for my BBS so others will call me?
A:  All ads for BBSs should be left in the BBS message area.
 
Q:  Other than PURSUIT and the outdial rotaries, can I use my PURSUIT
    account to access other services through Sprint?
A:  Yes, there are a number of direct connect BBS services that are
    available with your PURSUIT account.  These include PORTAL and PLINK.
    You are charged for these services just like you are for using the
    outdial rotaries.

Q:  What does the DISCONNECT message mean?
A:   
    ####### DISCONNECTED 00 40 00:00:02:39 143 16
      ^                  ^  ^  ^  ^  ^  ^   ^  ^
      |                  |  |  |  |  |  |   |  |
      |                  |  |  |  |  |  |   |  +-- Packets from user
      |                  |  |  |  |  |  |   +----- Packets to user
      |                  |  |  |  |  |  +--------- Seconds connected
      |                  |  |  |  |  +------------ Minutes connected
      |                  |  |  |  +--------------- Hours connected
      |                  |  |  +------------------ Days connected
      |                  |  +--------------------- Clearing diagnostic
      |                  +------------------------ Clearing cause
      +------------------------------------------- Remote address

   (thanks to Vann Hall for supplying this information)

-------------------------------------------------------------------------------
                                                                                                                                                                                                                                                                                                                                                                                                                                                      
                                                                                                                                                                                                                                                             

	Dear PC Pursuit Customers:
                                                                                                                                                                                                                    
	Based on a request for clarification from the Product Management                                                                                                                                 
	message area, please note the following information:                                                                                                                               
                                                                                                                                    
	1.  Calls of 90 seconds or less will not be billed.

	2.  Usage is rounded to the next minute for the purpose of 
	    calculating total usage on each connection.  This means 
	    that a call of 11:59 minutes will rounded to 12 minutes.

	3.  All calls are subject to a minimum call duration of two 
	    minutes unless they are 90 seconds or less. This means a 
	    1:29 minutes call will not be billed, but a call of 1:31 
	    minutes will be billed as a two minutes call.

	4.  Calls that begin on the last day of the month and do not 
	    terminate until after midnight will be billed in the ending
	    month and treated as that month's current usage for purposes
	    of computing minimum usage charges.


-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                     
                                                                                                                                                                                                                                                            
                                                                                                                                                                                                          
                    PC  BUSINESSCALL
                                                                                                                                                                                                                                    
-------------------------------------------------------------------------------                                                                                                                                                                      
 
                                                                                                                                                                                        
     PC BusinessCall is designed for professionals and for small-
to medium-sized businesses that typically spend between 5 to 300
hours per month accessing PCs, bulletin boards or host computers
by dialing long distance.  Using the Sprint Public Data Network
to carry the long distance portion of data calls, PC BusinessCall
saves customers up to 75% off their monthly long distance
charges.
 
     Sprint is offering PC BusinessCall in two pricing packages:
the Initiator Program for intermittent low-volume users, and the
Professional Program, which offers maximum discounts to customers
with consistent monthly usage.  The Professional plan requires a
$95 per month minimum, but this $95 prepays for the user's first
$175 of usage per month.  
 
     The Initiator plan has a $10./month account fee, plus rates
ranging from $2.95/hr to $7.50/hr for basic service.  Rates are
higher for US Outdial (OutWATS) or Dial-in WATS.  For the

Professional plan, the user has no $10./month account fee. 
Instead, a $95./month monthly minimum prepays the user's first
$175. of standard usage (not including US Outdial or In-WATS). 
Professional rates are also lower, ranging from $2.50/hr to
$6.95/hr for basic service.
 
 
INITIATOR:
 
     $50.00  one-time signup fee
     $10.00  monthly account fee
 
     7.50/hr  peak time usage
     5.50/hr  prime time usage
     2.95/hr  non-prime usage
 
    10.00/hr  prime time US Outdial
     6.50/hr  non-prime US Outdial
 
     7.75/hr  WATS Dial-in surcharge (prime time)
     5.50/hr  WATS Dial-in surcharge (non-prime)
 

PROFESSIONAL:
 
     $50.00  one-time signup fee
     $95.00 monthly minimum
 
     6.95/hr  peak time usage
     4.95/hr  prime time usage
     2.50/hr  non-prime usage
 
     9.00/hr  prime time US Outdial
     5.75/hr  non-prime US Outdial
 
     7.00/hr  WATS Dial-in surcharge (prime time)
     5.00/hr  WATS Dial-in surcharge (non-prime)
 
 
 
     PC BusinessCall uses the Sprint Public Data Network to 
access remote computers equipped with 300 bps, 1200 bps or 
2400 bps auto-answer modems.
 
     To use this service, a customer has his PC or terminal dial
a local telephone number to connect to the Sprint Public Data
Network.  Local access is provided from more than 18,000 cities
and towns in the United States.  The user enters the destination
city, and then enters a command for dialing the local phone
number of the system he is accessing.  A special outdial modem on
the network then completes the call and connects the user to the
database, remote PC or other information source of his choice.
 
     At present, PC BusinessCall is available for accessing
systems in the local calling area of 34 major cities in the
continental U.S., with additional expansion planned for 1990.
Access is provided to all other locations in the continental 
U.S. through US Outdial calling.
 
     Besides calling regional information systems, remote PCs, or
private computer systems, applications of PC BusinessCall include
retail store polling, collecting inventory or sales updates,
customer order delivery, hotel and airline reservation systems,
telex delivery, automated data back-up and recovery services, and
many more.
 
-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                                                                                                              
                                                                                                                                                                                                                                                                                     

   Restrictions regarding BBS access are generally done at the
    request of Sprint Network Security or TELCO.  It is not Sprint's
    intent to censor our customers;  however, we do want to protect
    customer ID's and passwords.  If a BBS is posting user ID's
    we will restrict access.  We do not shut down an entire exchange to
    restrict a BBS.

-------------------------------------------------------------------------------                                                                                                                                                                                                                                     

10/8/91

Dear PC Pursuit customers

  We are pleased to announce a new outdial
city.  The city is:
  
     New Orleans, LA 

  This city supports both 1200 and 2400 baud
modems, and its mnemonic addresses are:
  
       D/LANOR/12 for 1200 baud
       D/LANOR/24 for 2400 baud

   
 
  Product Management

-------------------------------------------------------------------------------                                                                                                                         

03/01/91

Dear Customers:

The following bulletin contains information relevant to three of 
the most frequent and "popular" file transfer questions we receive 
from our customer base. Special thanks to Vann Hall from Tech 
Support, and Ben Chen from Product Marketing, for making this 
bulletin possible.

Thanks,
Paul Golder
Outdial Product Management

QUESTION 1:

"If most file transfers don't allow flow control, then why is the 
default setting: "Enables flow control?"

ANSWER 1:

Because people use PC Pursuit for many things other than file 

*** Depress a key to continue ........ 
transfer -- sending messages, reading text files, etc. -- that work 
best with flow-control enabled. In addition, the file transfer 
protocols that perform the best across SprintNet, like ZModem, are 
designed to be used with flow-control.


QUESTION 2:

"I sometimes experience problems with large file transfers  -- any 
thoughts why? 

ANSWER 2:

Note: Additional info on file transfers can be found in the "How 
to Use US Sprint's PC Outdial Services" user guide, and in the file 
section of this BBS.

In brief, the network can handle data rates of 2400 baud -- and 
far greater -- with no problem. A datascope or other such measuring 
tool will show data flowing at that rate. What users see as delay, 
though, is the time lag caused by packetizing data.
      

For instance, every XModem block contains 131 bytes: 128 data 
bytes and three overhead/management bytes. When the transmitting PC 
sends the block, the network takes the first 128 bytes received and 
sends it across the network as a full packet of data. In the 
meantime, the PC sends the remaining three bytes. The network 
equipment then waits a predetermined period of time before
deciding the PC has nothing more to send before it packetizes
the remaining three bytes and sends them along.
      
The timeout value (called the "idle timer") is 0.1 seconds. That 
is, if the PC has not sent enough bytes to fill a network packet 
(128), the network equipment will wait 0.1 of a second before 
sending the data. At 2400 baud, this delay immediately reduces 
effective baud rate by 240 bps.

On the other side of the connection, the receiving PC has to send 
a one-byte acknowledgement/unacknowledgement of the XModem block. 
This ack/unack character also has to wait in the network PAD's 
buffers for 0.1 second before being forwarded, an effective baud 
rate of 100 bps.
      
Compounding this situation is the fact that the network induces 
                                                                                                                                                                                           
some delay on an end-to-end transmission. This delay is usually 
less than 0.25 seconds round-trip. With data flowing mainly one                                                                                            
direction or the other, the delay is unnoticeable -- if you're                                                                                                                         
sending 1 Mb of data, an additional quarter- or half-second is                                                                                                                  
nothing. However, if each end of the connection has to talk,                                                                                                                   
alternatingly, every so often, the delay affects each turn-around.                                                    
                                                                                                                                          
That's why the best protocols for PC Pursuit are those like 
ZModem, which calls for the receiving station to transmit only when 
an error is seen and not to positively acknowledge every block, or 
those like Windowed Xmodem or Windowed Kermit. These latter 
protocols allow the transmitting PC to send several blocks of data 
before having to receive an acknowledgement for the first block 
sent. Since the acknowledgement for the first block and the data 
for, say, the third block often "pass" each other in the network, 
the PCs can maintain an effectively uninterrupted data flow.
     

QUESTION 3:

"What can I do to eliminate the message "POSSIBLE DATA LOSS?


ANSWER 3:

POSSIBLE DATA LOSS messages (PDLs) are sent to warn the user that 
data may have been lost as a result of an X.25 reset occurring 
within the network. In most cases for PC Pursuit, the result is 
occurring internally within the network PAD equipment at either end 
of the connection.
      
To reduce the chances of receiving a PDL, flow-control should be 
enabled at both ends of the connection, and the user should not try 
to mismatch speeds. For instance, a user dialing into the network 
at 1200 baud can connect to a 2400-baud rotary and dial out to a 
BBS at 2400 baud. Should he try to review data with no flow-control 
enabled, data will enter the network at twice the speed they can 
exit. Although the network can buffer a certain amount of data, 
eventually it runs out of places to stuff bytes on hold, it issues 
a reset, and the PDL results.
      
Also, with flow-control enabled, users may still receive PDLs if 
they flow-control a port for too long. Say you're reading a message 
on a BBS, you Ctrl-S during the middle of it to stop it from 
scrolling, you get up for a moment: When you get back, you may see 
a PDL. What has happened is that buffers have gone unused for a 
while, and the PAD resets the link just in case the problem is 
internal to it.
      
To enable flow-control at both ends of the VC, users must issue 
both a SET? and an RST? command. Parameters 5 and 12 should both be 
set to a value of 1 at each end of the VC.

-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                       

 
                NEW ACCESS CENTERS AND RECENT CHANGES
----------------------------------------------------------------------
 
 
               NEW DOMESTIC ASYNCHRONOUS ACCESS CENTERS
            ----------------------------------------------
     EFFECTIVE  AREA
ST     DATE     CODE    ACCESS CENTER         300-2400 BPS       CLASS
-----------------------------------------------------------------
CA    7//91     (805)   ancaster                949-7396           B
CA    7/3/91    (714)   Saddle Brook Valley     458-0811           B
IN    7/3/91    (317)   Richmond                935-7532           B
MS    7/3/91    (601)   Port Gibson             437-8916           B
NC    7/3/91    (919)   Burlington              229-0032           B
SC    7/3/91    (803)   Florence                669-0042           B
SC    7/3/91    (803)   Myrtle Beach            626-9134           B
 
 
            NEW 2400 DOMESTIC ASYNCHRONOUS ACCESS CENTERS
         ---------------------------------------------------
     EFFECTIVE  AREA

ST     DATE     CODE    ACCESS CENTER           2400 BPS       CLASS
----------------------------------------------------------------------
FL    7/3/91    (407)   Boca Raton              338-3701          B
IN    7/3/91    (812)   Bloomington             331-8890          C
ME    7/3/91    (207)   Portland                761-9029          C
MA    7/3/91    (508)   Brockton                588-3315          B
NC    7/3/91    (919)   Tarboro                 823-7459          C
SC    7/3/91    (803)   Spartanburg             585-9197          B
SD    7/3/91    (605)   Rapid City              348-2048          C
TX    7/3/91    (915)   Abilene                 672-2280          B
TX    7/3/91    (903)   Athens                  677-1712          C
TX    7/3/91    (409)   Bryan                   779-0713          C
TX    7/3/91    (903)   Longview                758-1161          C
VT    7/3/91    (802)   Burlington              864-5485          B
WA    7/3/91    (206)   Tacoma                  383-2233          B
 
-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                                                               
                                                                                                                                                                                                                                                                                                                                                                      
                                                                                                                                                                                                                                                             
                                                                                                                                                                                                                                  

 ____________________________________________
 |                                           |
 |  NEW 800 NUMBERS FOR PC OUTDIAL SERVICES  |
 |                                           |
 --------------------------------------------

  To better serve you, Our Telemarketing Department has been 
reorganized, and can be reached by a new 800 number for:
      
      *  general information regarding PC Outdial Services 
      *  and to register for PC Pursuit and PC BusinessCall.

  The toll-free number is:
 
       1-800-736-1130  from 7:00 a.m. - 7:00 p.m. (CST)
                        Monday through Friday

	
   You can also register online for PC Pursuit by calling our
PC-PURSUIT BBS at:
 
       1-800-877-2006  (24 hours a day)

Thank you very much,
 
Product Management
12/03/1990 


-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        
                                                                                                                                                                                                                                                                                                                                   



                 PC Pursuit Service Availability
                 --------------------------------

     PC Pursuit can be used to access local numbers in the
     following cities.  Note that not all exchanges in a 
     given area code are accessible via PC Pusuit!  For a 
     list of exchanges in the individual cities,
     please see the exchange lists.

     Example of use:


        C D/DCWAS/12,<id>,<pw>


     City                         Code             City Entries
     --------------------------   ----             -------------

     Ann Arbor, MI                313              D/MIAAR/12
                                                   D/MIAAR/24

     Atlanta, GA                  404              D/GAATL/3

                                                   D/GAATL/12
                                                   D/GAATL/24

     Austin, TX                   512              D/TXAUS/12
						   D/TXAUS/24

     Boston, MA                   617              D/MABOS/3
                                                   D/MABOS/12
                                                   D/MABOS/24

     Chicago, IL                  312 \            D/ILCHI/3
                                  708  >           D/ILCHI/12
                                  815 /            D/ILCHI/24
                                  (for 708, must use 1708 + phone number)
                                  (for 815, must use 1815 + phone number)

     Cleveland, OH                216              D/OHCLE/3
                                                   D/OHCLE/12
                                                   D/OHCLE/24

     Colton, CA                   714              D/CACOL/3
                                                   D/CACOL/12

                                                   D/CACOL/24

     Columbus, OH                 614              D/OHCOL/12
						   D/OHCOL/24

     Dallas, TX                   214 \            D/TXDAL/3
                                       >           D/TXDAL/12
                                  817 /            D/TXDAL/24
				  (for 817, must use 817 + phone number)

     Denver, CO                   303              D/CODEN/3
                                                   D/CODEN/12
                                                   D/CODEN/24

     Detroit, MI                  313              D/MIDET/3
                                                   D/MIDET/12
                                                   D/MIDET/24

     Glendale, CA                 818 \            D/CAGLE/3
				       >           D/CAGLE/12
                                  213 /            D/CAGLE/24
				  (for 213, must use 1213 + phone number)


     Hartford, CT                 203              D/CTHAR/3
                                                   D/CTHAR/12
                                                   D/CTHAR/24

     Hempstead, NY                516              D/NYHEM/12
						   D/NYHEM/24

     Houston, TX                  713              D/TXHOU/3
                                                   D/TXHOU/12
                                                   D/TXHOU/24

     Indianapolis, IN             317              D/ININD/12
						   D/ININD/24

     Kansas City, MO              816 \            D/MOKCI/3
                                       >           D/MOKCI/12
                                  913 /            D/MOKCI/24

     Los Angeles, CA              213 \            D/CALAN/3
                                       >           D/CALAN/12
                                  818 /            D/CALAN/24

				  (for 818, must use 1818 + phone number)

     Miami, FL                    305              D/FLMIA/3
                                                   D/FLMIA/12
                                                   D/FLMIA/24

     Milwaukee, WI                414              D/WIMIL/3
                                                   D/WIMIL/12
                                                   D/WIMIL/24

     Minneapolis, MN              612              D/MNMIN/3
                                                   D/MNMIN/12
                                                   D/MNMIN/24

     Newark, NJ                   201 \            D/NJNEW/3
                                       >           D/NJNEW/12
                                  908 /            D/NJNEW/24
                                  (for 908, must use 1908 + phone number)  

     Memphis, TN                  901 \            D/TNMEM/12
			          601 /	           D/TNMEM/24
				  (for 601, must use 1601 + phone number)


     New Brunswick, NJ            908              D/NJNBR/12
				                   D/NJNBR/24

     New Orleans, LA              504              D/LANOR/12
						   D/LANOR/24

     New York, NY                 212 \            D/NYNYO/3
                                  516  \           D/NYNYO/12
                                  718  /           D/NYNYO/24
				  914 /
                                  (for 516, must use 1516 + phone number)
				  (for 718, must use 1718 + phone number)
				  (for 914, must use 1914 + phone number)

     Oakland, CA                  415              D/CAOAK/3
                                                   D/CAOAK/12
                                                   D/CAOAK/24

     Orlando, FL                  407              D/FLORL/12
						   D/FLORL/24


     Palo Alto, CA                415              D/CAPAL/3
                                                   D/CAPAL/12
                                                   D/CAPAL/24

     Philadelphia, PA             215              D/PAPHI/3
                                                   D/PAPHI/12
                                                   D/PAPHI/24

     Phoenix, AZ                  602              D/AZPHO/3
                                                   D/AZPHO/12
                                                   D/AZPHO/24
                                  (Some exchanges must use 1602 + phone number
				   please check AZPHO.xch for details)

     Pittsburgh, PA               412              D/PAPIT/12
						   D/PAPIT/24

     Portland, OR                 503              D/ORPOR/3
                                                   D/ORPOR/12
                                                   D/ORPOR/24

     Research Triangle Park, NC   919              D/NCRTP/3

                                                   D/NCRTP/12
                                                   D/NCRTP/24

     Sacramento, CA               916              D/CASAC/3
                                                   D/CASAC/12
                                                   D/CASAC/24
                                  (Some exchanges must use 1 + phone number
                                   please check CASAC.xch for details)


     Salt Lake City, UT           801              D/UTSLC/3
                                                   D/UTSLC/12
                                                   D/UTSLC/24

     San Diego, CA                619              D/CASDI/3
                                                   D/CASDI/12
                                                   D/CASDI/24

     San Francisco, CA            415              D/CASFA/3
                                                   D/CASFA/12
                                                   D/CASFA/24


     San Jose, CA                 408 \            D/CASJO/3
                                       >           D/CASJO/12
                                  415 /            D/CASJO/24
				  (for 415, must use 1415 + phone number)

     Santa Ana, CA                714 \            D/CASAN/3
                                       >           D/CASAN/12
                                  213 /            D/CASAN/24
				  (for 213, must use 1213 + phone number)

     Seattle, WA                  206              D/WASEA/3
                                                   D/WASEA/12
                                                   D/WASEA/24

     St. Louis, MO                314 \            D/MOSLO/3
                                       >           D/MOSLO/12
                                  618 /            D/MOSLO/24
                                  (for 618, must use 1618 + phone number)

     Tampa, FL                    813              D/FLTAM/3
                                                   D/FLTAM/12
                                                   D/FLTAM/24


     Washington, DC               202 \            D/DCWAS/3
                                  703  >           D/DCWAS/12
                                  301 /            D/DCWAS/24
                                  (for 703, must use 703 + phone number)
                                  (for 301, must use 301 + phone number)


          Note:    /3 = 300 bps,  /12 = 1200 bps,  /24 = 2400 baud


-------------------------------------------------------------------------------                                                                                                                                                                                                                                                                                                                                                                                                                          
                                                                                                                                                                                                                                                                                                                     

Type CTL-K to skip this


NEW ID/PASSWORD SOFTWARE RELEASE

We just recently implemented a new ID/Password software release on SprintNet.
With this implementation, PC Pursuit and PC BusinessCall IDs will only
allow connections to be made to the following types of network addresses:

	-- Standard Mnemonic outdial "city codes"
	-- Those addresses of public "Pursuitable" hosts such as DELPHI.

Calls attempted to numeric rotary addresses (violating the Outdial Terms
and Conditions) will be blocked, and you will receive the message "ACCESS TO
THIS ADDRESS NOT PERMITTED".  Calls to standard mnemonic "city codes" will
see no change in service.

If you experience difficulty in accessing any publicly available("Pursuitable")
SprintNet host, please contact us via either this BBS or Tech Support at 
1-800-877-5045.

Thanks,

PC Pursuit Management


-------------------------------------------------------------------------------                                                                                
                                                                                                                                                                                     

                       How To Use PC Pursuit Service
                       -----------------------------

    Placing a PC Pursuit Call
    -------------------------

      * Use a modem to dial your local SprintNet access telephone
        number with parameters settings of 8-N-1.

      * Type two CARRIAGE RETURNS (CR) D (CR)


      Telenet  Prompt      User Input              Comments
      ======================================================================

(1)   Terminal =        D1 (CR)                    Input Terminal ID.
                                                   D1 is typical for
                                                   PC's. If not known,
                                                   type CR.

(2)   @                 C D/NYNYO/12,YOUR ID (CR)  Type area code desired,
                                                   modem speed and your
                                                   user ID. (Note that
                                                   /3 = 300 bps, /12 = 1200
						   bps, /24 = 2400 bps).

(3)   PASSWORD =        PASSWORD (CR)              Enter user Password

(4)   D/NYNYO/12                                   Connected to target
      CONNECTED                                    city outdial modem.

(5)                     ATZ                        Type ATZ (in upper case)

(6)   OK                                           Modem responds as cleared.

(7)                     ATDT 7654321               Type ATDT (in upper case)
                                                   and the 7-digit number
                                                   you wish to dial.

(8)   CONNECT           (CR) (CR)                  You are now connected to
                                                   the computer that you
                                                   dialed. Procees as if
                                                   the  number was dialed
                                                   directly.


    NOTES:
    -----

    1. If the connection was not made, a BUSY will be seen within 30
       seconds. The BUSY message means that the number dialed was either
       busy, not in service, or an invalid attempt to dial more than 7
       digits. A BUSY will also be seen after disconnecting from the
       host computer, but you can dial another number by starting again
       at the fifth step and typing ATZ and dialing the number.

    2. PC Pursuit uses standard HAYES dialing commands, which enable
       you to type the A/ (no CR) command to redial the previously
       dialed number.

    3. When a typing mistake is made in the second and third steps,
       the log-on must be re-entered.


    To Disconnect from PC Pursuit
    -----------------------------

      Telenet Prompt      User Input               Comments
      ======================================================================

                          (CR) @ (CR)              Escape to SprintNet 
                                                   command level.

      @                   D (CR)                   At the @ sign,issue
                                                   disconnect command.

      D/NYNYO/12                                   Disconnect from the
      DISCONNECTED                                 target city complete.
                                                   User is still connected
                                                   to SprintNet at the local
                                                   dial-up city. A PC Pursuit
                                                   can now be placed to
                                                   another city.


    NOTES:
    ------

    1. To DISCONNECT FROM SPRINTNET, log off your computer as usual, or
       hang-up.



<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

                    Equipment and Software Requirements
                    -----------------------------------

       To use PC PURSUIT, all you need are --

       - a telephone line
       - a modem - 300 or 1200 bps
       - a terminal or a PC with asynchronous communications software

       PARAMETERS:
       -----------
       Communication parameters for your hardware should be set-up
       consistent with the PC or BBS or host computer you wish to dial.

       FILE TRANSFERS:
       ---------------
       Most transfer protocols are compatible with PC PURSUIT.
       Across SPRINTNET'S Public Data Network, PC PURSUIT transmits
       data utilizing 8 bit transparency. Due to XMODEM'S use of
       single block by block acknowledgement of data sent, XMODEM
       file transfers can take slightly longer. There are
       however, more efficent transfer protocols such as KERMIT,
       SUPER KERMIT and YMODEM.

       You can now dial into SprintNet as 7-E-1 or 8-N-1.  If you dial
       in at 7-E-1, you can switch your parameters to 8-N-1 with
       your software to prepare for a file transfer.  Or, dial
       SprintNet at 8-N-1 to begin with, using these steps --

       1) Dial your SprintNet local access number with your settings
          at 8-N-1.

       2) Enter  (cr) D (cr)

       3) At "Terminal = ", enter  D1 (cr)

       4) proceed with your session....

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>


            PC PURSUIT AND SPRINTNET LOCAL ACCESS NUMBERS


     FOR THE MOST UP-TO-DATE LISTING OF THE PC PURSUIT U.S. ACCESS
     TELEPHONE NUMBERS, DO THE FOLLOWING:

     1. USE A MODEM TO DIAL 1-800-546-1000 WITH PARAMETERS SET AT
        7-E-1.

     2. TYPE THREE CARRIAGE RETURNS (CR) (CR) (CR)

     3. INPUT YOUR AREA CODE AND LOCAL EXCHANGE

     4. YOU WILL THEN RECEIVE THE PROMPT  SIGN "@"

     5. THEN, TYPE:
                    MAIL (CR)
                    USER NAME: PHONES (CR)
                    PASSWORD: PHONES  (CR)

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>
<*>                         File Transfers                                 <*>  
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>

     This section outlines the most common  file  transfer  protocols  used
     with  PC  Pursuit. The performance of the protocols in the direct con-
     nect and PC Pursuit environments are also indicated.

     The following protocols were tested via the  Chicago  in-dial  to  the
     Washington DC out-dial; the observations are summarized below.


     XMODEM

     PC Pursuit XMODEM file transfers performed at an average throughput of
     34%  when  the  correct  hunt-confirm  and terminal type was utilized.
     XMODEM does not support flow control, therefore it is  suggested  that
     the  "relaxed"  mode  be invoked if the user's communications software
     permits this feature.


     YMODEM

     The performance of YMODEM file transfers VIA PC Pursuit was  found  to
     have  an  average  throughput of 77% when the correct hunt confirm and
     terminal type is employed.  Although  YMODEM  does  not  support  flow
     control, it uses large 1024 byte packets which the network PAD handles
     quite  readily  under  normal conditions. As a result, YMODEM is rated
     one of the faster protocols for file transfer via PC Pursuit.


     WXMODEM

     WXMODEM file transfers utilizing the correct hunt-confirm and terminal
     type performed well  with  an  average  transfer  rate  of  82%.  This
     protocol  is  capable  of  handling  flow  control which enables it to
     perform with better reliability in the PC Pursuit  environment.  Users
     should  be  aware  that an early version of PROCOMM is known to have a
     software problem which can affect  the  performance  of  WXMODEM  file
     transfers.

     KERMIT

     An  optimum  average  throughput  of  65%  was obtained by KERMIT file
     transfers via PC Pursuit. The throughput was obtained  with  a  packet
     size of 90 and a window size of 31. KERMIT software which supports the
     sliding  window  feature  performs  with  optimum efficiency in the PC
     Pursuit environment.

     SEALINK

     SEALINK file transfers via PC  Pursuit  performed  exceptionally  well
     with  an  average  throughput of 91% with the correct hunt-confirm and
     terminal type. SEALINK supports  flow  control  and  was  specifically
     designed  to  operate  in the networking environment. Some versions of
     SEALINK however, do not provide proper error recovery which could pose
     a problem for some users.

     ZMODEM

     File transfers utilizing ZMODEM protocol via  PC  Pursuit  yielded  an
     average  transfer  rate of 93%. ZMODEM performs well in the PC Pursuit
     environment at the default settings. Depending on  the  type  of  user
     equipment,  ZMODEM  options  may need to be modified to permit optimum
     throughput. The ZMODEM command line used in our test configuration was
     simply as follows:


         Uploads:     DSZ port 1 rz
         Downloads:   DSZ port 1 sz


     The  X.3  PAD  parameters  which  provide  optimum   performance   are
     1:0,4:10,5:1, 7:8,12:1. In addition, flow control (XON/XOFF) should be
     enabled  at  the user PC and the host. It should be noted that in most
     cases these additional PAD parameters are optional and  need  only  be
     employed if the user is experiencing difficulty transferring files via
     ZMODEM.


     STEP 1.:    Set PC communications software to 8 bits, no parity,
                 1 stop bit, full duplex. At this time, the user may wish
                 disable or enable local (XON/XOFF) flow control depending
                 on the type of protocol to be used.

     STEP 2.:    Dial local rotary with the communications software
                 set at the desired speed.

     STEP 3.:    Upon connect use the correct hunt confirm sequence:
                     At 300/1200bps use - <CR D CR>
                     At 2400bps         - <@ D CR>
                     NOTE: "D" MUST BE UPPER CASE.

     STEP 4.:    At prompt "TERMINAL = " enter  <D1> and return.

     STEP 5.:    At the "@" prompt enter the destination mnemonic,
                 out-dial speed, ID and password.  It is important
                 that out-dial speed matches in-dial speed.
                 DO NOT MIX IN-DIAL AND OUT-DIAL SPEEDS.

     STEP 6.:    If OPTIONAL X.3 pad parameters are to be changed, do
                 so at this point by entering <@ CR>. To set parameters
                 as prescribed perform the following:

                 To set parameters enter <SET parameter,parameter>
                     Example: SET 7:8,4:10,5:1,7:8,12:1
                 To read parameters enter <PAR?>

                 Return to out-dial port by entering
                 <CONT>.

     STEP 7.:    Upon connecting to the destination pad, ensure
                 communication with the out-dial modem by entering <ATZ>.
                 The destination modem will respond with "OK".

     STEP 8.:    Enter <ATD> and the local number you wish to dial.

     STEP 9.:    Queue host file transfer and start file transfer.


     If you are experiencing trouble with PC Pursuit  check  the  following
     items:

     * Verify the correct hunt-confirm sequence

     * Verify user software comm parameters are set to 8 bits, no parity and
       1 stop bit.

     * If problems with file transfer only, try the optional ITI PAD parameters.


                                  FILE TRANSFER
                              PERFORMANCE STATISTICS

  General Communication Parameters = 8 bits
                                     1 stop bit
                                     N no parity

  Terminal Type = D1

  |          PERFORMANCE STATISTICS DIRECT CONNECT       |
  |                                                      |
  |                                                      |
  |                                                XFR   |
  | PROTOCOL    SPEED  SECONDS      CPS       BPS  RATE  |
  |======================================================|
  |                                                      |
  | ZMODEM UP    1200   ***394   114.36   1143.55   95%  |
  | ZMODEM UP    2400   ***199   226.41   2264.12   94%  |
  | ZMODEM DN    1200   ***394   114.36   1143.55   95%  |
  | ZMODEM DN    2400   ***196   229.88   2298.78   96%  |
  |                                                      |
  | SEALINK UP   1200   ***418   107.79   1077.89   90%  |
  | SEALINK UP   2400   ***200   225.28   2252.80   94%  |
  | SEALINK DN   1200   ***400   112.64   1126.40   94%  |
  | SEALINK DN   2400   ***205   219.79   2197.85   92%  |
  |                                                      |
  | WXMODEM UP   1200   ***405   111.25   1112.49   93%  |
  | WXMODEM UP   2400   ***205   219.79   2197.85   92%  |
  | WXMODEM DN   1200    **277    96.12    961.16   80%  |
  | WXMODEM DN   2400   ***216   208.59   2085.93   87%  |
  |                                                      |
  | YMODEM UP    1200   ***387   116.42   1164.24   97%  |
  | YMODEM UP    2400   ***194   232.25   2322.47   97%  |
  | YMODEM DN    1200   ***385   117.03   1170.29   98%  |
  | YMODEM DN    2400   ***199   226.41   2264.12   94%  |
  |                                                      |
  | KERMIT UP    1200   ***553    81.48    814.76   68%  |
  | KERMIT UP    2400   ***287   156.99   1569.90   65%  |
  | KERMIT DN    1200   ***571    78.91    789.07   66%  |
  | KERMIT DN    2400   ***295   152.73   1527.32   64%  |
  |                                                      |
  | XMODEM UP    1200   ***425   106.01   1060.14   88%  |
  | XMODEM UP    2400   ***219   205.74   2057.35   86%  |
  | XMODEM DN    1200   ***436   103.34   1033.39   86%  |
  | XMODEM DN    2400   ***228   197.61   1976.14   82%  |
   =======================================================

  * Optional PAD parameters which optimize performance
  ** File size = 26624   *** File size = 45056



|                                               PERFORMANCE STATISTICS VIA PCP                    
                  |
|                                                                                                 
                  |
|                                                HUNT             OPTIONAL ITI                    
                  |
|                                         XFR  CONFIRM   FLOW     X.3 PAD                         
                  |
| PROTOCOL   SPEED SECONDS    CPS      BPS  RATE  SEQUENCE CONTROL  PARAMETERS               NOTES
                  |
|=================================================================================================
==================|
|                                                                                                 
                  |
| ZMODEM UP   1200  ***399  112.92  1129.22  94%  CR D CR  XON/XOFF *1:0,4:10,5:1,7:8,12:1 *Host a
terminal XON/XOFF |
| ZMODEM UP   2400  ***200  225.28  2252.80  94%   @ D CR  XON/XOFF *1:0,4:10,5:1,7:8,12:1 *Host a
terminal XON/XOFF |
| ZMODEM DN   1200  ***398  113.21  1132.06  94%  CR D CR  XON/XOFF *1:0,4:10,5:1,7:8,12:1 *Host a
terminal XON/XOFF |
| ZMODEM DN   2400  ***204  220.86  2208.63  92%   @ D CR  XON/XOFF *1:0,4:10,5:1,7:8,12:1 *Host a
terminal XON/XOFF |
|                                                                                                 
                  |
| SEALINK UP  1200  ***420  107.28  1072.76  89%  CR D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
| SEALINK UP  2400  ***202  223.05  2230.50  93%   @ D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
| SEALINK DN  1200  ***402  112.08  1120.80  93%  CR D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
| SEALINK DN  2400  ***207  217.66  2176.62  91%   @ D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
|                                                                                                 
                  |
| WXMODEM UP  1200  ***406  110.98  1109.75  92%  CR D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
| WXMODEM UP  2400  ***263  171.32  1713.16  71%   @ D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
| WXMODEM DN  1200  ***469   96.07   960.68  80%  CR D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
| WXMODEM DN  2400  ***214  210.54  2105.42  88%   @ D CR  XON/XOFF *7:8,1:0               *Host a
terminal XON/XOFF |
|                                                                                                 
                  |
| YMODEM UP   1200  ***467   96.48   964.80  80%  CR D CR     NONE  *7:8,1:0                      
                  |
| YMODEM UP   2400  ***252  178.79  1787.94  74%   @ D CR     NONE  *7:8,1:0                      
                  |
| YMODEM DN   1200  ***461   97.74   977.35  81%  CR D CR     NONE  *7:8,1:0                      
                  |
| YMODEM DN   2400  ***263  176.00  1760.00  73%   @ D CR     NONE  *7:8,1:0                      
                  |
|                                                                                                 
                  |
| KERMIT UP   1200  ***558   80.75   807.46  67%  CR D CR  XON/XOFF *7:8,1:0                      
                  |
| KERMIT UP   2400  ***285  158.09  1580.91  66%   @ D CR  XON/XOFF *7:8,1:0                      
                  |
| KERMIT DN   1200  ***579   77.82   778.17  65%  CR D CR  XON/XOFF *7:8,1:0                      
                  |
| KERMIT DN   2400  ***297  151.70  1517.04  63%   @ D CR  XON/XOFF *7:8,1:0                      
                  |
|                                                                                                 
                  |
| XMODEM UP   1200  ***985  45.74   457.42   38%  CR D CR     NONE  *7:8,1:0                      
                  |
| XMODEM UP   2400  ***636  70.84   708.43   30%   @ D CR     NONE  *7:8,1:0                      
                  |
| XMODEM DN   1200 ***1001  45.01   450.11   38%  CR D CR     NONE  *7:8,1:0                      
                  |
| XMODEM DN   2400  ***636  70.84   708.43   30%   @ D CR     NONE  *7:8,1:0                      
                  |
===============================================================================

 * Optional PAD parameters  ** File size = 26624   *** File size = 4506


<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>
<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>
<*>                     What the f***! is a Racal-Vadic?!?                  <*>
<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>



 OVERVIEW
----------
   The Racal-Vadic mode is an unsupported and to date, poorly documented
feature of the outdial modems that are currently in use with PC Pursuit.
It enables you to better understand what is happening at the other end of
your connection by telling you what is happening. This type of operation is
known as "call progression" because it gives you a response as the modem
progresses through the phone call.


 ACITVATING AND DEACTIVATING THE MODE
--------------------------------------
   The first thing we will cover is how to activate and de-activate the
Racal-Vadic mode. Some of you may have already experienced the rather
unexpected "MANUAL ANSWER" response after entering the Hayes command
"ATZ". What has happened is that you have connected with a modem that
is already in the Racal-Vadic mode of operation. When you entered "ATZ",
the 'A' was sensed by the modem as the command to manualy answer the
phone line. If this happens, just press your return key. This will make
the modem return to command mode signified by the '*' prompt. While at
this prompt you could enter an 'I' and then press return. This will make
the modem <I>dle the Racal-Vadic mode and return you to the Hayes mode
of operation.

   If, on the other hand, you were to receive the normal "OK" response
from the modem after entering the "ATZ" command. You can activate the
Racal-Vadic mode by entering <CTRL>-E and pressing the return key. The
modem will now respond with "HELLO, I'M READY" and the '*' prompt.

   To summarize activation and de-activation:

      From the Hayes mode - <CTRL>-E and <RETURN> - to activate.

      From the '*' prompt - <I> and <RETURN> - to de-activate.

   I suggest getting into the habit of sending the de-activation sequence
when you first connect to a city node so that you know exactly what mode
the modem is in. You should also send an "ATZ" to make sure that the modem
is operational by seeing if the modem sends you back an "OK" response.
You can then send the activation command to enter Racal-Vadic mode.

   There are two cases where the modem will return by itself to the Hayes
mode. The first is after you connect to a BBS. The other is while you're
at the command prompt and haven't entered anything for a short period of
time. 


 DIALING
---------
   Now your ready to dial a phone number using the Racal-Vadic mode.
To do this, just enter a 'D' followed by the number you wish to dial.
For example, "D1234567", (pressing return of course!) will dial 123-4567.

   Well, we've dialed a phone number, what now? After all, any modem can
dial a number, right? But not every modem can tell you what follows...


 RESPONSE MESSAGES
-------------------
   The following is a short description of each response the Racal-Vadic
mode can give you while dialing. They are, for the most part, self-
explanatory. But there are a few things you should consider with some of
them and I'll point those out just in case.

   DIALING...   -  The modem has detected a dial tone and is now dialing
                  the phone number.

   NO DIAL TONE -  Just what it means, no dial tone was detected. Try again,
                  if you keep getting this then there is something wrong with
                  either the modem or the telephone line on that end. Contact
                  Customer Support and tell them you experienced this, tell 
                  them the city node you were connected to also.

   BUSY!        -  A busy signal has been detected. This is not the same
                  kind of BUSY as you'd get in the Hayes mode. There is
                  circuitry in the modem that can sense a busy signal, so
                  it will return to the command mode quicker to allow you
                  to decide what to do next. (Please see my note about the
                  BUSY response below also)

   RINGING...   -  Self-explanatory.

   ANSWER TONE  -  Self-explanatory.
 
   ON LINE      -  Self-explanatory.

   FAILED CALL  -  The phone rang for ten times with no answer. Either the
                  the BBS you called is down or no longer in existence, or
                  you reached someone's home and they weren't there.


 REDIALING A NUMBER
--------------------
   After you have received a BUSY! response you can re-dial the same 
phone number up to 9 times with the 'R' command. To use this command,
enter an "R" and press the return key.


 DISCONNECTING WHILE ONLINE
----------------------------
   In a manner similar to the "+++" "ATH" Hayes command sequence, there
is a two control code sequence that will dis-connect you from the BBS
you are connected to. To activate it press <CTRL>-C then <CTRL>-D.

   Prior to disconnecting from the city node, make sure the modem is not
in Racal-Vadic mode by issuing the <I>dle command. Be nice to others that
may not be aware of this mode of operation yet!


 OTHER COMMANDS
----------------
   The command 'P' or '?' will print the following list of commands that
the modem is designed to use. Since these are not needed in order to use
the Racal-Vadic mode effectively they will not be discusssed. This list
is here purely for your information.


                     A            MANUAL ANSWER
                     D            DIAL NUMBER
                     G            MANUAL ORGINATE
                     I            IDLE
                     K            PAUSE
                     O            OPTIONS
                     P,?          PRINT MENU
                     R            REDIAL
                     T            TABLE OF OPTIONS
                     CONTROL  A   ALB TEST
                     CONTROL (CD) DISCONNECT
                     CONTROL  D   REQUEST DLB TEST
                     CONTROL  H   BACKSPACE


 BEWARE THE BUSY
-----------------
   The BUSY! response primarily indicates that the phone number you dialed
was busy, common sense tell you that. What I want to point out to you in
this section is that there are other possibilities that could mean that
something else is actually occuring.


 a. CONTINUOUS BUSIES
----------------------
      The first thing to be aware of is Telenet's exchange lock-out feature.
   This prevents you from making a long-distance call or any local calls
   to exchanges that Telenet would be charged more than is profitable. All
   you will know is that you constantly get BUSY! responses when you dial a
   certain phone number. The response tends to be returned from the modem
   much quicker then a legitimate BUSY! for a valid phone number. This is
   not a hard and fast rule though. Two methods that are available to you
   for determining if this is the cause of the continuous busies are:

      1. -   Check the exchange lists provided by Telenet, if the exchange is
            not listed for the number your calling, you may as well stop
            wasting anymore time calling that number. It is a victim of the
            exchange lock-out.

      2. -   If the exchange is listed but you've always received a BUSY!
            response, try this. Hang-up from Telenet and dial the number
            direct. If you hear a busy signal you can continue trying some
            more, you may have latched onto a very, very busy system. But
            if the phone rings, hang-up immediately. This way you won't be
            charged for the call. You should then leave word with Customer
            Support or on the Net-Exchange that this happened. Telenet may
            have a typo concerning that exchange.


 b. RINGING... BUSY!
---------------------
      There are a few things that can cause this. Although I'm not talking
   about the RING BUSY RING BUSY... loop that can occure when you first
   connect to a city node. You can get out of that by rapidly and repeatedly
   sending an "ATZ" to the modem in an effort to break out of the loop. There
   is a narrow window where this will succeed, but it can be done.

      The main cause of this is by dialing a person's phone instead of a BBS.
   This will usually be followed by a variable number of rings prior to
   getting the BUSY!. Make certain that the phone number you have is really
   a BBS. If you've never called that BBS before, you may have a case where
   the BBS folded and someone else received the phone number after the sysop
   canceled that phone line. A BBS less than 6 months old or with less than
   24 hour access can be highly suspect. New and odd-hour BBS's tend to come
   and go rather often.

      If you want to continue to dial this number, first call direct to make
   sure that it isn't a person's phone. Constantly getting a carrier signal
   in your ear is not a pleasurable experience. You would also be doing them
   a favor by letting them know that their new phone number used to be a
   BBS. If that's the case they've probably been getting a ton of bizzare
   calls, especially late at night, and could benefit from your call so that
   they can get their number changed.

      If, on the other hand, you receive a carrier signal, try the other
   Baud rate. if that doesn't work you could have reached a private system
   that is looking for a logon sequence immediately or will dis-connect you.

      Another possibility is that the BBS you've called has bombed and the
   modem is dutifully answering calls but there is no computer program 
   operating to give you feed-back.

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><
<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><
<*>               Making the Best of your protocols                         <*>
<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><
To modify MNP setting in the Hayes command mode:

    AT*E0      No MNP
    
    AT*E1      Auto MNP
 
    AT*E2      Force MNP (call will fail if MNP unavailable)
 
To modify MNP setting in Racal-Vadic mode:

    connect to modem and get to R/V mode (^E<cr>)
    O<cr>
    2<cr>    (you want one of the options in group 2)
    (system reponds with a list)
    19<cr>
    (system responds with option 19 and possible settings)

    1<cr>   (auto error control)
         --or--
    2<cr>   (disable error control)
         --or--
    3<cr>   (force error control)

    0<cr>   (return to previous menu)
    0<cr>   (return to previous menu)
    4<cr>   (menu item is "EXECUTE")

    At this point you will get back the * prompt of the 
    Racal-Vadic mode.

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

                 How to access and set the ITI parameters


    All commands are entered at the Telenet network @ prompt.


    X.3 ITI Parms
    -------------

    To Display:

            Enter:

                   "PAR?<cr>"


            The network will respond:

                   "PAR1:<value>,2:<value>,..."


    To Change:

            Enter:

                   "SET? <parm>:<value>,<parm>:<value>,...."

            The network will respond:

                   "PAR<parm>:<value>,..."


    Telenet ITI Parms
    -----------------

    To Display:

            Enter

                   "PAR? 0,<parm>,<parm>,..."

            The network will respond:

                   "PAR<parm>:<value>,<parm>:<value>,..."


    To Change:

            Enter
                  "SET? 0:33,<parm>:<value>,<parm>:<value>,..."


            The network will respond:

                   "PAR0:33,<parm>:<value>,..."


<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

                             X.3 ITI Parameters
                             ------------------

  Para-
  meter  Description
  -----  -----------

    0    National Options Marker

         This parameter serves to mark the division between International
         (X.3) parameters and Network Dependent (e.g., Telenet) paramaters
         in an X.28 or X.29 parameters list.  All parameters preceding the
         marker are X.3, and those following are Network Dependent.  Values
         may be:

             0  CCIT specified value
            33  Telenet permitteed value

         Telenet accepts either value.  Whenever possible, the CCITT
         specified value of zero should be used.


    1    Escape to Command Level

         This paramter allows the terminal to initiate an escape from Data
         Transfer Mode, in order to send a command to the PAD. Values are:

             0  Escape not possible
             1  Escape possible (default)


    2    Echo

         This paramter provides for all characters received from the
         terminal to be transmitted back to the terminal, as well as being
         interpreted and forwarded by the PAD to the the remote DTE.
         Values are:

             0  No echo
             1  Echo (default)


    3    Data Forwarding

         This paramter allows the PAD to recognize defined character(s)
         received from the terminal as an indication to complete assembly
         of characters to forward a DATA packet to the remote DTE.  Values
         may be OR-ed together (e.g., value of 3=1+2=Alphanumerics plus
         Carriage Return)

             0  No signal
             1  Alphanumerics
             2  Carriage Return (Default)
             4  Escape
             8  Editing Characters
            16  Terminators
            32  Form Effectors
            64  Control Characters
           128  Other Characters (Not valid according to CCITT
                recommendations)


    4    Idle Timer

         Should the interval between successive characters received from
         the terminal exceed the selected Idle Timer delay, the PAD will
         terminate assembly of characters and forward a DATA packet to the
         remote DTE.  Values are:

             0  Timer disabled
             n  multiples of 50 ms (.05 seconds), where 1<=n<=255.  n=1
                n=1 and n=2 not recommended.  (Default is 80, 4 seconds)


    5    Ancillary Device Control

         This paramter enables flow control between the PAD and the
         terminal.  The PAD uses the XON and XOFF characters (decimal 17
         and 19) to indicate to the terminal whether ir not it is ready to
         accept characters.  Values are:

             0  No use if XON/XOFF (default)
             1  Use XON/XOFF


    6    Suppression of Service Signals

         This paramter provides for the supression of all messages sent by
         the PAD to the terminal.  Values are:

             0  Signals not transmitted (messages not sent)
             1  Signals transmitted (messages sent) (Default)


    7    Break Options

         This paramter specifies the action taken on receipt of a Break
         signal from the terminal.  The only valid values are:

             0  Do nothing (Default)
             1  Send INTERRUPT Packet to Host
             2  Send RESET Packet to Host
             8  Escape to PAD Command State
            21  Flush-on-Break (Discard Output, Send Indication of Break
                and Send INTERRUPT)


    8    Discard Output

         This controls transmission of data to the terminal.  Values are:

             0  Normal data delivery to the terminal (Default)
             1  Discard all output to the terminal


    9    Carriage Return Padding

         This paramter provides for automatic insertion by the PAD of null
         character padding after the transmission of a carriage return to
         the terminal.  Values are:

             0  No padding
          1-31  Number of character delays


   10    Line Folding

         This provides for automatic insertion by the PAD of appropriate
         format effectors to prevent overprinting at the end of a terminal
         print line.  Values are:

             0  No line folding
             n  Character per line before folding, where 1<=n<=255


   11    Binary Speed

         This paramter is set by the PAD when the terminal establishes a
         physical connection to the network.  This allows the remote DTE
         or terminal user to examine the speed, as determined by the PAD.
         Values are:

             0    110    bps
             1    134.5
             2    300
             3    1200
             4    600
             5    75
             6    150
             7    1800
             8    200
             9    100
            10    50
            11    75/1200
            12    2400
            13    4800
            14    9600
            15    19,200
            16    48,000
            17    56,000
            18    64,000


   12    Flow Control of the PAD by the terminal

         This allows for flow control between the terminal and the PAD.
         The terminal indicates whether or not it is ready to accept
         characters from the PAD, via XON and XOFF characters.  Values
         are:

             0  No use of XON/XOFF
             1  Use XON/XOFF


   13    Linefeed Insertion

         This paramter instructs the PAD to routinely insert a linefeed
         (LF) character into the data stram following each appearance of a
         carriage return (CR) character.  Values may be OR-ed together:

             0  No LF Insertion (TP4 Default)
             1  Insert LF after CR on output to the terminal
             2  Insert LF after CR on input from the terminal
             4  Insert LF after CR on echo to the terminal


   14    Linefee Padding

         This paramter provices for automatic insertion by the PAD of null
         character padding after the transmission of a linefeed to the
         terminal.  Values are:

             0  No padding
          1-15  null characters


   15    Editing

         This paramter enables local editing of text within the PAD before
         transmission through the network.  Note, if editing is enabled,
         transmission on timers is disabled.  Values are:

             0  Editing disabled (Default)
             1  Editing enabled


   16    Character Delete

         Parameter 16 specifies the editing character which causes the PAD
         to erase the previous character entered by the terminal.  Parameter
         16 is only valid if editing is enabled.  Default is 127.


   17    Line Delete

         Parameter 17 specifies the editing character which causes the PAD
         to erase the entire buffer.  If data is forwarded on carriage
         return only, the buffer contains one line at a time.  Parameter 17
         is only valid if editing is enabled.  Default is 24.


   18    Line Display

         Parameter 18 specifies the editing character which causes the PAD
         to echo the entire buffer to the terminal.  Paramter 18 is only
         valid if editing is enabled.  Default is 18.

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

                           Telenet ITI Parameters
                           ----------------------


                      Summary of Telenet ITI Parameters
                      ---------------------------------

 Para-                               Para-
 meter  Description (Default Value)  meter  Description (Default Value)
 -----  ---------------------------  -----  ---------------------------
   1    Line feed Insertion (0)       31+   Interrupt Character (0)
   2    Network Message Display (0)   32    Automatic Hang-up (0)
   3    Echo (1)                      33+   Flush Output (0)
   4    Echo Mask (163)               34    Transmit on Timers (1)
   5    Transmit Mask (2)             35    Idle Timer (80)
   6*   Buffer Size (0)               36    Interval Timer (0)
   7*   Command Mask (127)            37    Network Usage Display (0)
   8*   Command Mask (3)              38    Carriage Return PAD (Variable)
   9    Carriage Return PAD (Fixed)   39    Padding Options (1)
  10    Linefeed Padding              40    Insert on Break (0)

  11    Tab Padding                   41    PAD-Terminal Flow Control (0)
  12    Line Width                    42    PAD-Terminal XON Character (17)
  13    Page Length (0)               43    PAD-Terminal XOFF Character (19)
  14    Line Folding (1)              44*   Generate Break (INV)
  15    Page Wait (0)                 45*   APP on Break (0)
  16    Interrupt on Break (0)        46    Input Unlock Option (0)
  17    Break Code (0)                47    Input Unlock Timer (0)
  18    NVT Options (0)               48    Input Unlock Character (0)
  19    Initial Keyboard State (0)    49    Output Lock Option (2)
  20    Half/Full Duplex              50    Output Lock Timer (10)

  21    Real Character Code           51    Output Lock Option (0)
  22    Printer Style                 53*   Break Options (0)
  23    Terminal Type                 54    Terminal-PAD Flow Control (0)
  24    Permanent Terminal (0)        55    Terminal-PAD XON Character (17)
  25    Manual or Auto Connect (0)    56    Terminal-PAD XOFF Character (19)
  26    Rate                          57    Connection Mode (2)
  27    Delete Character (127)        58    Escape to Command Mode (1)
  28    Cancel Character (24)         59*   Flush Output on Break (0)
  29    Display Character (18)        60    Delayed Echo
  30+   Abort Output Character (0)    63    Eight-bit Transparency (1)
                                      64+   Early ACK (0)
                                      65    More-Data Bit Generation (3)
				      66    Defer Processing of User (0)
				      67    ESP Packetizing Option (0)
				      68    Escape Sequence Timer (0)
				      69    Escape Sequence Maximum Length (0)
				      70    Escape Sequence Initiator (0)
				      71    Parameter Reset on Disconnect (0)

  Note:  All Telenet Parameters must follow the National Option Marker
         (Parameter 0, value '21' Hex) in PAD Messages.

         Parameters marked with "*" should not be used.

         Parameters marked with "+" should be used with caution.






            Telenet ITI Parameters Arranged by Functional Category
            ------------------------------------------------------

 Para-                                 Para-
 meter  Description (Default Value)    meter  Description (Default Value)
 -----  ---------------------------    -----  ---------------------------

            (CONNECTION MODE)                  (BREAK HANDLING)
  57   Connection Mode (2)               16    Interrupt on Break (0)
  58   Escape to Command Mode (1)        40    Insert on Break (0)
                                         17    Break Code (0)
      (CALL ESTABLISHMENT & CLEARING)    44*   Generate Break (INV)
  25   Manual or Auto Connect (0)        45*   APP on Break (0)
  32   Automatic Hang-up (0)             59*   Flush Output on Break (0)
                                         53*   Break Options (0)
          (COMMAND PROTECTION)
   7*  Command Mask (127)                     (VIRTUAL TERMINAL DEVICE)
   8*  Command Mask (3)                  39    Padding Options (1)
                                          9    Carriage Return PAD (Fixed)
          (DEVICE DEPENDENT)             38    Carriage Return PAD (Variable)
  24   Permanent Terminal (0)            10    Linefeed Padding
  23   Terminal Type                     11    Tab Padding
  20   Half/Full Duplex                  12    Line Width
  21   Real Character Code               13    Page Length (0)
  22   Printer Style                     14    Line Folding (1)
  26   Rate                              15    Page Wait (9)
  63   Eight-bit Transparency (1)         1    Linefeed Insertions (0)

          (TERMINAL DISPLAY)                   (VIRTUAL TERMINAL PROCESS)
   3   Echo (1)                          18    NVT Options (0)
   4   Echo Mask (163)                   27    Delete Character (127)
   2   Network Message Display (0)       28    Cancel Character (24)
   37  Network Usage Display (0)         29    Display Character (18)
   60  Delayed Echo (0)                  31    Interrupt Character (0)
                                         30    Abort Output Character (0)
      (PACKET ASSEMBLY/DISASSEMBLY)      33    Flush Output (0)
   6*  Buffer Size (0)                  
   5   Transmit Mask (2)
  34   Transmit on Timers (1)                 (2741 Terminal Support)
  35   Idle Timer (80)                   19    Initial Keyboard State (0)
  36   Interval Timer (0)                46    Input Unlock Option (0)
  60   Delayed Echo                      47    Input Unlock Timer (0)
  64   Early ACK (0)                     48    Input Unlock Character (0)
  65   More-Data Bit Generation (3)      49    Output Lock Option (2)
                                         50    Output Lock Timer (10)
      (RESELECT HANDLING)                51    Output Lock Option (0)
  66   Defer Processing of Input
  71   Parameter Reset on Disc (0)          (ESCAPE SEQUENCE PROCESSING)
                                         67    ESP Packetizing Option (0)
             (FLOW CONTROL)		 68    Escape Sequence Timer (0)
  41   PAD-Terminal Flow Control (0)	 69    Escape Sequence Length (0)
  42   PAD-Terminal XON Character (17)   70    Escape Sequence Initiator (0)
  43   PAD-Terminal XOFF Character (19)
  54   Terminal-PAD Flow Control (0)
  55   Terminal-PAD XON Character (17)
  56   Terminal-PAD XOFF Character (19)


               Parameters marked with "*" should not be used.


                       Detail of Telenet ITI Parameters
		
  Following is a description of each of the Telenet ITI parameters. Defaults
  for Telenet Public Dial Ports are noted

  As noted by (+) use the equivalent X.3 parameter wherever possible

  Parameters marked (*) are archaic and should not be used.


  Para-
  meter  Description
  -----  -----------

   +1    Linefeed Insertion

         This parameter instructs the PAD to routinely insert a linefeed
         (LF) character into the data stream following each appearance of a
         carriage return (CR) character.  Values may be OR-ed together:

             0  No LF Insertion (Default)
             1  Insert LF after CR on output to the terminal
             2  Insert LF after CR on input from the terminal
             4  Insert LF after CR on echo to the terminal


   +2    Network Message Display

         This parameter controls the transmission of network-oriented
         messages to the terminal.  Values are:

             0  Transmit network-oriented messages (Default)
             1  Suppress network-oriented messages


   +3    Echo

         This specifies whether or not the network returns images of
         characters entered from the terminal during Data Transfer mode.
         Values are:

             0  Network does not echo
             1  Network echoes according to the Echo Mask (Default)


    4    Echo Mask

         The Echo Mask specifies which characters are to be echoed during
         Data Transfer mode.  Values may be OR-ed together:

             1  Alphanumerics
             2  Carriage Return
             4  Escape
             8  Editing Characters
            16  Terminators
            32  Form Effectors
            64  Control Characters
           128  Other Characters

           Default is 163 = 1+2+32+128 (Alphanumerics, Carriage Return, Form
           Effectors, and Other Characters).


   +5    Transmit Mask

         The Transmit Mask specifies those characters which indicate a
         logical break in the data being entered from a terminal and which
         force transmission of that data to its destination.  Values may be
         OR-ed together:

             0  Transmission on Transmit Mask disabled
             1  Alphanumerics
             2  Carriage Return  (Default)
             4  Escape
             8  Editing Characters
            16  Terminators
            32  Form Effectors
            64  Control Characters
           128  Other Characters

	   Note:  see Character Codes and Masking Categories below


   *6    Buffer Size

         This parameter is archaic and should no longer have any affect on a
         TP.  It is used to specify the maximum number of characters that
         will be accumulated by the network before they are forwarded to the
         Host.

             0  Buffer 256 characters (Default)
         1-255  Buffer 1-255 characters


   *7    Command Mask

         This is an archaic parameter.  Its use has been phased out, but the
         parameter number has not be redefined for another function.


   *8    Command Mask

         This is an archaic parameter which has not been redefined to
         support another function.


   +9    Carriage Return Padding

         The Carriage Return Padding parameters specify the number of PAD
         character times to be inserted after each carriage return
         character sent to the terminal.  Parameter 9 specifies the Fixed
         Component. Values may run from 0 through 31 character-times of
         padding provided.


  +10    Linefeed Padding

         This specifies the number of pad character delays inserted after
         each linefeed (LF) character sent to the terminal.  Values may
         range from 0 through 15 character-times of padding provided.


   11    Tab Padding

         This specifies the number of pad character delays inserted after
         each horizontal tabulation (HT) character sent to the terminal.
         Values may range from 0 through 15 character-times of padding
         provided.


   12    Line Width

         This identifies the number of character positions per terminal
         print line.  Values range from 1 through 255 characters per line;
         or 0, which specifies 256 characters per line.


   13    Page Length

         This parameter identifies the number of lines per terminal page or
         display screen.  Values range from 1 through 255 lines per page; or
         0, which specifies an infinite page length.


   14    Line Folding

         This parameter specifies whether or not the PAD begins a new line
         when the number of characters in a print line exceeds the line
         width:

             0  Disable line folding
             1  Enable line folding (Default)


   15    Page Wait

         This parameter specifies whether or not the PAD automatically
         enters a flow controlled state (X-OFFed) at the end of each page.
         Page length is defined by Telenet parameter 13, above.

             0  Page Wait disabled (Default)
             1  Page Wait enabled


  +16    Interrupt on Break

         This parameter specifies whether or not the PAD will transmit an
         INTERRUPT packet to the Host when a break signal is received from
         the terminal.  Values are:

             0  No INTERRUPT packet sent on break (Default)
             1  Send INTERRUPT packet on break


   17    Break Code

         The Break Code specifies an eight-bit representation for the break
         signal condition.  Codes may be any number from 1 through 255.
         Default is 0 (No break code).


  +18    Network Virtual Terminal (NVT) Option

         This parameter enables or disables NVT facilities by functional
         group (The Process Control function should no longer be used):

             0  NVT disabled (Default)
             2  Enables Process Control function *
             4  Enables Editing Function

             * use with caution


  *19    Initial Keyboard State

         This archaic parameter defined the initial state of the terminal
	 keyboard at the beginning of a virtual call.

             0  Keyboard initially locked (Default)
             1  Keyboard initially unlocked


   20    Half/Full Duplex

         This parameter specifies the echoing requirement of the terminal.
         Values are:

             0  Full duplex terminal
             1  Half duplex terminal


  *21    Real Character Code

         This parameter specified the communications code for representing
         data generated or recognized by the terminal.  Values are:

             0  ASCII
             1  Correspondence (standard Selectric)
             2  EBCD
             3  APL ASCII (typewriter-paired)
             4  APL ASCII (bit-paired)
             5  APL Correspondence
             6  APL EBCD


   22    Printer Style

         This identifies the class of printing mechanism used by the
         terminal:

             0  Typewriter style terminal
             1  Line printer style terminal


   23    Terminal Type

         This identifies the specific make and model of the terminal.
         Values are:

             0  Unknown or Synchronous Host
         1-126  Terminal codes
           127  Asynchronous Hosts


   24    Permanent Terminal

         This determines whether the network queries for a terminal
         identifier or employs a pre-set identifier.  Values are:

             0  Request identifier (Default)
             1  Use pre-set identifier


   25    Manual/Automatic Connection

         This parameter specifies whether a pre-defined virtual circuit is
         to be established automatically for the terminal, or it the call
         must be initiated by a C(onnect) or ID command entered from the
         terminal.  Values are:

             0  Manual (Connect or ID required) (Default)
             1  Automatic (Address pre-defined)


  +26    Rate

         This parameter specifies the transmission speed of the terminal,
         as determined by the network:

             0   110   bps
             1   134.5
             2   300
             3   1200
             4   600
             5   75
             6   150
             7   1800
             8   200
             9   100
            10   50
	    11   75/1200
	    12   2400
	    13   4800
	    14   9600
	    15   19,200
	    16   48,000
	    17   56,000
	    18   64,000


  +27    Delete Character

         This specifies the character to be used for single-character
         editing.

             0  Function disabled
         1-127  Identifies the character to be used

         Default is decimal 127.


  +28    Cancel Character

         Specifies the character to be used to delete input data buffered
         for the terminal at the PAD.

             0  Function disabled
         1-127  Identifies the character to be used

         Default is decimal 24.


  +29    Display Character

         Specifies the character to be used for displaying data which has
         been accumulated by the PAD.

             0  Function disabled
         1-127  Identifies the character to be used

         Default is decimal 18.


  *30    Abort Character

         This is an NVT Process Control parameter and should no longer be
	 used.  If NVT Process Control was enabled (Telenet 18:2), then
	 this parameter specified the character which, when received from
	 the terminal, caused the PAD to Flush Output (Telenet 33:1) and
	 generate an X.25 INTERRUPT containing F5 hex in the optional data
	 byte.  Note, data remained flushed until X.3 parm 8 or Telenet
	 parm 33 was reset to zero.

             0  Function disabled (Default)
         1-127  Identifies the character to be used


  *31    Interrupt Character

         This is an NVT Process Control parameter and should no longer be
	 used.  If NVT Process Control was enabled (Telenet 18:2), then
	 this parameter specified the character which, when received from
	 the terminal, caused the PAD to generate an X.25 INTERRUPT 
	 containing F4 hex in the optional data byte.

             0  Function disabled (Default)
         1-127  Identifies the character to be used


   32    Automatic Hang Up

         This specifies whether the terminal is to be physically
         disconnected from the network or left in Command Mode at the end
	 of a virtual call.  Values are:

             0  Leave in Command Mode upon disconnect (Default)
             1  Hang up upon disconnect


  +33    Flush Output

         This parameter controls the transmission of all data from the Host
         to the terminal:

             0  Transmit all information sent from (Default)
                the Host to the terminal

             1  Discard all information sent from
                the Host to the terminal


   34    Transmit on Timers

         This specifies that characters accumulated by the network are
         forwarded upon expiration of either the Idle or Interval Timer.
         Values are:

             0  Disable transmission on timers
             1  Enable transmission on timers (Default)


  +35    Idle Timer

         The Idle timer defines the time interval between characters
         arriving from the terminal which, when exceeded, causes the
         network to transmit any accumulated characters to the Host.
         Values are:

             0  Timer disabled
         2-255  Multiples of 50 ms (.05 seconds)

         Note: Default is 80 (4 seconds)


   36    Interval Timer

         The Interval Timer specifies the maximum time period during which
         the network PAD will accumulate characters before forwarding them
         to their destination.  Values are:

             0  Timer disabled (Default)
         2-255  multiples of 50 ms (.05 seconds)


   37    Network Usage Display

         This controls the transmission of information on chargeable network
         usage provided at the end of a virtual call.  Values are:

             0  Exclude network-generated usage information
                from the DISCONNECTED message (Default)

             1  Include network-generated usage information
                from the DISCONNECTED message


   38    Carriage Return Padding (Variable)

         This specifies the amount of time-delay padding to be provided
	 after each carriage return sent to the terminal, for every 10
	 printable characters on the line (E.g., no padding for nine
	 characters; five time the value of parameter 38 for 50 characters.)
	 Values may run from 0 through 7.


   39    Padding Options

         This parameter specifies whether or not the network provides time
         delay padding after form effectors sent to the terminal.  Values
         are:

             0  Network provides no time delay padding

             1  Network provides time delay padding (Default)
                after CR, LF, and HT characters


   40    Insert on Break

         This specifies whether or not the PAD inserts the Break Code in the
         data stream at the point at which the break signal is received from
         the terminal.  Values are:

             0  Do not insert on break (Default)
             1  Insert Break Code on break


  +41    PAD-to-Terminal Flow Control

         This parameter specifies network XON/XOFF control of transmission
         from the terminal.  Values are:

             0  No PAD-to-Terminal Flow Control (Default)
             1  Network provides flow control


   42    PAD-to-Terminal XON Character

         This identifies the character which, when sent from the network to
         the terminal, causes the terminal to resume transmission of
         buffered data.  Value may be any character from 1 to 127.  Default
         is 17 (19 octal, 11 hex).


   43    PAD-to-Terminal XOFF Character

         This identifies the character which, when sent from the network to
         the terminal, causes the terminal to temporarily suspend
         transmission of buffered data.  Value may be any character from 1
         to 127.  Default is 19 (21 octal, 13 hex).


  *44    Generate Break

         This parameter used to cause a break signal to be transmitted
         from the PAD to the terminal.  It is no longer valid to set this
         parameter.


  *45    APP on Break

         This parameter specified whether or not the PAD transmitted a
	 SET & READ PARAMETERS PAD Message to the Host system when a break
	 signal was received from the terminal.  This parameter should no
	 longer be used.

             0  No SET & READ PARAMETERS PAD Message (Default)
                generated on break

             1  SET & READ PARAMETERS PAD Message generated
                on break


  *46    Input Unlock Option

         This archaic parameter specifies what action the PAD took after the
         terminal user had entered a line of data, the keyboard had been
         locked, and the PAD had no data to deliver to the terminal. Values
         are:

             0  Unlock based on timer expiration (Default)
             1  Unlock based on input data content


  *47    Input Unlock Timer

         This archaic parameter specified the time interval that the PAD
	 would wait before unlocking the terminal keyboard, if the PAD had
	 no data pending delivery to the terminal and parameter 46 was set
	 to 0.  Values ranged from 0 through 255 multiples of 50 ms (.05
	 seconds).  Default was 0 seconds.


  *48    Input Unlock Character

         This archaic parameter specified the character which, when appearing
	 at the beginning of a data line, caused the PAD to leave the keyboard
         locked at the end of the data line (if there is no data pending
         delivery to the terminal).  Value was any character code from 0
         through 127; or 240, which leaves the keyboard locked after all
         characters. Default was 0.


  *49    Output Lock Option

         This archaic parameter specified the action the PAD took when it
	 received data for delivery to the terminal, when the keyboard was
	 unlocked for input from the terminal.  Values are:

             0  Discard output data
             1  Transmit output after input completion
             2  Transmit output id input idle (Default)


  *50    Output Lock Timer

         This archaic parameter defined the interval between characters
	 arriving from the terminal which, when exceeded, caused the PAD
	 to lock the keyboard when it had output pending delivery to the
	 terminal.  Values may range from 0 through 255 multiples of 50 ms
	 (.05 seconds).  Default was 10 (500ms).


  *51    Output Lock Option

         This archaic parameter specified what action the PAD took after it
	 had transmitted all pending data to the terminal.  Values are:

             0  Unlock based on timer (Default)
             1  Unlock based on output completion
             2  Unlock based on output data content


  +53    Break Options

         This allows for a combination of options for handling break signals
         from the terminal.  Values may be OR-ed together:

             0  No options selected (Default)
             1  Interrupt on break
             4  APP on break
            32  Insert on break

         Note, X.3 parameter 7 should be used instead of this parameter


   54    Terminal-to-PAD Flow Control

         This parameter specifies XON/XOFF control of transmission from the
         network.  Values are:

             0  No Terminal-to-PAD flow control (Default)
             1  Network respects flow control


   55    Terminal-to-PAD XON Character

         This identifies the character which, when sent to the network,
         causes the network to resume the transmission of buffered data.
         Value may be any character code from 1 through 127.  Default is 17
         decimal.


   56    Terminal-to-PAD XOFF Character

         This identifies the character which, when sent to the network,
         causes the network to temporarily suspend the transmission of
         buffered data.  Value may be any character code from 1 through 127.
         Default is 19.


   57    Connection Mode

         This parameter specifies which level of terminal code conversion
         the PAD is to perform during data transfer mode.  Values are:

             0  Transparent
             1  Real
             2  Virtual  (Default)


  +58    Connection Escape

         This parameter specifies whether or not the terminal may escape
         from Data Transfer mode to Network Command mode.  Values are:

             0  Escape not possible
             1  Escape possible (Default)


  *59    Flush Output on Break

         This parameter specified whether or not the PAD transmitted a SET &
         READ PARAMETER PAD Message to the Host and began discarding output
         to the terminal when a break signal was received from the terminal.
	 Rather than using this parameter set X.3 parameter 7 to 21
	 (decimal).

             0  No SET & READ PARAMETERS PAD Message (Default)
                sent and no output flushed

             1  SET & READ PARAMETERS PAD Message sent and output
                to the terminal


   60    Delayed Echo

         This parameter identified whether echo from the PAD to the terminal
	 will occur immediately or whether it will be delayed to appear
	 between data from incoming packets.  If 60:1, then once the PAD has
	 begun processing an incoming packet, it will buffer echo characters
	 until it completes the packet.  At that point, it will transmit all
	 buffered echo characters back to the terminal before processing the
	 next incoming packet.  Values are:

             0  Echo immediately   (Default)
             1  Delay echo to occur between incoming packets


   63    Eight-bit Transparency

         This parameter identifies whether the terminal uses the eighth
	 (most significant) bit for data or as a parity bit.  Note, if
	 Telenet parameter 57:2, this parameter cannot be set to zero. 
	 Values are:

             0  No parity, eight-bit transparency
             1  Parity required (Default)


   64    Early ACK

         This parameter specifies whether or not the PAD for terminal
         support should acknowledge data packets received for the terminal
         prior to transmitting the packets (in the form of a character
         stream) to the terminal.  Values are:

             0  Acknowledge data packets after transmission
                to the terminal (Default)

           1-7  Acknowledge data packets 1-7 packets prior to
                transmission to the terminal

         Note:  *Extreme Caution* should be exercised when modifying this
                parameter.  The increased "artificial window" size does not
                guarantee packet delivery to the terminal.  Large amounts of
                data could be lost from any form of network disconnect.
                Values of 5 or greater should never be used.


   65    M-bit handling

         This parameter specifies whether the terminal PAD will set the M-bit
	 on all full packets, on certain full packets, or on packets.  Values
	 are:

             0  M-bit is always zero
             1  M-bit is set to one for certain full packets
             3  M-bit is set to one in all full packets  (Default)

         If parameter 65:1, the PAD will set the M-bit on all full packets
	 except where the last user-entered character is a data-forwarding
	 character, as defined by X.3 parameter 3 (Transmit Mask).  If,
	 however, the final character in the packet is a carriage return and
	 X.3 parameter 13 causes a line feed insertion following the carriage
	 return and X.3 parameter 3 marks carriage return as a data-forwarding
	 character, then the M-bit will be set to 1.  The PAD will then 
	 transmit a second packet, with M-bit set to 0, containing only a
	 line feed character.

	 If, after sending a packet with M-bit set to one, the PAD must send
	 a data-qualified packet (Q-bit=1), this is considered a data-
	 forwarding condition.  Thus, the PAD will send a data packet with
	 M-bit = 0 containing the characters currently in its buffer.  If
	 the buffer is empty the PAD will send an empty packet with M-bit = 0.
	 This prevents a protocol violation.


   66    Defer Processing of User Input

	 This parameter instructs the PAD to halt processing of user input
	 data and buffer the data (to a maximum of 32-64 characters).  Upon
	 disconnect, parameter 66 is rest and processing of user data resumes.
	 If the disconnect triggers a reselection (e.g., forwarding of the
	 call by TAMS), the buffered data is sent to the new called DTE
	 Otherwise, or if reselection fails, the data is interpreted by the
	 PAD as a command during command mode.  Values are

             0  Process user input normally (Default)
	     1  Defer processing of user input data

   67    ESP Packetizing Option

	 This parameter specifies whether accumulated data is to be packet-
	 izied when the Escape Sequence Initiator is received (i.e., before
	 the Escape Sequence) and when the Escape Sequence is completed. 
	 Values are:

                   Packetize   Packetize
		    Before       After

	     0        No          No    (Default)
	     1        No          Yes
	     2        Yes         No
	     3        Yes         Yes


   68    Escape Sequence Timer

	 This parameter specifies the maximum idle time allowed before ESP
	 processing expires.  Values range from zero through 255 and
	 represent 50 ms intervals.  Resolution of the timer is zero to 
	 minus 50 ms (e.g., a value of 2 represents 50ms < timer < 100ms).
	 Default is zero.


   69    Escape Sequence Maximum Length
	
	 This parameter specifies the maximum number of characters that may
	 be contained in an Escape Sequence, including the Escape Sequence
	 Initiator.  A value of zero disables parameter 69 and the maximum
	 Escape Sequence is 128 characters.  Default is zero and values
	 greater than 127 are not allowed.

	
   70    Escape Sequence Initiator

	 This parameter specifies the seven-bit representation of the Escape
	 Sequence Initiator character (values 1-127).  The default value of
	 zero disables Escape Sequence Processing altogether.


   71    Parameter Reset on Disconnect

	 This parameter specifies the manner in which parameters are to be 
	 treated upon disconnect.  Values are:

             0  Reset ITIs to their initial values  (Default)
	     1  Do not reset ITIs, except for reselect-related
		parameters (66 and 71)
	     2  Do not reset ITIs, except set 66:0 and 71:1
	     3  Do not reset ITIs, except set 66:0

	 Value 1 makes parameter 71 a "one-shot" parameter, this is it 
	 clears itself after being invoked once.  Value 2 is a "two-shot"
	 value and value 3 leaves parameter 71 active until explicitly
	 reset.


<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                
                                                                                                                                                                                                                                                                                                                                                                                                                               

                        HUNT/CONFIRM SEQUENCE



========================================================================

  BITS/STOP/PARITY    MODEM TERMINAL     DUPLEX        HUNT/CONFIRM
                          SPEED                      SPRINTNET PROCEDURE

========================================================================


  7    1    EVEN        300-1200         FULL            <CR><CR>
  7    1    EVEN        300-1200         HALF            <CR>;<CR>
  7    1    EVEN          2400           FULL              @<CR>
  7    1    EVEN          2400           HALF              @;<CR>


  8    1    NONE        300-1200         FULL            <CR>D<CR>
  8    1    NONE        300-1200         HALF            <CR>H<CR>
  8    1    NONE          2400           FULL              @D<CR>
  8    1    NONE          2400           HALF              @H<CR


  NOTE:  If you are using an automated procedure to connect to a SprintNet 
	 modem at 2400 BPS, please use a half-second pause BEFORE and
	 AFTER the @ sign.

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>


                            Terminal Identifiers


   The following tables matches Terminal numerical IDs (telenet parmater 23)
   Generic and Specific Terminal Identifiers.

        ID #    Generic    Term ID    Terminal Type (note)
        ----    -------    -------    ---------------------------

          0                           Unknown or Synch. Host
          1        B1       AJ63      Anderson Jacobson 630
          2        B5       AJ86      Anderson Jacobson 860 (9)
          3        A2       CD30      CDI 1030
          4        D1       DP22      Datapoint 2200
          5        D2       DP30      Datapoint 3000 & 3300
          6        D3       HP21      Hewlett-Packard 2100s (9)
          7        A2       CT30      CT Execuport 300
          9        A4       GE30      GE Terminet 300
         10        A3       GE12      GE Terminet 1200
         11        D1       HZ20      Hazeltine 2000
         12        E1       IBM1      2741 EBCD (5)
         13        E2       IBM2      2741 EBCD (6)
         14        E3       IBM3      2741 EBCD (7)
         15        E4       IBM4      2741 EBCD (8)
         16        C1       IBM5      2741 Correspondence (1)
         17        C2       IBM6      2741 Correspondence (2)
         18        C3       IBM7      2741 Correspondence (3)
         19        C4       IBM8      2741 Correspondence (4)
         20        D1       T4/2      Special Terminal
         26        A1       TT33      Teletype 33
         27        A1       TT35      Teletype 35
         30        D1       TT40      Teletype 40
         32        A7       TI25      TI 725
         33        A2       TI33      TI 733  (Default)
         34        A6       TI45      TI 735
         35        B2       UV50      Univac DCT 500
         38        D1       IFVD      Infoton Vistar Display
         39        D1       RI34      Teleray 3300-3700
         40        A5       TN30      GE Terminet 30
         41        A8       DECW      DEC LA35/36 Decwriter II
         43        A3       TN12      GE Terminet 120
         44        A9       CT12      CT Execuport 1200
         45        A1                 Generic Terminal
         46        A2                 Generic Terminal
         47        A3                 Generic Terminal
         48        A4                 Generic Terminal
         49        A5                 Generic Terminal
         50        A6                 Generic Terminal
         51        A7                 Generic Terminal
         52        A8                 Generic Terminal
         53        A9                 Generic Terminal
         54        D1       ADDS      ADDS 520, 580, 980
         55        B3       AJ83      AJ 830 & 832
         56        B1                 Generic Terminal
         57        B2                 Generic Terminal
         59        D1       BHMB      Beehive MiniBee 2
         60        C1                 Generic Terminal
         61        C2                 Generic Terminal
         62        C3                 Generic Terminal
         63        C4                 Generic Terminal
         64        D1       CD11      CDI 1132
         65        A2       CD12      CDI 1202 & 1203
         66        D1                 Generic Terminal
         67        D2                 Generic Terminal
         68        D1       DECV      DEC VT50 & VT52
         69        D1       DGLG      Digi-Log 33, Telecomputer I
         70        A1       DPPT      Data Products Portaterm
         71        B3       DS16      Diablo 1550 & 1620
         72        E1                 Generic Terminal
         73        E2                 Generic Terminal
         74        E3                 Generic Terminal
         75        E4                 Generic Terminal
         76        B3       GS30      Gen-Comm Systems 300
         77        D1       HP26      HP 2640, 2644, 2645
         78        D1       LSAM      Lear Siegler ADM1, 2, 3
         79        A2       NC60      NCR 260
         80        B1       TD40      Trendata 4000
         81        D1       TI45      TI 745
         82        D2       TI65      TI 763, 765 (10)
         83        D1       TK40      Tektronix 4002-4023
         84        B3       TT43      Teletype 43
         85        A3       WU30      Western Union EDT 30
         86        A4       WU12      Western Union EDT 1200
         87        B3       DT30      Data Term & Comm DCT 300-30 2
         88        B3                 Generic Terminal
         89        B4                 Generic Terminal
         90        B5                 Generic Terminal (9)
         91        D3                 Generic Terminal (9)
        127                           Asynchronous Hosts




     The following are terminal models with corresponding generic terminal
     types supported by the terminal handler.

         Terminal Model                              ID (note)
         -------------------------------------       ---------

         ADDS Consul 520, 580, 980                    D1 (1)
         ADDS Envoy 620, Regent                       D1 (1)
         Alanthus Data Terminal T-133                 A1
                                T-300                 A8
                                T-1200                A3
         Alanthus Miniterm                            A2
         AM-Jacquard Amtext 425                       D1 (1)
         Anderson Jacobsen 510                        D1 (1)
         Anderson Jacobsen 630                        B1
         Anderson Jacobsen 830 & 832                  B3 (2)
         Anderson Jacobsen 860                        B5
         Apple II                                     D1 (1)
         Atari 400, 800                               D1 (1)
         AT&T Dataspeed 40/1, 40/2, 40/3              D1 (1)
         Beehive MiniBee, MicroBee                    D1 (1)
         Centronics 761                               A8
         Commodore Pet                                D1 (1)
         Compu-Color II                               D1 (1)
         Computer Devices CDI 1030                    A2
         Computer Devices Teleterm 1132               A8
         Computer Devices Miniterm 1200 series        A2
         Computer Transceiver Execuport 300           A2
         Computer Transceiver Execuport 1200          A2
         Computer Transceiver Execuport 4000          A2
         CPT 6000, 8000                               D1 (1)
         Datamedia Elite                              D1 (1)
         Datapoint 1500, 1800, 2200, 3000, 3300,
                   3600, 3800                         D1 (1)
         Data Products Portaterm                      A1
         Data Terminal & Comm DTC 300, 302            B3 (2)
         Diablo Hyterm                                B3 (2)
         Digi-log 33 & Telecomputer II                D1 (1)
         DEC (LA 35-36) Decwriter II                  A8
         DEC (LA 120) Decwriter III                   A8
         DEC VT50, VT52, VT100, WS78, WS200           D1 (1)
         Gen-Comm Systems 300                         B3 (2)
         GE Terminet 30                               A5
         GE Terminet 120, 1200                        A3
         GE Terminet 300                              A4
         General Terminal GT-100A, GT-101, GT-110,
                          GT-400, GT-400B             D1 (1)
         Hazeltine 1500, 1400, 2000                   D1 (1)
         Hewlett Packard 2621                         D3
         Hewlett Packard 2640 series                  D1 (1)
         IBM PC (and compatibles)                     D1 (1)
         IBM 3101                                     D1 (1)
         Informer I304, D304                          D1 (1)
         Infoton 100, 200, 400, Vistar                D1 (1)
         Intelligent Systems Intecolor                D1 (1)
         Intertex Intertube II                        D1 (1)
         Lanier Word Processor                        D1 (1)
         Lear Siegler ADM series                      D1 (1)
         Lexitron 1202, 1303                          D1 (1)
         Memorex 1240                                 A2
         Micom 2000, 2001                             D1 (1)
         NBI 3000                                     D1 (1)
         NCR 260                                      A2
         Perkin-Elmer Model 110, Owl, Bantam          D1 (1)
         Perkin-Elmer Carousel 300 Series             A8
         Radio Shack TRS 80                           D1 (1)
         Research Inc. Teleray                        D1 (1)
         Tektronix 4002-4023                          D1 (1)
         Teletype Model 33, 35                        A1
         Teletype Model 40                            D1 (1)
         Teletype Model 43                            B3 (2)
         Teletype Model 40/1, 40/2, 40/3              D1 (1)
         Texas Instrument 725                         A7
                          733                         A2
                          735                         A6
                          743, 745, 763, 765          D1 (1)
                          820                         B3 (2)
                          99/4                        D1 (1)
         Trendata 4000 (ASCII)                        B1
         Tymshare 110, 212                            A2
                  315                                 A8
                  325                                 B3 (2)
         Univac DCT 500                               B4
         WANG 20, 25, 30, 105, 130, 145               D1 (1)
         Western Union EDT 30, 35                     A1
                           300                        A4
                           1200                       A4
         XEROX 800, 850, 860                          D1 (1)
         XEROX 1700                                   B3 (2)

     Notes:   (1)  Use D3 if you wish Telenet to respond to XON/XOFF
                   flow control.
              (2)  Use B5 if you wish Telenet to respond to XON/XOFF
                   flow control.





     The following are the major characteristics of the generic terminal
     types supported by the terminal handler:

     Generic  Tab   LF    CR Pad   CR Pad   Line   Code
              Pad   Pad   Fixed    Var'bl   Size   Type (note)
     -------  ---   ---   ------   ------   ----   -----------------------

       A1      0     1       0        0      72    ASCII
       A2      0     2       7        0      80    ASCII
       A3      0     0       0        0     120    ASCII - Printer
       A4      0     6       0        0     120    ASCII
       A5      0     5       5        0     120    ASCII
       A6      0     0       1        1      80    ASCII
       A7      0     4       0        2      80    ASCII
       A8      2     0       1        0     132    ASCII
       A9     12    10      16        6     132    ASCII

       B1      1     0       2        1     132    ASCII--BUFFERED
       B2      0     2       6        0     132    ASCII--BUFFERED
       B3      0     0       0        0     132    ASCII--BUFFERED
       B4      0     2      10        0     132    ASCII--BUFFERED
       B5      0     0       0        0     132    ASCII--BUFFERED (9)

       C1      1     1       4        1     130    2741 Correspondence (1)
       C2      1     1       4        1     130    2741 Correspondence (2)
       C3      1     1       4        1     130    2741 Correspondence (3)
       C4      1     1       4        1     130    2741 Correspondence (4)

       D1      0     0       0        0      80    ASCII--CRT
       D2      0     0       0        0      72    ASCII--CRT
       D3      0     0       0        0      80    ASCII--CRT (9)

       E1      1     1       4        1     130    2741 EBCD (5)
       E2      1     1       4        1     130    2741 EBCD (6)
       E3      1     1       4        1     130    2741 EBCD (7)
       E4      1     1       4        1     130    2741 EBCD (8)


       Notes:

       (1)  Corresponds with Ball Types:  001, 005, 007, 008, 012, 020, 030,
            050, 053, 067, 070, and 085.  Ball Type code can be found
            underneath the locking tab of the ball on an IBM 2741 terminal.

       (2)  Corresponds with Ball Types:  006, 010, 015, 019, 059, and 090.

       (3)  Corresponds with Ball Types:  021, 025, 026, 027, 028, 029, 031,
            032, 033, 034, 035, 036, 037, 038, 029, 060, 068, 086, 123, 129,
            130, 131, 132, 133, 134, 135, 146, 137, 138, 139, 140, 141, 142,
            143, 144, 145, 156, and 161.

       (4)  Corresponds with Ball Types:  043 and 054.

       (5)  Corresponds with Ball Types:  963, 996, and 998.

       (6)  Corresponds with Ball Types:  938, 939, 961, 962, and 997.

       (7)  Corresponds with Ball Types:  942 and 943.

       (8)  Corresponds with Ball Types:  947 and 948.

       (9)  Terminal Types D3 and B5 enable Terminal-to-PAD flow control in
            the Terminal PAD (TFLOW).

      (10)  The specific Terminal ID, TI65, incorrect maps to the generic
            ID, D2.  Since TI 763 and 765 print 80 character per line, users
            with these terminals should specify a generic TERM ID of either
            D3 (TFLOW enabled) or D1 (TFLOW not specified).

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

<< This is what the troubleshooters of PCPursuit are given to answer queries>>
<< from the legitamit users of its system.  very interestinghow they work   >>

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

1/18/87                TROUBLESHOOTING PC PURSUIT CALLS
               (Tips for helping Cust. Svc. help Pursuit callers)

   This is a list of typical questions about PC Pursuit and some answers that
should help.  I will not swear that everything--or anything--is accurate.
However, most of the explanations will, at least, help most PC Pursuit
customers.


GENERAL RULES
"""""""""""""
   First, listen to what the customer is saying.  Some of these guys have more
experience with data communications than anyone in this building, let alone in
this department.  They will obviously not be impressed if you run on autopilot
through the typical "are you at 8 bits and no parity" sort of question.  Calls
tend to be one of two types: general, simple informational questions and
specific technical problems.  If you treat one of the latter as if it were one
of the former, you will do little to convice the customer that you are steering
him correctly.
   Second, don't be too eager to dump the customer onto someone else or off the
line.  This will make life easier for whoever has to eventually solve the
problem.


SPECIFIC PROBLEMS
"""""""""""""""""
"I can't connect to a port; I keep getting D/DCWAS/12 [or whatever] BUSY."
----------------------------------------------------------------------------

   Explain that these are legitimate busies and that port expansion, both in
adding new cities and in expanding existing rotaries, is underway.
We *will* be adding several hundred new lines to the system.  Many cities
have already been upgraded, and more are being completed all the time.


"I connect to a port but I get hung.  Not even ATZ will appear."
------------------------------------------------------------------

   If they're currently in the frozen port (some users know enough to hold it
open and call us on another line), run a port scan to see where they're
connected.  Reset the port to knock them out, C-space to it, and if you can't
clear the trouble, busy it out and send a ticket to the field.  (This should be
old hat by now, with the troubles we've recently found in the new DC modems.)

   If they are not connected, your only approach is to try to connect directly
to each port and see if any refuses to respond.  If you can't find a malfunc-
tioning modem, make sure the user was entering "ATZ" in capital letters.


"I connect to a port and enter ATZ but everything seems to hang."
--------------------------------------------------------------------
   Check to see if they are using a Hayes compatible modem.  The PCP modems use
a limited subset of the Hayes "AT" commands.  In theory, a working Hayes or
compatible modem will ignore these commands while in a data transfer state.  To
place such a modem in command mode, the user must rapidly enter three plus
signs (+) in a row and then wait until the modem acknowledges the command
before entering any more data.

   However, malfunctioning modems or some of the not-quite-compatible (usually
cheaper) modems will act on "AT" commands from within data transfer.  When the
user enters the ATZ command to wake up the PCP modem, it instead resets the
user's modem, usually dropping the connection.  This would also happen if the
string "ATZ" was encountered during a file transfer.

   There's not a lot we can do to diagnose this, and PCP users
take none too kindly to the suggestion that their bargain modems are no
bargain.  As a test, have the user connect to a port and enter one of the Hayes
commands not supported by the PCP modems--for instance, ATH0, which hangs up
the modem, or ATH1, which "lifts" it off the hook.  If they are actually
talking to the PCP modem, it will respond with an "OK" and do nothing else; if
they are talking to their own modem, it will drop carrier.

   To use PCP successfully, they will either (1) have to replace or repair
their modem, (2) find a way to disable its break to command mode, or (3) try
to throw the PCP port into Racal-Vadic mode (with a Ctrl-E).  Note that the
latter solution does not always work unless the modem has been reset with an
ATZ command--which, of course, is out of the question--and may not always be an
option, depending on hardware manufacturer and version.

   I have yet to find an instance of this that was not trouble on the
customer's end, but I expect we will.



"I try to call this number from a PCP modem and I get a busy.  I dial it
immediately after hanging up [or from another line] and I get through.   I try
it again on PCP and get a busy."
--------------------------------------------------------------------------------

   First, make sure that the number they are dialing is within the accepted
exchanges for a given city (see the list in the PCP guide).  Note that there
are a few exchanges that can be reached that are not on the list; a slightly
more up-to-date list is available on the Net Exchange BBS.

   If the number should be valid, see if you can isolate the port the user is
calling from.  Connect to that port, issue "ATZ", and send the modem a Ctrl-E
and carriage return.  This will throw the modem into Racal-Vadic mode, which
provides better diagnostics than Hayes mode.  Try to dial the number and see
what transpires.  Racal-Vadic mode will report on the absence of a dial tone,
each ring as it occurs, and the ultimate outcome of the call.  Take appropriate
action.  (Also, the new modems--the new ones in DC, not the ones that will be
used for the expansion--give a "NO DIAL TONE" message from within Hayes
emulation mode.)

   If the user is certain that the exchange is local to the PCP city, ask him
to leave a message to the SysOp (i.e., Dave) on the Net Exchange board.
If you get a connection or what appears to be a legitimate busy, inform the
customer and chalk it up to chance and a busy BBS.



"Sometimes when I connect to a port, I get a message that says 'MANUAL ANSWER'
and I can't do anything but disconnect."
-------------------------------------------------------------------------------

   Since the Racal-Vadic mode provides better diagnostics (see above), many
users shift into it before dialing their BBS.  If they terminate abnormally
(that is, if the session, not the user, terminates abnormally), the modem may
be left in Racal-Vadic mode.

   For instance, User A uses Racal-Vadic mode to call a board.  He then gets
bumped off the line (or perhaps hangs up before returning the modem to Hayes
emulation) and User B connects to the port before the modem has a chance to
reset (assuming it resets at all).  The modem has sent the Racal-Vadic prompt--
an asterisk--to User A and is waiting for a command.  User B sees no response--
the prompt has already been sent--so he assumes the modem is in Hayes mode.  He
enters "ATZ" and waits for the "OK".  (To make matters worse, perhaps he is
using a command script that needs to "see" an "OK" before proceeding.)

   The modem, currently ignorant of Hayes commands, interprets the "A" of the
"ATZ" as being the Racal-Vadic command to answer a call manually; that is, to
take the line off-hook and respond to the call.  It does so, having first sent
the user the message "MANUAL ANSWER."  Since people rarely dial *into* a PC
Pursuit line, nothing happens and the modem just sits.

   To get the user out of this trap, have him enter carriage returns until the
modem drops the line and prompts him with another "*".  At this prompt, have
the user enter "I".  This is a nonintuitive command--the "I" stands for "IDLE"
--but it has the happy result of returning the modem to Hayes mode.

There is a file called rvprimer.txt on the Net Exchange which describes the
Racal-Vadic mode.



"I use XMODEM across the system and transfers take twice [or thrice] as long as
they should.  Why?"
--------------------------------------------------------------------------------

   As best as I can tell, the information we were passed from the Net Exchange
BBS was well-meaning but wrong.  Here is the scenario as I figger it--someone
let me know if I'm wrong, too.

   XMODEM sends data in a 132-byte block that resembles a mini-packet:

   <-------------------------  Direction of transmission

   [SOH] [#] [#] [DATA] [CHK]
     |    |   |    |      |___ "Checksum" (kinda) for error-detection
     |    |   |    |__________ 128 bytes of data
     |    |   |_______________ "One's complement" of block number
     |    |___________________ Block number
     |________________________ Start of header (ASCII 01)


This closely matches the size of a Telenet packet (generally 128 bytes) and
can, for our purposes, be considered a packet's worth of data.  PC Pursuit is
set to forward data only on full packets and on expiration of idle timers
(which are set for 1/10 second).

  The delay occurs because a connection through PC Pursuit goes through four
modems and two entirely separate data transmissions.  Each block of data must
undergo the following (assuming a download from the BBS to the user):
 _____           _________           __________
|     |____     (         )____     |          |
| BBS |    /____(   PDN   )    /____| PCP user |
|_____|         (_________)         |__________|

       |_______| |_______| |_______|
           |         |         |_____  1.1 seconds
           |         |_______________  Variable (0.1 to 1+ seconds)
           |_________________________  1.1 seconds


That's potentially 3+ seconds to transfer data that would take slightly over
1 second to transmit in a direct connection--maybe 35% efficiency.

   To make matters worse, the acknowledgment (ACK) from the user to the BBS may
take upwards of a second--instead of a fraction of a second--to be transmitted
back into the network, have idle timers expire, be forwarded to the outdialer,
and be transmitted to the BBS.  As you can see, though, the real delay is *not*
because of the delay in sending the ACK, but because the block size and packet
size so nearly match, the two computers are almost never working
simultaneously.

   A protocol that uses a larger block size--YMODEM, for instance--will run
faster over the system, but not because it needs fewer acknowledgements.
Instead, while sending the larger block, it causes data forwarding on a full-
packet condition.  After the first packet gets sent, both machines are doing
work for most of the rest of the transmission, as such:

                      BBS                           USER
                      """                           """"
Start of 1K block     Sends packet 1                Does nothing
                      Sends packet 2                Receives packet 1
                      Sends packet 3                Receives packet 2
                      Sends packet 4                Receives packet 3
                      Sends packet 5                Receives packet 4
                      Sends packet 6                Receives packet 5
                      Sends packet 7                Receives packet 6
End of 1K block       Sends packet 8                Receives packet 7
                      Does nothing                  Receives packet 8


(Of course, the BBS is not really sending the *packet*, just a packet's worth
of data.)  In effect, YMODEM wastes only 2 of every 9 128-byte transfers; it
should run at about 75% efficiency.  In addition, since it only has a single
ACK per kilobyte (instead of 8), less time is spent in waiting for the idle
timer to expire.

   Of course, to make things more confusing, there are XMODEM packages using
256-byte and 1K blocks and XMODEM packages that allow a "window" of
unacknowledged blocks to be sent, among other flavors.  If the user is using
one of the strange XMODEMs, he'll usually know enough to mention it.

   Recently, the default parameters for the PC Pursuit ports were changed; by
whom, I don't know.  For best results, users should break to command mode and
set X.3 parameters 1 and 10 to 0 (disables break to command mode and word wrap)
and set ITI parameter 57 to 1 and parameter 63 to 0 (enable 8-bit transparent
mode).  This is all done with similar commands as those issued when connecting
to Exec PC.



"I can't use PUNTER protocol across the network."
-------------------------------------------------

   I have sent word (through a friend) for Steve Punter to call me to discuss
what might be going wrong with his procotol for Commodore machines.  However,
as best as I can tell, PUNTER protocol has a severely restrictive time-out
setting--the amount of time it will wait for an acknowledgement back from the
receiving site before assuming a block was lost and retransmitting it.  As the
diagram above shows, PC Pursuit introduces a lot of delay into the loop, and
this is too much for the BBS to take.  It starts to send the "lost" block
again; the receiving station finally receives and acknowledges the block; and
everything falls apart.  (This is complete assumption, by the way; I haven't
been able to find any hard info on PUNTER, although I am told it works in 256-
byte blocks.)  If this is true, I doubt PUNTER would even work over a satellite
long-distance connection, so PUNTER BBSs will probably soon offer a "relaxed"
PUNTER.  Often, Commodore users having no luck with PUNTER have been able to
run successful XMODEM transfers.



"I have no [or little] trouble downloading from a BBS, but my uploads often
fail."
-----------------------------------------------------------------------------

   This also seems to be related to time-out periods, but I'm not sure.
Because a 132-byte block will be sent in 2 packets and, thus, activity on
sending and receiving ends may overlap slightly, it is conceivable that the
delay between sending the last byte of a data block and receiving the ACK would
be a tiny bit less than the delay between sending the ACK and receiving the
first byte of the next block.  (Note: Here I am grasping for straws.)  If the
BBS has a particularly unforgiving time-out setting, it might reject the block
or get out of sync (see the PUNTER hypothesis, above).  Several Texas
Instrument computer users have been able to trick PC Pursuit into handling
transfers by calling into the networkj at 300 baud but calling out at 1200; I
haven't the foggiest idea why this works, unless the time-out period is
relatively more relaxed at the faster speed.



"I can't get the listing of BBSs on the Net Exchange BBS to download" or "I've
downloaded the listing of BBSs but can't read it; it's garbage."
-------------------------------------------------------------------------------

   Files with the extension .SQ have been squeezed; there are a number of
slightly different programs and variations for doing this, some compatible with
others.  Many machines have access to some sort of squeezing utility; whether
or not the file downloaded is in the proper format is another question.

   Files with the extension .LBR have been libraried; this procedure combines a
number of files into a single file, usually without data compression.  The
resulting file is easier to download and catalog than the individual files
would be, and takes up slightly less room.  LU is the main program for
librarying files in the IBM-compatible environment; I know of no comparable
programs for other machines.

   Files with the extension .ARC have been archived; this is a technique that
both squeezes and libraries files.  Files are usually archived with ARC, a
user-supported program distributed by System Enhancement Associates.  As far as
I know, there is only an official ARC for IBM-style computers; I think, but am
not sure, that there is a compatible program for CP/M-based machines (like the
Kaypro) and machines running Un*x.  I know of no other computers that can make
use of .ARC files.



"What do NO CARRIER and NO ERROR CONTROL mean?  I saw them in a recent
connection to Wash D.C. (D/DCWAS)."
------------------------------------------------------------------------

The modems in Wash D.C. are the new Vadic modems, which will also
support 2400 outdial when deployed.  These new modems have expanded response
messages.  NO CARRIER is seen in the Hayes mode when carrier has been
dropped between the Telenet outdial modem and the target BBS which the
user dialed.  The user still has control of the modem and can dial a
new number in the city if desired.

   NO ERROR CONTROL - is displayed whenever one of the new modems is
connected on-line with the target BBS.  It simply means that the outdial
modem is not in the MNP reliable modem (with local loop error protection).
You see, MNP is built into these new modems, and that means that when these
new modems call another modem with MNP in it, they will hand-shake and
come up in the Microcom reliable mode - which provides error protection in
the local phone loop.  If it is not using MNP and says NO ERROR CONTROL,
the call will still go through just fine to the remote BBS.



"How do I get the Racal-Vadic command mode?"
----------------------------------------------

The Hayes command mode is the only officially supported command mode for
PC Pursuit at this time - to simplify support and ease of use for users.
However, users may use the R-V mode, which does give some better
response messages (such as "Dialing", and also has re-dial).  To get
to the R-V mode, type ATZ to get the OK, then  ctrl-E  and you should
wake up the modem into the R-V mode as it responds "Hello, I'm ready"
with a  * .   Type ? (cr) for a list of the commands available.
When done with your session, the modem will reset itself into the
Hayes mode as you enter  I (cr) to Idle the modem.  (or depending on
how you disconnect, it will automatically reset to Hayes mode for the
next user within 10 - 100 seconds).


<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>

<><><><><><><><><><><><><><><><><><><><><><><><><><><><><><>
                                                                                                                                                                                                                                                                                                                                                                                                                      
                                                                           

----------------------------------------------------------------------

Outdial Site: D/NJNEW
300  bps: 311020100001
1200 bps: 311020100301
2400 bps: 311020100022

201        200 207 216 217 224 226 227 228 232 233 235 239 241 242 245 
201        256 259 266 268 272 273 276 277 278 279 284 288 289 298 301 
201        304 305 309 312 313 314 315 317 318 319 322 325 330 332 333 
201        338 339 340 342 343 344 345 346 348 351 352 353 354 355 365 
201        368 371 372 373 374 375 376 377 378 379 381 382 386 388 392 
201        393 394 396 399 401 403 408 413 414 416 419 420 421 423 427 
201        428 429 430 432 433 434 435 436 437 438 440 441 450 451 456 
201        460 461 464 465 467 468 470 471 472 473 474 478 480 481 482 
201        483 484 485 486 487 488 489 499 503 504 507 509 514 515 516 
201        522 523 527 533 535 541 546 547 558 564 565 567 568 569 570 
201        574 575 578 581 582 585 587 589 592 593 594 595 596 601 602 
201        608 614 617 621 622 623 624 626 628 633 634 635 636 641 642 
201        643 645 646 648 649 653 654 656 659 661 662 665 667 669 672 
201        673 674 675 676 677 678 680 684 686 687 688 690 692 694 695 
201        696 701 703 705 708 709 712 714 716 731 733 736 737 740 742 
201        743 744 746 748 750 751 759 760 761 762 763 765 771 772 773 
201        777 778 779 783 785 789 790 791 792 794 795 796 797 798 801 
201        802 803 804 807 808 812 814 815 816 817 820 822 823 824 833 
201        836 837 843 845 851 854 855 857 858 860 861 862 863 864 865 
201        866 867 868 869 871 877 881 882 884 886 887 889 890 893 894 
201        896 902 904 907 909 912 913 915 916 923 925 926 931 933 935 
201        939 941 942 943 944 945 947 952 955 956 960 961 963 964 965 
201        966 969 977 991 992 994 997 998 

Number of exchanges: 338


----------------------------------------------------------------------

Outdial Site: D/WASEA
300  bps: 311020600205
1200 bps: 311020600206
2400 bps: 311020600208

206        223 224 226 227 228 232 233 234 235 236 237 241 242 243 244 
206        246 248 251 255 271 277 281 282 283 284 285 286 287 292 296 
206        298 320 322 323 324 325 326 328 329 340 343 344 345 346 358 
206        361 362 363 364 365 367 368 382 386 389 391 392 393 394 395 
206        421 431 432 433 439 441 442 443 447 448 451 453 454 455 461 
206        462 464 467 477 481 483 485 486 487 488 489 522 523 524 525 
206        526 527 528 542 543 544 545 546 547 548 554 557 562 575 583 
206        585 587 621 622 623 624 625 626 628 630 631 632 633 634 635 
206        637 639 641 643 644 646 649 654 655 656 657 661 662 667 670 
206        672 682 684 685 720 721 722 723 725 726 727 728 742 743 744 
206        745 746 747 762 763 764 767 768 771 772 773 774 775 776 778 
206        781 782 783 784 787 788 789 820 821 822 823 824 827 828 836 
206        838 839 842 850 852 854 859 861 865 867 868 869 870 872 874 
206        878 880 881 882 883 885 889 930 932 933 935 936 937 938 940 
206        941 946 947 948 949 953 954 955 965 969 972 977 979 982 986 
206        989 991 993 994 995 996 997 998 999 

Number of exchanges: 234


----------------------------------------------------------------------

Outdial Site: D/NYNYO
300  bps: 311021200315
1200 bps: 311021200316
2400 bps: 311021200412
other   : 311021200028

212        200 205 206 207 208 210 213 214 216 218 219 220 221 222 223 
212        225 226 227 228 230 231 232 233 234 235 236 237 238 239 240 
212        241 242 243 244 245 246 247 248 249 250 251 252 254 255 260 
212        262 264 265 266 267 268 269 272 276 277 279 280 281 283 285 
212        286 288 289 290 291 292 293 294 295 296 297 298 299 301 302 
212        303 304 305 306 307 308 309 310 312 313 314 315 316 319 320 
212        321 322 323 324 325 326 328 329 330 333 334 335 337 339 340 
212        341 342 344 346 348 349 350 351 352 353 354 355 356 357 358 
212        359 360 361 362 363 364 365 367 368 369 370 371 373 374 378 
212        379 380 382 385 390 391 392 393 395 396 397 398 399 401 402 
212        404 406 407 408 409 410 412 413 414 415 416 418 419 420 421 
212        422 425 427 428 430 431 432 433 436 437 439 440 446 447 448 
212        449 451 452 453 455 456 457 458 459 460 461 463 464 465 466 
212        467 468 469 472 473 474 475 476 477 480 481 482 483 484 485 
212        486 487 488 489 490 491 492 493 495 496 502 503 504 505 506 
212        508 509 510 512 513 514 515 517 518 519 520 521 522 523 524 
212        525 527 528 529 530 531 532 533 534 535 536 537 538 541 542 
212        543 545 546 547 548 549 551 552 553 554 556 557 558 559 560 
212        561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 
212        576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 
212        593 594 595 597 598 599 601 602 603 605 606 607 608 609 610 
212        612 613 614 616 617 618 619 620 621 623 624 625 627 628 629 
212        632 633 635 637 639 640 641 642 643 644 645 648 649 650 652 
212        653 654 655 656 657 658 659 661 662 663 664 665 666 667 668 
212        669 671 673 674 675 676 677 678 679 681 682 683 684 685 686 
212        687 688 689 690 691 692 693 694 695 696 697 698 701 702 703 
212        704 705 707 708 709 711 713 714 715 716 717 719 720 721 722 
212        724 725 727 730 731 732 733 734 735 736 737 740 741 742 744 
212        745 746 747 749 750 751 752 753 754 755 757 758 759 760 761 
212        764 765 766 767 768 769 770 772 775 776 777 779 781 785 786 
212        787 790 791 792 793 794 795 796 797 798 799 804 806 807 808 
212        809 812 813 815 818 819 820 822 823 824 825 826 827 828 829 
212        830 831 832 836 837 838 839 840 841 842 844 847 848 850 852 
212        853 854 855 856 858 860 861 862 863 864 865 866 867 868 869 
212        870 871 872 873 874 876 877 878 879 880 881 882 883 884 885 
212        886 887 888 889 891 892 893 898 899 901 902 903 904 905 906 
212        907 908 909 912 916 918 920 921 922 923 924 925 926 927 928 
212        929 930 931 932 933 935 936 938 940 941 942 943 944 945 947 
212        949 951 952 953 954 955 956 957 960 962 963 964 966 967 968 
212        969 971 972 973 974 975 977 978 979 980 982 983 984 985 986 
212        988 989 991 992 993 994 995 996 997 998 999 

Number of exchanges: 611


----------------------------------------------------------------------

Outdial Site: D/CTHAR
300  bps: 311020300120
1200 bps: 311020300121
2400 bps: 311020300105

203        223 224 225 229 231 232 233 236 240 241 242 243 244 246 247 
203        249 252 257 258 273 275 277 278 279 280 282 285 286 289 291 
203        292 293 296 297 298 299 520 521 522 523 524 525 527 528 529 
203        547 548 549 557 559 560 561 563 565 566 568 569 623 627 633 
203        643 644 645 646 647 648 649 651 653 654 657 658 659 660 665 
203        666 667 668 673 674 675 676 677 678 679 683 688 693 721 722 
203        724 725 726 727 728 826 827 828 829 841 843 870 871 872 875 
203        930 936 951 952 953 954 

Number of exchanges: 111

----------------------------------------------------------------------

Outdial Site: D/DCWAS
300  bps: 311020200115
1200 bps: 311020200116
2400 bps: 311020200117

202        200 204 206 207 208 209 210 213 214 217 218 220 222 223 224 
202        225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 
202        240 241 242 243 244 245 246 247 248 249 250 251 252 254 255 
202        256 258 259 260 262 263 264 265 266 267 268 269 270 271 272 
202        273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 
202        288 289 291 292 293 294 295 296 297 298 299 306 307 309 310 
202        317 319 320 321 322 323 324 325 326 328 329 330 331 332 333 
202        334 336 337 338 339 340 341 342 343 344 345 346 347 348 350 
202        351 352 353 354 355 356 357 358 359 360 362 363 364 365 366 
202        369 370 371 372 373 374 376 377 378 379 380 382 383 384 385 
202        386 387 388 389 390 391 392 393 394 395 396 397 398 399 401 
202        402 403 404 406 407 408 409 415 416 417 418 420 421 422 423 
202        424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 
202        439 440 441 442 443 444 445 447 448 449 450 451 452 453 454 
202        455 456 457 458 459 460 461 462 463 464 466 467 468 469 470 
202        471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 
202        486 487 488 490 492 493 495 496 497 498 499 501 502 503 504 
202        505 506 507 509 513 514 516 517 519 520 521 522 523 524 525 
202        526 527 528 529 530 532 533 534 535 536 537 538 539 540 541 
202        542 543 544 545 546 547 548 549 550 551 552 553 554 556 557 
202        558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 
202        573 574 575 576 577 578 580 581 582 583 584 585 586 587 588 
202        589 590 591 592 593 595 597 598 599 601 602 603 604 605 606 
202        608 610 613 618 619 620 622 623 624 625 626 627 628 630 631 
202        632 633 634 635 636 637 638 639 640 641 642 643 644 646 647 
202        648 649 650 651 652 653 654 656 657 658 659 660 661 662 663 
202        664 665 666 667 668 669 670 671 673 675 676 678 679 680 681 
202        682 683 684 685 686 687 688 689 690 691 692 693 694 695 696 
202        697 698 699 702 706 707 708 709 712 713 714 715 719 722 723 
202        724 725 726 727 728 731 732 733 734 735 736 737 738 739 742 
202        745 746 749 750 751 752 753 755 756 758 759 760 761 762 763 
202        764 765 767 768 769 770 772 773 774 775 776 778 779 780 781 
202        783 784 785 786 787 789 790 794 795 797 799 801 802 803 805 
202        806 807 808 812 815 816 817 818 820 821 822 823 824 825 826 
202        827 828 829 830 832 833 834 835 836 837 838 839 840 841 842 
202        843 844 845 846 847 848 849 850 851 852 853 856 857 860 861 
202        862 863 864 865 866 868 869 870 871 872 874 875 876 877 879 
202        881 882 883 885 887 888 889 890 891 892 893 894 895 896 897 
202        898 899 901 904 906 907 912 913 914 916 917 920 921 922 924 
202        925 926 927 928 929 930 931 933 934 935 936 937 938 939 940 
202        941 942 943 944 946 947 948 949 951 952 953 954 955 956 957 
202        960 961 962 963 965 966 967 968 971 972 974 975 977 978 979 
202        980 981 982 983 984 985 986 989 990 991 994 996 998 

Number of exchanges: 643

----------------------------------------------------------------------

Outdial Site: D/CASAN

213        430 431 433 434 438 439 493 494 498 592 594 596 597 598 797 
213        799 985 987 

Number of exchanges: 18


----------------------------------------------------------------------

Outdial Site: D/CAGLE
300  bps: none listed
1200 bps: 311021300412
2400 bps: 311021300413

213        201 202 203 204 205 221 222 223 224 225 226 227 228 229 230 
213        236 237 238 239 245 250 251 252 253 254 255 256 257 258 259 
213        270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 
213        285 286 287 288 289 303 310 314 315 319 340 341 342 343 345 
213        347 351 353 362 380 381 382 383 384 385 386 387 388 389 392 
213        393 394 395 396 399 400 413 415 450 451 452 453 454 455 458 
213        459 460 461 462 463 464 465 466 467 468 469 480 481 482 483 
213        484 485 486 487 488 489 520 550 551 552 553 556 557 558 559 
213        573 580 612 613 614 617 619 620 621 622 623 624 625 626 627 
213        628 629 650 651 652 653 654 655 656 657 658 659 660 661 662 
213        663 664 665 666 667 668 669 680 681 682 683 684 686 687 688 
213        689 714 730 731 732 733 734 735 736 737 738 739 740 741 742 
213        743 744 745 746 747 748 749 765 785 828 829 836 837 838 839 
213        840 841 842 849 850 851 852 854 855 856 857 858 859 870 871 
213        872 873 874 875 876 877 878 879 891 892 893 894 895 896 912 
213        913 930 931 932 933 934 935 936 937 938 939 955 960 962 963 
213        964 965 966 967 968 969 972 974 975 977 

Number of exchanges: 250
----------------------------------------------------------------------
Outdial Site: D/CALAN
(dial 1213+number)
300  bps: none listed
1200 bps: 311021300412
2400 bps: 311021300413

213        200 201 202 203 204 205 206 207 208 209 212 214 215 216 217 
213        219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 
213        234 235 236 237 238 239 241 245 248 249 250 251 252 253 254 
213        255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 
213        270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 
213        285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 
213        300 301 302 303 304 305 306 307 308 309 310 312 313 314 315 
213        316 318 319 320 321 322 323 324 327 328 329 330 331 332 333 
213        334 335 336 337 338 340 341 342 343 345 347 351 353 362 370 
213        371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 
213        386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 
213        402 404 406 408 410 412 413 414 415 416 417 418 419 440 442 
213        443 444 445 446 447 450 451 452 453 454 455 458 459 460 461 
213        462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 
213        477 478 479 480 481 482 483 484 485 486 487 488 489 500 512 
213        515 516 520 527 531 532 533 535 536 537 538 540 541 542 543 
213        544 545 546 550 551 552 553 554 556 557 558 559 560 561 562 
213        563 564 565 566 567 568 569 573 574 578 580 581 582 583 584 
213        585 586 587 588 589 600 601 602 603 604 605 606 607 608 609 
213        612 613 614 615 616 617 618 619 620 621 622 623 624 625 626 
213        627 628 629 630 631 632 633 634 635 636 637 638 639 640 641 
213        642 643 644 645 646 647 648 649 650 651 652 653 654 655 656 
213        657 658 659 660 661 662 663 664 665 666 667 668 669 670 671 
213        672 673 674 675 676 677 678 679 680 681 682 683 684 685 686 
213        687 688 689 692 693 695 696 698 699 700 702 703 712 713 714 
213        715 716 717 718 719 720 721 722 723 724 725 726 727 728 729 
213        730 731 732 733 734 735 736 737 738 739 740 741 742 743 744 
213        745 746 747 748 749 750 751 752 753 754 755 756 757 758 759 
213        760 761 762 763 764 765 769 770 771 772 773 774 775 776 777 
213        778 779 780 781 782 783 785 791 794 801 802 803 804 806 807 
213        809 812 813 814 819 820 821 822 823 824 825 826 827 828 829 
213        836 837 838 839 840 841 842 846 849 850 851 852 854 855 856 
213        857 858 859 860 861 862 863 864 865 866 867 868 869 870 871 
213        872 873 874 875 876 877 878 879 881 887 888 889 891 892 893 
213        894 895 896 903 904 907 908 912 913 920 921 922 923 924 925 
213        926 927 928 929 930 931 932 933 934 935 936 937 938 939 940 
213        941 942 944 945 946 948 949 955 960 962 963 964 965 966 967 
213        968 969 970 971 972 973 974 975 977 978 979 

Number of exchanges: 566

----------------------------------------------------------------------

Outdial Site: D/TXDAL
300  bps: 311021400117
1200 bps: 311021400118
2400 bps: 311021400022

214        202 203 204 205 212 216 217 218 219 220 221 222 223 224 225 
214        226 227 228 229 230 231 233 234 235 238 239 240 241 242 243 
214        244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 
214        259 260 262 263 264 266 269 270 271 272 275 276 278 279 281 
214        284 285 286 287 288 289 290 291 293 296 298 299 301 302 303 
214        305 306 307 308 309 313 314 315 316 317 318 319 320 321 323 
214        324 327 328 330 331 332 333 336 337 339 340 341 343 348 349 
214        350 351 352 353 357 358 360 361 363 368 369 371 372 373 374 
214        375 376 380 381 384 385 386 387 388 391 392 393 394 397 398 
214        399 401 402 403 404 406 407 412 413 414 416 417 418 420 421 
214        422 423 424 426 428 434 436 437 438 441 442 443 444 445 446 
214        450 453 456 458 462 464 466 470 471 475 480 484 487 490 492 
214        494 495 497 502 503 504 506 508 513 514 516 517 518 519 520 
214        521 522 526 528 530 533 539 541 550 553 554 556 557 558 559 
214        565 570 573 574 575 578 579 580 590 591 594 596 601 602 603 
214        604 605 606 607 608 609 612 613 615 616 618 620 621 630 631 
214        634 637 638 641 642 644 647 650 651 653 655 658 659 660 661 
214        669 670 676 680 681 686 688 689 690 691 692 696 698 699 701 
214        702 704 705 706 707 708 709 712 713 714 715 716 717 718 720 
214        721 724 727 733 739 740 741 742 744 745 746 747 748 749 750 
214        751 754 760 761 767 770 771 780 781 783 787 788 790 791 799 
214        804 808 812 815 818 819 820 821 823 824 826 827 828 830 840 
214        841 844 850 851 855 864 867 869 871 879 880 881 888 890 891 
214        902 904 905 907 909 913 917 918 919 920 922 929 931 933 934 
214        939 941 942 943 944 946 948 949 951 952 953 954 956 957 960 
214        964 969 977 978 979 980 985 986 987 988 991 992 993 995 996 
214        997 999 

Number of exchanges: 392


----------------------------------------------------------------------

Outdial Site: D/PAPHI
300  bps: 311021500005 (this outdial currently 2400)
1200 bps: 311021500112
2400 bps: 311021500022

215        221 222 223 224 225 226 227 228 229 231 232 233 235 236 237 
215        238 241 242 243 244 245 246 247 248 254 259 260 263 265 270 
215        271 272 275 276 277 278 279 280 281 283 284 288 289 291 293 
215        299 324 328 329 330 331 332 333 334 335 336 337 338 339 341 
215        342 349 350 351 352 353 354 356 359 365 379 382 386 387 389 
215        422 423 424 425 426 427 438 440 446 447 448 449 450 452 455 
215        456 457 460 461 462 463 464 465 466 467 468 470 471 472 473 
215        474 476 477 480 482 483 485 487 490 492 494 496 497 499 520 
215        521 522 523 525 526 527 528 531 532 533 534 535 537 539 540 
215        542 543 544 545 546 548 549 551 552 553 557 560 561 563 564 
215        565 566 567 568 569 570 572 573 574 576 577 578 580 581 583 
215        585 586 587 590 591 592 595 596 597 620 621 622 623 624 625 
215        626 627 628 629 630 631 632 634 635 636 637 638 639 641 642 
215        643 645 646 649 653 657 659 660 662 663 664 665 667 668 671 
215        673 676 677 680 684 685 686 687 688 690 697 698 722 724 725 
215        726 727 728 729 732 734 735 737 739 742 743 744 745 747 748 
215        751 753 755 761 763 765 768 769 782 784 786 787 789 790 823 
215        824 825 828 829 830 831 833 834 835 836 839 840 841 842 843 
215        844 846 848 849 851 853 854 864 870 871 872 874 875 876 877 
215        878 879 880 881 884 885 886 887 891 892 893 894 895 896 897 
215        898 899 920 922 923 924 925 927 928 930 931 934 936 937 938 
215        940 941 947 951 952 955 960 961 962 963 964 969 971 972 973 
215        975 977 978 980 981 985 986 988 990 991 998 

Number of exchanges: 341


----------------------------------------------------------------------

Outdial Site: D/OHCLE
300  bps: 311021600020
1200 bps: 311021600021
2400 bps: 311021600120

216        221 226 228 229 231 232 234 235 236 237 238 241 243 247 248 
216        249 251 252 261 265 266 267 268 271 278 281 283 289 291 292 
216        295 299 321 328 331 333 338 341 344 348 349 351 356 361 362 
216        363 368 371 381 382 383 389 391 397 398 421 423 425 429 431 
216        432 433 439 441 442 443 444 445 446 447 449 451 459 461 463 
216        464 467 468 469 471 473 475 476 479 481 486 487 491 521 522 
216        523 524 526 529 531 541 543 561 562 566 572 574 575 578 579 
216        581 582 585 586 587 589 591 621 622 623 631 634 641 642 646 
216        651 656 659 661 662 663 664 671 676 681 687 689 691 692 694 
216        696 721 728 729 731 732 734 736 737 741 749 751 752 754 761 
216        765 766 771 777 779 781 789 791 795 822 826 831 835 838 842 
216        843 844 845 851 861 871 881 883 884 885 886 888 891 892 899 
216        921 931 932 941 942 943 944 946 951 953 961 975 987 991 995 

Number of exchanges: 195



----------------------------------------------------------------------

Outdial Site: D/DCWAS
300  bps: 311020200115
1200 bps: 311020200116
2400 bps: 311020200117
                                                                                                                                                                                                                                                
301        206 209 210 217 220 227 229 230 231 236 238 240 248 249 251 
301        258 262 270 277 279 283 286 292 294 295 297 299 306 309 317 
301        320 322 330 336 340 341 344 345 350 353 365 369 372 380 384 
301        386 390 394 402 403 409 417 420 421 422 423 424 427 428 431 
301        434 436 439 441 443 445 449 454 459 460 464 468 469 470 474 
301        480 490 492 493 495 496 497 498 499 502 505 507 509 513 520 
301        530 540 552 559 564 565 567 568 570 571 572 577 580 585 587 
301        588 589 590 593 595 598 599 601 604 608 618 622 627 630 640 
301        649 650 652 654 656 657 670 680 681 688 699 702 713 725 731 
301        735 736 738 753 762 763 770 772 773 774 776 779 794 805 807 
301        808 816 839 840 843 851 852 853 856 864 868 869 870 871 881 
301        888 890 891 894 897 899 907 913 916 921 924 925 926 927 929 
301        930 933 935 937 940 942 946 948 949 951 952 953 961 963 967 
301        972 975 977 980 981 982 983 984 985 986 989 990 

Number of exchanges: 207

----------------------------------------------------------------------

Outdial Site: D/CODEN
300  bps: 311030300114
1200 bps: 311030300115
2400 bps: 311030300021

303        200 220 230 231 232 233 234 235 236 237 238 239 252 255 261 
303        266 270 271 273 277 278 279 280 281 286 287 288 289 290 291 
303        292 293 294 295 296 297 298 299 320 321 322 329 331 333 337 
303        340 341 343 344 348 355 360 361 363 364 366 367 368 369 370 
303        371 372 373 375 377 388 393 394 397 398 399 420 421 422 423 
303        424 425 426 427 428 429 430 431 433 440 441 442 443 444 447 
303        449 450 451 452 455 457 458 460 461 465 466 467 469 470 477 
303        478 480 492 494 497 499 526 530 534 538 556 571 572 573 575 
303        581 592 595 620 623 624 628 629 631 639 640 642 643 649 650 
303        654 657 659 660 665 666 670 671 673 674 676 680 681 688 689 
303        690 691 692 693 694 695 696 697 698 699 720 721 722 727 730 
303        733 739 740 741 743 744 745 750 751 752 753 755 756 757 758 
303        759 760 761 762 763 764 766 770 771 773 777 778 779 780 781 
303        782 786 787 788 789 790 791 792 793 794 795 796 797 798 799 
303        820 821 825 826 829 830 831 832 836 837 839 840 841 843 844 
303        850 851 855 860 861 863 866 868 869 871 877 880 888 889 890 
303        891 892 893 894 896 898 899 922 924 930 932 933 934 935 936 
303        937 938 939 940 964 965 966 969 971 972 973 977 978 979 980 
303        985 986 987 988 989 

Number of exchanges: 275

----------------------------------------------------------------------

Outdial Site: D/FLMIA
300  bps: 311030500120
1200 bps: 311030500121
2400 bps: 311030500122

305        220 221 222 223 224 226 227 230 232 233 235 238 242 245 246 
305        247 248 250 251 252 253 254 255 257 258 261 262 263 264 266 
305        267 268 270 271 274 279 284 285 324 325 326 327 329 332 342 
305        343 347 348 349 350 352 353 354 358 361 362 363 364 365 366 
305        371 372 373 374 375 376 377 378 379 380 381 382 385 386 387 
305        388 397 399 441 442 443 444 445 446 447 448 449 460 464 470 
305        471 477 478 520 526 529 530 531 532 534 535 536 538 539 541 
305        542 543 544 545 547 548 549 550 551 552 553 554 556 557 558 
305        559 560 567 571 573 575 576 577 578 579 590 591 592 593 594 
305        595 596 598 599 620 621 623 624 625 628 633 634 635 636 637 
305        638 642 643 644 649 651 652 653 654 661 662 663 665 666 667 
305        669 670 672 673 674 681 685 687 688 691 693 694 696 751 754 
305        756 757 758 759 762 769 770 773 775 780 787 789 794 795 821 
305        822 823 825 827 829 835 836 854 855 856 858 859 861 864 865 
305        866 867 868 871 873 874 876 880 881 882 883 884 885 886 887 
305        888 889 891 892 893 895 899 931 932 933 935 937 939 940 944 
305        945 947 948 949 951 952 953 956 957 993 995 

Number of exchanges: 251

----------------------------------------------------------------------

Outdial Site: D/ILCHI

	Note:  This is an interim exchange list while the 312 area code
	undergoes a split to produce area code 708.  While the Chicago
	area is in transition, numbers which had been 312 (and are now
	708) should be accessible as a 7 digit call to area code 312
	or an 11 digit call (1708+number) to the new area.  HOWEVER:
	the phone company will be installing a voice intercept on calls
	placed to the 7 digit number before routing you to the new
	11 digit number and we do not know how the modems will respond
	to this intercept message.  You should therefore begin using the
	new 1708 number ASAP.  Exchanges in 708 are also listed in
	the 312 table below during this transition.

300  bps: 311031200410
1200 bps: 311031200411
2400 bps: 311031200024

312        200 201 202 203 204 205 206 207 208 209 210 213 214 215 216 
312        218 220 221 222 223 224 225 226 227 228 229 230 231 232 233 
312        234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 
312        249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 
312        264 265 266 267 268 269 271 272 273 274 275 276 277 278 279 
312        280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 
312        295 296 297 298 299 301 302 303 304 306 307 308 310 313 314 
312        315 316 317 318 319 321 322 323 324 325 326 327 328 329 330 
312        331 332 333 334 335 336 337 338 339 341 342 343 344 345 346 
312        347 348 349 350 351 352 353 354 355 357 358 359 360 361 362 
312        363 364 366 367 368 369 371 372 373 374 375 376 377 378 379 
312        380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 
312        396 397 398 399 401 402 403 404 405 406 407 408 409 410 412 
312        413 415 416 417 418 419 420 421 422 423 424 425 426 427 428 
312        429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 
312        444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 
312        459 460 461 462 463 465 467 468 469 470 471 472 473 474 475 
312        476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 
312        491 492 493 495 496 498 499 501 502 503 504 505 506 507 508 
312        509 510 512 513 514 515 516 517 518 519 520 521 522 523 524 
312        525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 
312        540 541 542 543 544 545 547 548 549 550 551 558 559 560 561 
312        562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 
312        577 578 579 580 581 582 583 584 585 586 588 589 590 591 592 
312        593 594 595 596 597 598 599 601 602 603 604 605 606 607 608 
312        609 612 613 614 615 617 618 619 620 621 622 623 624 625 626 
312        627 628 629 630 631 632 633 634 635 636 637 638 639 640 641 
312        642 643 644 645 646 647 648 649 650 651 652 653 654 655 656 
312        657 658 659 660 661 662 663 664 665 666 667 668 670 671 672 
312        673 674 675 676 677 678 679 680 681 682 684 685 686 687 688 
312        689 690 691 692 693 694 695 696 697 698 699 701 702 703 704 
312        705 706 707 709 712 713 714 715 716 717 718 719 720 721 722 
312        723 724 725 726 727 728 729 730 731 732 733 734 735 736 737 
312        738 739 741 742 743 744 745 746 747 748 749 750 751 752 753 
312        754 755 756 757 758 759 760 761 762 763 764 765 766 767 768 
312        769 770 771 772 773 774 775 776 777 778 779 780 781 782 783 
312        784 785 786 787 788 789 790 791 792 793 794 795 796 797 798 
312        799 801 802 803 804 805 806 807 808 810 812 814 816 817 818 
312        819 820 821 822 823 824 825 826 827 828 829 830 831 832 833 
312        834 835 836 837 838 839 840 841 842 843 844 845 846 847 848 
312        849 850 851 852 853 854 855 856 857 858 859 860 861 862 863 
312        864 865 866 867 868 869 870 871 872 873 874 875 876 877 878 
312        879 880 881 882 883 884 885 886 887 888 889 890 891 892 893 
312        894 895 896 897 898 899 901 902 903 904 905 906 907 908 909 
312        910 913 914 915 916 917 918 919 920 921 922 923 924 925 926 
312        927 928 929 930 931 932 933 934 935 936 937 938 939 940 941 
312        942 943 944 945 946 947 948 949 951 952 953 954 955 956 957 
312        960 961 962 963 964 965 966 967 968 969 971 972 973 974 975 
312        977 978 979 980 981 982 983 984 985 986 987 988 989 990 991 
312        992 993 994 995 996 997 998 

Number of exchanges: 742

---------------------------------------------------------------------

Outdial Site: D/MIAAR
300  bps: none accessable
1200 bps: 311031300216
2400 bps: 311031300024

313        420 426 428 429 434 437 439 449 451 453 454 455 459 475 481 
313        482 483 484 485 486 487 495 572 662 663 665 668 677 747 761 
313        763 764 769 930 936 971 973 981 994 995 996 998 

Number of exchanges: 42

----------------------------------------------------------------------

Outdial Site: D/MIDET
300  bps: 311031300214 
1200 bps: 311031300216
2400 bps: 311031300024

313        222 223 224 225 226 237 240 245 252 255 256 259 267 270 271 
313        272 273 274 275 276 277 278 291 292 295 297 298 320 321 322 
313        323 328 330 331 336 337 341 342 343 345 361 365 366 368 369 
313        371 372 381 382 383 386 388 389 390 393 396 430 431 436 438 
313        440 441 444 446 448 460 491 493 494 496 499 520 521 526 527 
313        531 532 533 534 535 536 537 538 554 556 560 561 562 563 564 
313        565 567 568 571 577 579 581 582 584 592 593 594 596 599 630 
313        690 745 770 780 821 822 823 824 829 831 832 833 834 835 836 
313        837 838 839 841 842 843 845 846 849 861 862 863 864 865 866 
313        867 868 869 871 872 873 874 875 876 881 882 883 884 885 886 
313        891 892 893 894 895 896 897 898 899 921 922 923 924 925 926 
313        927 928 929 931 933 934 935 937 940 943 945 956 961 962 963 
313        964 965 966 972 974 976 980 983 993 

Number of exchanges: 189

----------------------------------------------------------------------

Outdial Site: D/MOSLO
300  bps: 311031400020
1200 bps: 311031400021
2400 bps: 311031400005

314        225 227 231 232 233 234 235 241 247 253 259 261 263 268 275 
314        277 289 291 296 298 321 331 342 343 344 349 351 352 353 355 
314        361 362 367 371 381 382 383 385 388 389 391 394 421 423 424 
314        425 426 427 428 429 432 434 436 441 444 454 458 464 466 469 
314        476 481 487 489 521 522 523 524 525 529 531 532 533 534 535 
314        538 539 541 542 544 551 553 554 567 569 571 572 576 577 578 
314        595 621 622 623 631 638 644 645 647 652 653 658 664 671 677 
314        679 694 721 725 726 727 731 739 741 746 747 752 755 758 768 
314        771 772 773 776 777 781 791 795 821 822 823 826 829 831 832 
314        836 837 838 839 841 842 843 845 846 848 849 851 854 855 862 
314        863 865 867 868 869 871 872 878 879 889 891 892 894 895 899 
314        921 928 938 939 941 942 946 947 949 957 961 962 963 965 966 
314        968 969 973 982 984 991 992 993 994 997 

Number of exchanges: 190


----------------------------------------------------------------------

Outdial Site: D/ININD
300  bps: none accessable
1200 bps:
2400 bps:

317        200 222 226 228 230 231 232 233 235 236 237 238 239 240 241 
317        242 243 244 247 248 251 252 253 254 255 256 257 259 261 262 
317        263 264 265 266 267 269 271 272 273 274 276 277 278 283 290 
317        291 293 297 298 299 321 322 326 328 335 351 352 353 355 356 
317        357 359 422 424 425 431 432 439 441 442 443 445 461 462 464 
317        465 466 467 469 470 471 485 486 488 535 539 541 542 543 545 
317        546 547 549 556 571 573 574 575 576 577 578 579 580 630 631 
317        632 633 634 635 636 637 638 639 681 684 685 686 687 691 694 
317        736 738 745 769 773 776 780 781 782 783 784 786 787 788 823 
317        831 835 838 839 841 842 843 844 845 846 848 849 852 856 861 
317        862 867 870 871 872 873 875 876 877 878 879 881 882 885 887 
317        888 889 891 892 894 895 896 897 898 899 920 921 923 924 925 
317        926 927 928 929 976 994 996 

Number of exchanges: 187



----------------------------------------------------------------------

Outdial Site: D/GAATL
300  bps: 311040400113
1200 bps: 311040400114
2400 bps: 311040400022

404        200 212 215 220 221 222 223 225 230 231 233 237 238 239 240 
404        241 242 243 244 246 247 248 249 250 252 255 256 257 260 261 
404        262 263 264 266 270 271 279 280 281 284 286 288 289 292 294 
404        296 297 299 310 312 313 314 315 316 319 320 321 325 329 330 
404        331 332 333 339 341 343 344 346 347 348 349 350 351 352 355 
404        360 361 362 363 364 365 366 368 370 371 372 373 377 378 380 
404        381 383 388 389 390 391 392 393 394 395 396 399 413 416 417 
404        420 421 422 423 424 425 426 427 428 429 431 432 433 434 435 
404        436 438 439 441 442 443 445 446 447 448 449 451 452 454 455 
404        457 458 460 461 463 466 469 471 473 474 475 476 477 478 482 
404        483 484 487 488 489 491 493 494 496 497 498 499 505 508 512 
404        513 515 520 521 522 523 524 525 526 527 528 529 530 533 550 
404        551 552 558 559 564 565 566 570 572 573 577 578 580 581 584 
404        586 587 588 589 590 591 593 594 603 607 610 618 619 621 622 
404        623 624 626 627 631 633 634 636 639 640 641 642 651 653 656 
404        658 659 661 662 664 668 669 671 676 679 680 681 683 686 688 
404        690 691 696 697 698 699 712 717 723 726 727 728 729 730 732 
404        739 740 741 744 750 751 752 753 755 756 758 760 761 762 763 
404        765 766 767 768 772 774 785 792 794 799 804 808 810 815 822 
404        827 833 835 837 839 840 841 842 843 847 848 850 851 852 853 
404        859 870 871 872 873 874 875 876 877 879 880 881 885 888 890 
404        892 894 897 898 899 907 916 920 921 922 923 924 925 926 928 
404        929 932 933 934 936 938 939 941 942 943 944 945 946 948 949 
404        951 952 953 954 955 956 957 960 961 962 963 964 968 969 971 
404        972 973 974 975 977 978 979 980 981 982 984 985 986 987 988 
404        991 992 993 994 995 996 997 998 999 

Number of exchanges: 384

----------------------------------------------------------------------

Outdial Site: D/FLORL
(dial 1+407)
300  bps: None accessable
1200 bps: 311030500121
2400 bps: 311030500122

407        222 228 236 237 238 239 240 244 246 247 249 256 257 260 262 
407        263 273 275 277 281 282 290 291 292 293 294 295 297 298 299 
407        327 331 332 339 341 342 345 351 352 354 356 363 365 366 380 
407        381 382 420 422 423 424 425 438 469 539 560 568 578 579 623 
407        628 629 644 645 646 647 648 649 651 656 657 658 660 661 671 
407        672 675 677 678 679 682 695 696 699 740 767 774 788 823 824 
407        825 826 827 828 830 831 834 836 839 841 843 849 850 851 855 
407        856 857 859 862 869 872 875 876 877 880 884 886 889 894 895 
407        896 897 898 899 934 939 

Number of exchanges: 126

----------------------------------------------------------------------

Outdial Site: D/CASJO
300  bps: 311040800110
1200 bps: 311040800111
2400 bps: 311040800021

408        221 223 224 225 226 227 234 235 236 237 238 241 243 244 245 
408        246 247 248 249 251 252 253 255 256 257 258 259 262 263 264 
408        265 266 267 268 269 270 272 274 275 276 277 279 280 281 282 
408        283 284 285 286 287 288 289 291 292 293 294 295 296 297 298 
408        299 332 345 353 354 356 358 365 370 371 374 376 377 378 379 
408        395 398 399 432 433 434 435 436 437 441 446 447 448 452 453 
408        463 473 491 492 496 499 522 524 534 552 553 554 559 562 575 
408        578 629 720 721 723 725 727 729 730 732 733 734 735 736 737 
408        738 739 741 742 743 744 745 746 747 748 749 752 756 765 773 
408        864 865 866 867 879 920 922 923 924 925 926 927 929 942 943 
408        945 946 947 954 957 970 971 972 973 974 977 978 980 982 983 
408        984 985 986 987 988 989 991 992 993 994 995 996 997 998 

Number of exchanges: 179
----------------------------------------------------------------------

Outdial Site: D/PAPIT
(dial 1+412)
300  bps: 311021500005
1200 bps: 311021500112
2400 bps: 311021500022

412        200 221 227 231 232 234 236 237 241 242 243 244 247 255 256 
412        257 261 262 263 264 268 269 271 273 276 279 281 288 298 321 
412        322 323 328 331 333 338 341 343 344 351 355 359 361 362 363 
412        364 365 366 367 369 371 372 373 374 381 389 391 392 393 394 
412        421 422 427 429 431 433 434 441 442 456 461 462 464 466 469 
412        471 472 476 481 486 487 488 491 492 497 521 531 551 553 561 
412        562 563 565 566 571 572 578 594 621 622 623 624 633 636 642 
412        644 645 647 648 653 655 661 664 665 672 673 674 675 678 681 
412        682 683 687 692 699 731 734 741 747 749 751 754 761 762 765 
412        766 767 771 777 778 781 782 784 787 788 793 795 798 821 822 
412        823 824 825 826 828 829 831 833 835 840 854 855 856 858 859 
412        881 882 884 885 889 892 921 922 923 928 931 936 937 939 961 
412        963 967 

Number of exchanges: 182

----------------------------------------------------------------------

Outdial Site: D/WIMIL
300  bps: 311041400020
1200 bps: 311041400021
2400 bps: 311041400120

414        221 222 223 224 225 226 227 228 229 237 241 242 243 246 251 
414        252 253 254 255 256 257 258 259 263 264 265 266 271 272 273 
414        274 276 277 278 281 282 283 287 288 289 291 297 298 299 321 
414        322 323 327 332 341 342 343 344 345 347 351 352 353 354 355 
414        357 358 359 362 365 367 372 374 375 377 382 383 384 385 421 
414        422 423 425 427 438 442 444 445 447 449 453 454 461 462 463 
414        464 466 471 475 476 481 482 483 486 491 521 523 524 527 529 
414        535 536 538 541 542 543 544 545 546 547 548 549 562 575 579 
414        581 643 645 647 649 662 663 671 672 678 679 691 744 747 761 
414        762 764 765 768 769 771 774 778 781 782 783 784 785 786 789 
414        791 792 796 797 798 799 821 835 844 871 873 874 881 896 931 
414        933 935 936 937 941 955 961 962 963 964 966 

Number of exchanges: 176


----------------------------------------------------------------------

Outdial Site: D/CAJO
(dial 1+415)
300  bps: 311040800021
1200 bps: 311040800110
2400 bps: 311040800111

415        226 335 336 438 490 498 623 651 656 657 659 683 691 694 770 
415        940 941 948 949 960 961 962 964 965 966 967 968 969 

Number of exchanges: 28


----------------------------------------------------------------------

Outdial Site: D/CASFA
300  bps: 311041500215
1200 bps: 311041500216
2400 bps: 311041500217

415        200 202 204 206 207 208 215 219 221 222 223 225 227 231 232 
415        233 234 235 236 237 238 239 241 243 244 251 252 253 254 255 
415        257 258 259 261 262 263 264 265 266 267 268 269 271 272 273 
415        274 279 281 282 285 287 288 289 291 292 296 297 298 301 302 
415        307 308 309 310 312 330 331 332 333 334 337 338 339 340 341 
415        342 343 344 345 346 347 348 349 351 352 355 357 358 359 362 
415        371 374 375 376 377 378 381 383 385 386 387 388 389 391 392 
415        393 394 395 396 397 398 399 403 406 407 409 410 412 414 419 
415        420 421 425 428 430 431 433 434 435 436 437 441 442 444 445 
415        446 448 451 452 453 454 456 457 459 461 464 465 466 467 468 
415        469 472 474 476 477 478 479 482 483 485 486 488 491 492 495 
415        499 502 504 507 509 512 513 515 517 518 519 520 521 522 523 
415        524 525 526 527 528 529 530 531 532 533 534 535 536 539 540 
415        541 542 543 544 545 546 547 548 549 550 552 553 554 556 557 
415        558 559 561 562 563 564 565 566 567 568 569 570 571 572 573 
415        574 575 576 577 578 579 583 584 585 586 587 588 589 596 597 
415        601 605 607 608 612 613 614 615 616 618 620 621 622 624 626 
415        627 631 632 633 635 636 638 639 641 642 643 644 645 647 648 
415        649 652 653 654 655 658 661 664 665 666 667 668 673 677 678 
415        681 692 695 696 697 701 703 704 705 708 710 715 716 717 718 
415        721 722 724 729 731 737 738 739 741 742 744 748 749 750 751 
415        752 753 755 756 758 759 761 762 763 764 765 768 769 771 772 
415        773 774 775 776 777 781 788 789 801 804 807 809 810 814 816 
415        819 821 822 824 826 832 834 835 836 839 840 841 843 845 848 
415        849 860 861 863 864 865 869 871 872 873 874 875 876 877 878 
415        882 885 891 893 894 895 896 902 904 905 910 912 913 914 918 
415        921 922 923 924 925 927 928 929 931 936 951 952 953 954 955 
415        956 957 970 971 972 973 974 978 979 981 982 983 984 985 986 
415        987 989 990 991 992 993 994 995 996 997 998 999 

Number of exchanges: 432


----------------------------------------------------------------------

Outdial Site: D/CAOAK
300  bps: 311041500108
1200 bps: 311041500109
2400 bps: 311041500224

415        200 202 204 206 207 208 210 215 219 221 222 223 225 227 231 
415        232 233 234 235 236 237 238 239 241 243 244 245 251 252 253 
415        254 255 256 261 262 263 264 265 266 267 268 269 271 272 273 
415        274 276 278 279 281 282 283 284 285 287 288 289 291 292 293 
415        295 296 297 298 301 302 307 308 309 310 317 330 331 332 333 
415        334 337 338 339 346 351 352 357 362 374 376 385 386 387 391 
415        392 393 394 395 396 397 398 399 403 406 407 409 410 412 414 
415        419 420 421 425 428 430 431 433 434 435 436 437 441 442 444 
415        445 446 448 451 452 464 465 466 467 468 469 474 476 477 478 
415        481 482 483 486 495 502 504 509 512 515 517 518 519 520 521 
415        522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 
415        537 538 539 540 541 542 543 544 545 546 547 548 549 550 552 
415        553 554 556 557 558 559 561 562 563 564 565 566 567 568 569 
415        575 576 577 581 582 583 584 585 586 587 588 589 596 597 601 
415        605 607 608 612 613 614 615 616 618 620 621 622 624 626 627 
415        631 632 633 635 636 638 639 641 642 643 644 645 647 648 649 
415        652 653 654 655 658 661 664 665 666 667 668 670 673 677 678 
415        681 695 701 703 704 705 708 710 715 716 717 718 722 724 727 
415        729 731 732 733 736 737 739 741 742 743 744 746 748 749 750 
415        751 752 753 755 756 758 759 761 762 763 764 765 768 769 771 
415        772 773 774 775 776 777 781 782 783 784 785 786 788 789 799 
415        801 804 807 809 810 814 816 819 820 821 822 824 826 831 832 
415        834 835 836 837 838 839 840 841 843 845 848 849 860 861 863 
415        864 865 869 871 872 873 874 875 876 877 878 881 882 884 885 
415        886 887 888 889 891 893 894 895 896 902 904 905 906 910 912 
415        913 914 918 921 922 923 928 929 930 931 932 933 934 935 936 
415        937 938 939 942 943 944 945 946 947 951 952 953 954 955 956 
415        957 970 971 972 973 974 975 977 978 979 981 982 983 984 985 
415        986 987 989 990 991 992 993 994 995 996 997 998 999 

Number of exchanges: 433

----------------------------------------------------------------------

Outdial Site: D/CAPAL
300  bps: 311041500108
1200 bps: 311041500011
2400 bps: 311041500005

415        226 276 278 321 322 323 324 325 326 327 328 329 335 336 340 
415        341 342 343 344 345 347 348 349 354 358 361 363 364 365 366 
415        367 368 369 371 375 377 378 424 429 438 471 475 481 487 489 
415        490 493 494 496 497 498 537 538 570 571 572 573 574 578 579 
415        581 582 591 592 593 594 595 598 623 637 651 656 657 659 670 
415        683 688 691 694 696 722 723 725 727 732 733 745 770 780 782 
415        783 784 785 786 790 791 792 793 794 795 796 797 851 852 853 
415        854 855 856 857 858 859 881 884 886 887 888 889 926 940 941 
415        948 949 960 961 962 964 965 966 967 968 969 

Number of exchanges: 131


----------------------------------------------------------------------

Outdial Site: D/LANOR
300  bps: None accessable
1200 bps:
2400 bps:

504        241 242 243 244 245 246 253 254 255 257 260 271 277 278 279 
504        282 283 286 288 340 341 347 348 349 361 362 363 364 366 367 
504        368 391 392 393 394 398 431 436 441 443 450 451 454 455 456 
504        461 462 464 465 466 467 468 469 482 483 484 486 488 521 522 
504        523 524 525 527 528 529 552 561 565 566 568 569 581 582 583 
504        584 585 586 587 588 589 592 593 595 596 597 656 662 671 676 
504        682 684 689 731 733 734 736 737 738 739 762 821 822 824 826 
504        827 830 831 832 833 834 835 836 837 838 861 862 865 866 883 
504        884 885 887 888 889 891 895 896 897 899 941 942 943 944 945 
504        947 948 949 976 

Number of exchanges: 139


----------------------------------------------------------------------

Outdial Site: D/CASFA
(dial 1+510)
300  bps: 311041500215
1200 bps: 311041500216
2400 bps: 311041500217

510        200 204 208 215 222 223 231 232 233 234 235 236 237 251 253 
510        254 261 262 263 264 265 268 269 271 272 273 279 287 297 298 
510        302 308 309 339 351 352 357 374 376 385 420 425 428 430 436 
510        437 444 446 448 451 452 464 465 466 482 483 486 509 518 519 
510        521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 
510        536 539 540 547 548 549 559 562 568 569 577 596 601 608 613 
510        614 618 620 631 632 633 635 636 638 639 642 643 644 645 649 
510        652 653 654 655 658 667 678 704 710 716 717 718 722 724 729 
510        741 748 758 762 763 769 801 810 814 819 832 834 835 836 839 
510        840 841 843 845 848 849 860 865 869 874 891 893 895 910 970 
510        971 987 990 999 

Number of exchanges: 154

____________________________________________________________________

Outdial Site: D/CAOAK
(dial 1+510)
300  bps: 311041500108
1200 bps: 311041500109
2400 bps: 311041500224

510        200 204 208 215 222 223 231 232 233 234 235 236 237 245 251 
510        253 254 256 261 262 263 264 265 268 269 271 272 273 276 278 
510        279 283 284 287 293 295 297 298 302 308 309 317 339 351 352 
510        357 374 376 385 420 425 428 430 436 437 444 446 448 451 452 
510        464 465 466 481 482 483 486 509 518 519 521 522 523 524 525 
510        526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 
510        547 548 549 559 562 568 569 577 581 582 596 601 608 613 614 
510        618 620 631 632 633 635 636 638 639 642 643 644 645 649 652 
510        653 654 655 658 667 670 678 704 710 716 717 718 724 727 729 
510        732 733 736 741 743 746 748 758 762 763 769 782 783 784 785 
510        786 799 801 810 814 819 820 831 832 834 835 836 837 838 839 
510        840 841 843 845 848 849 860 865 869 874 881 884 886 887 888 
510        889 891 893 895 910 930 932 933 934 935 937 938 939 942 943 
510        944 945 946 947 970 971 975 977 987 990 999 

Number of exchanges: 206

----------------------------------------------------------------------

Outdial Site: D/NYHEM
(dial 1+516)
300  bps: 311021200315
1200 bps: 311021200412
2400 bps: 311021200413
other   : 311021200028

516        220 221 222 223 227 228 229 235 236 237 238 239 248 249 252 
516        255 264 270 285 292 293 294 295 296 299 326 328 333 334 335 
516        336 338 346 349 352 354 355 357 358 364 365 367 371 374 378 
516        379 383 384 391 394 420 431 432 433 437 454 463 466 481 482 
516        483 484 485 486 487 488 489 496 520 521 522 526 531 535 536 
516        538 541 542 546 559 560 561 562 564 565 566 568 569 573 574 
516        575 576 577 579 593 596 598 599 621 623 624 625 626 627 628 
516        629 644 647 656 658 659 663 671 674 676 677 678 679 681 682 
516        683 684 686 691 692 694 731 733 735 739 741 742 745 746 747 
516        752 753 755 756 759 763 764 766 767 773 775 777 781 783 785 
516        789 791 794 795 796 797 798 799 822 823 824 825 826 829 832 
516        833 842 844 845 847 867 868 869 872 873 876 877 883 887 889 
516        890 897 921 922 925 926 931 932 933 934 935 937 938 939 942 
516        943 944 949 997 

Number of exchanges: 199

----------------------------------------------------------------------

Outdial Site: D/NYNYO
(dial 1+516)
300  bps: 311021200315
1200 bps: 311021200316
2400 bps: 311021200412
other   : 311021200028

516        221 222 223 227 228 229 235 236 237 238 239 248 249 252 255 
516        264 270 285 292 293 294 295 296 299 326 328 333 334 336 338 
516        346 349 352 354 357 358 364 365 367 371 374 378 379 391 420 
516        431 432 433 437 454 463 466 481 482 483 484 485 486 487 488 
516        489 496 520 521 526 531 535 536 538 541 542 546 559 560 561 
516        562 564 565 566 568 569 574 575 576 577 579 593 596 598 599 
516        621 623 624 625 626 627 628 629 644 647 656 658 663 671 674 
516        676 677 678 679 681 682 683 684 686 691 692 694 731 733 735 
516        739 741 742 745 746 747 752 753 755 756 759 763 764 766 767 
516        773 775 781 783 785 789 791 794 795 796 797 798 799 822 823 
516        824 825 826 829 832 842 844 845 847 867 868 869 872 873 876 
516        877 883 887 889 890 897 921 922 926 931 932 933 934 935 937 
516        938 939 942 943 944 949 997 

Number of exchanges: 187





----------------------------------------------------------------------

Outdial Site: D/TNMEM
(dial 1+601)
300  bps: 3110 
1200 bps: 3110
2400 bps: 3110

601        342 349 393 781 851 

Number of exchanges: 5

----------------------------------------------------------------------

Outdial Site: D/AZPHO
300  bps: 311060200022
1200 bps: 311060200023
2400 bps: 311060200026

602        220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 
602        235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 
602        250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 
602        265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 
602        280 285 320 331 336 340 345 350 351 352 370 371 375 376 377 
602        379 381 382 389 390 391 392 393 395 396 397 412 420 423 431 
602        433 434 435 436 437 438 439 440 441 443 450 451 460 461 464 
602        468 470 481 482 483 484 486 490 491 493 494 495 496 497 498 
602        528 530 531 534 540 542 543 545 547 548 549 551 553 554 563 
602        585 588 589 596 597 598 630 631 640 641 644 649 650 661 678 
602        681 693 730 731 732 752 756 759 784 786 788 789 820 821 827 
602        829 830 831 832 833 834 835 838 839 840 841 842 843 844 846 
602        848 849 852 853 856 860 861 862 863 864 866 867 869 870 872 
602        873 876 877 878 879 890 891 892 893 894 895 897 898 899 921 
602        924 925 926 929 930 931 932 933 934 935 936 937 938 939 940 
602        941 942 943 944 945 946 947 948 949 951 952 953 954 955 956 
602        957 961 962 963 964 965 966 967 968 969 970 971 972 973 974 
602        975 977 978 979 980 981 985 986 990 991 992 993 994 995 996 
602        997 998 

Number of exchanges: 272

602        566 583 584 546 492 561 581 582 780 569 586 471 837 373 380 
602        983 982 984 986 983 671 987 988 

Number of exchanges: 22
(These exchanges require 1+602 XXX-XXXX dialing)

----------------------------------------------------------------------

Outdial Site: D/MNMIN
300  bps: 311061200120
1200 bps: 311061200121
2400 bps: 311061200022 

612        220 221 222 223 224 227 228 229 290 291 292 293 296 297 298 
612        323 330 331 332 333 334 335 336 337 338 339 340 341 342 343 
612        344 347 348 349 368 370 371 372 373 374 375 376 377 378 379 
612        420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 
612        435 436 437 438 439 440 441 443 444 445 446 447 448 449 450 
612        451 452 454 455 456 457 458 459 460 461 462 463 464 469 470 
612        471 472 473 474 475 476 477 478 479 481 482 483 484 487 488 
612        489 490 491 492 493 494 496 497 498 499 520 521 522 526 527 
612        529 533 534 535 536 537 538 540 541 542 544 545 546 552 553 
612        557 559 560 561 566 569 571 572 574 588 591 593 620 621 622 
612        623 624 625 626 627 631 633 635 636 638 639 640 641 642 643 
612        644 645 646 647 648 649 653 663 667 673 681 683 687 688 690 
612        696 698 699 720 721 722 723 724 725 726 727 728 729 730 731 
612        733 735 736 737 738 739 741 750 753 754 755 757 770 771 772 
612        774 776 777 778 779 780 781 782 784 785 786 788 789 822 823 
612        824 825 827 828 829 830 831 832 835 851 853 854 858 861 863 
612        865 866 867 868 869 870 871 872 874 879 881 884 885 887 888 
612        890 891 892 893 894 895 896 897 920 921 922 924 925 926 927 
612        929 931 932 933 934 935 936 937 938 939 941 942 944 949 976 
612        977 989 

Number of exchanges: 287


----------------------------------------------------------------------

Outdial Site: D/MABOS
300  bps: 311061700311
1200 bps: 311061700313
2400 bps: 311061700026

617        200 223 224 225 226 227 230 231 232 233 234 235 236 237 239 
617        241 242 243 244 245 246 247 248 252 253 254 257 258 261 262 
617        263 264 265 266 267 268 269 271 274 275 276 277 278 279 280 
617        282 284 285 286 287 288 289 290 292 296 298 320 321 322 323 
617        324 325 326 327 328 329 330 331 332 333 335 337 338 340 343 
617        345 348 349 350 353 354 357 361 362 364 367 375 377 380 381 
617        382 387 389 391 393 394 395 396 397 421 423 424 426 427 428 
617        429 431 432 434 436 437 438 439 442 444 445 446 449 450 451 
617        455 456 457 461 463 464 466 469 471 472 473 479 482 483 484 
617        486 487 488 489 491 492 493 494 495 496 497 498 499 522 523 
617        524 527 532 534 536 538 539 541 542 546 547 552 553 556 558 
617        560 561 562 565 566 567 568 569 570 571 572 573 574 576 577 
617        578 579 581 586 589 592 593 594 595 596 598 599 621 622 623 
617        625 628 629 630 633 635 637 638 641 642 643 646 647 648 654 
617        661 662 665 666 669 674 680 684 693 694 695 696 698 720 721 
617        722 723 724 725 726 727 728 729 730 731 732 733 734 735 736 
617        737 738 739 740 742 743 748 749 756 770 773 774 776 781 782 
617        783 786 787 789 825 841 842 843 845 846 847 848 849 855 859 
617        860 861 862 863 864 868 873 876 884 887 889 890 891 893 894 
617        895 899 923 924 925 926 929 930 931 932 933 935 936 937 938 
617        942 944 945 951 954 955 956 958 962 964 965 966 969 972 973 
617        974 979 981 983 984 985 

Number of exchanges: 321
----------------------------------------------------------------------

Outdial Site: D/OHCOL
(dial 1+614)
300  bps: 311021600020
1200 bps: 310021600021
2400 bps: 311021600120

614        221 222 223 224 225 227 228 229 231 235 236 237 238 239 243 
614        248 249 251 252 253 258 261 262 263 265 267 268 271 272 274 
614        275 276 278 279 281 288 291 292 293 294 296 297 299 325 329 
614        337 338 341 351 361 365 371 395 421 424 431 433 436 438 442 
614        443 444 445 447 451 457 459 460 461 462 463 464 466 469 471 
614        475 476 478 479 481 486 487 488 491 492 497 523 538 548 575 
614        621 644 645 752 755 756 759 761 764 766 771 777 785 786 791 
614        792 793 794 821 833 836 837 841 842 846 847 848 851 852 855 
614        860 861 863 864 866 868 870 871 875 876 877 878 879 881 882 
614        885 888 889 890 891 895 898 899 927 964 965 

Number of exchanges: 146


----------------------------------------------------------------------

Outdial Site: D/MOSLO
(dial 1+618)
300  bps: 311031400020
1200 bps: 311031400021
2400 bps: 311031400005

618        271 274 337 451 452 482 583 797 

Number of exchanges: 8


----------------------------------------------------------------------

Outdial Site: D/CASDI
300  bps: 3110
1200 bps: 3110
2400 bps: 3110

619        221 222 223 224 225 226 229 230 231 232 233 234 235 236 237 
619        238 239 258 260 262 263 264 265 266 267 268 270 271 272 273 
619        274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 
619        289 290 291 292 293 294 295 296 297 298 299 336 338 390 401 
619        404 406 408 412 413 416 417 419 420 421 422 423 424 425 426 
619        427 428 429 435 437 440 441 442 443 444 447 448 449 450 451 
619        452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 
619        469 470 472 474 475 476 477 479 482 483 484 485 487 488 490 
619        491 492 493 494 495 496 497 502 505 506 508 514 518 522 524 
619        525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 
619        540 541 542 543 544 545 546 547 548 549 551 552 553 554 556 
619        557 558 559 560 561 562 563 565 566 569 570 571 573 574 575 
619        576 578 579 580 581 582 583 584 585 586 587 588 589 592 594 
619        604 660 661 662 668 669 670 672 673 690 691 692 693 694 695 
619        696 697 698 699 701 702 717 980 981 987 990 991 

Number of exchanges: 222




----------------------------------------------------------------------

Outdial Site: D/DCWAS
(dial 1+703)
300  bps: 311020200115
1200 bps: 311020200116
2400 bps: 311020200117

703        204 207 214 218 222 235 237 239 241 242 243 246 247 250 255 
703        256 260 263 264 266 271 273 274 276 278 280 281 284 285 321 
703        323 325 329 339 351 352 354 355 356 358 359 360 370 378 379 
703        385 391 406 407 415 418 425 430 435 437 438 440 442 444 448 
703        450 451 455 461 471 476 478 481 482 486 487 503 506 516 517 
703        519 521 522 524 525 527 528 532 533 534 536 538 548 549 550 
703        551 553 556 557 558 560 569 573 578 591 602 603 620 631 641 
703        642 643 644 648 658 660 661 664 671 683 684 685 689 690 691 
703        698 706 709 712 715 719 733 734 739 742 746 749 750 751 756 
703        758 759 760 761 764 765 768 769 780 781 787 790 795 799 802 
703        803 815 817 818 820 821 823 824 826 827 830 834 836 838 841 
703        845 846 847 848 849 850 860 866 874 875 876 883 892 893 904 
703        912 914 920 922 931 934 938 941 960 968 971 974 978 979 998 

Number of exchanges: 195

-----------------------------------------------------------------------

Outdial Site: D/ILCHI

	Remember:  the exchanges listed below are duplicated in the
	312 list!  Also, you MUST dial 1708-xxx-yyyy to reach numbers
	in the 708 (and 815) area code.

300  bps: 311031200410
1200 bps: 311031200411
2400 bps: 311031200024

708        200 201 203 205 206 208 209 210 213 215 216 218 223 228 231 
708        232 234 240 244 246 249 250 251 253 255 256 257 258 259 260 
708        272 279 289 290 291 293 295 296 297 298 299 301 303 304 307 
708        310 314 315 316 317 318 319 323 325 328 330 331 333 335 336 
708        339 343 344 345 349 350 351 352 354 355 357 358 359 360 361 
708        362 364 366 367 369 371 377 381 382 383 385 386 387 388 389 
708        390 391 392 393 394 396 397 398 401 402 403 405 406 409 412 
708        416 418 420 422 423 424 425 426 428 429 430 432 433 437 438 
708        439 441 442 446 447 448 449 450 451 452 453 455 456 457 458 
708        459 460 462 469 470 473 474 475 479 480 481 482 484 485 490 
708        491 492 495 496 498 499 501 502 503 504 505 506 510 512 513 
708        515 516 517 518 519 520 524 526 529 530 531 532 534 535 537 
708        540 541 543 544 547 550 551 560 562 563 564 566 570 571 572 
708        573 574 575 576 577 578 579 584 590 593 594 595 596 597 598 
708        599 603 605 607 608 612 613 614 615 617 618 619 620 623 627 
708        628 629 632 634 635 636 639 640 647 652 653 654 655 656 657 
708        658 659 662 665 668 671 672 673 674 675 676 677 678 679 680 
708        681 682 687 688 689 690 691 692 695 696 697 698 699 705 706 
708        709 713 714 717 719 720 724 729 730 739 741 742 746 747 748 
708        749 754 755 756 757 758 759 766 771 773 780 788 789 790 795 
708        798 799 801 803 806 810 816 817 818 820 823 824 825 827 830 
708        831 832 833 834 835 837 839 840 841 843 844 848 849 850 851 
708        852 857 858 859 860 862 863 864 865 866 867 868 869 870 872 
708        877 879 882 884 885 887 888 891 892 893 894 895 896 897 898 
708        904 905 910 913 914 916 919 920 926 931 932 934 937 940 941 
708        945 946 948 949 952 953 954 956 957 960 961 963 964 965 966 
708        967 968 969 971 972 974 979 980 981 982 983 985 986 990 991 
708        998 

Number of exchanges: 406

----------------------------------------------------------------------

Outdial Site: D/TXHOU
300  bps: 311071300113
1200 bps: 311071300114
2400 bps: 311071300024

713        200 220 221 222 223 224 225 226 227 228 229 230 233 235 236 
713        237 238 240 241 242 244 246 247 252 253 254 261 263 264 265 
713        266 267 268 269 270 271 272 274 277 278 280 282 283 284 285 
713        286 287 289 293 295 320 324 326 328 331 332 333 334 335 336 
713        337 338 339 341 342 343 346 347 350 351 353 354 355 356 358 
713        359 360 363 364 367 370 371 373 374 376 377 378 383 388 390 
713        391 392 393 394 395 420 421 422 424 425 426 427 428 431 432 
713        433 434 436 437 438 439 440 441 442 443 444 445 446 447 448 
713        449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 
713        464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 
713        479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 
713        494 495 496 497 498 499 520 521 522 523 524 525 526 527 528 
713        529 530 531 535 536 537 540 541 542 546 547 548 549 550 551 
713        552 556 558 561 563 565 568 571 575 577 578 579 580 583 584 
713        586 587 588 589 590 591 596 599 620 621 622 623 626 627 629 
713        630 631 633 635 636 639 640 641 643 644 645 649 650 651 652 
713        653 654 655 656 657 658 659 660 661 662 663 664 665 666 667 
713        668 669 670 671 672 673 674 675 676 678 679 680 681 682 683 
713        684 685 686 688 690 691 692 694 695 696 697 699 720 721 723 
713        726 728 729 731 732 733 734 738 739 741 744 746 747 748 749 
713        750 751 752 753 754 757 758 759 761 762 763 764 765 768 769 
713        771 772 774 775 776 777 778 779 780 781 782 783 784 785 786 
713        787 788 789 790 791 792 793 794 795 796 797 798 799 820 821 
713        822 823 824 825 826 827 828 829 831 833 834 835 836 840 841 
713        842 844 845 846 847 850 852 853 854 855 856 857 858 859 861 
713        862 863 864 865 866 867 868 869 870 871 872 873 874 875 876 
713        877 878 879 880 882 883 884 886 888 890 891 892 893 894 895 
713        896 897 898 899 920 921 922 923 924 926 928 929 930 931 932 
713        933 935 937 938 939 940 941 943 944 946 947 948 951 952 953 
713        954 955 956 957 960 961 963 964 965 966 967 968 969 971 972 
713        973 974 975 977 978 980 981 983 984 985 986 987 988 989 991 
713        992 993 995 996 997 998 999 

Number of exchanges: 472



----------------------------------------------------------------------

Outdial Site: D/CACOL
300  bps: 311071400119
1200 bps: 311071400121
2400 bps: 311071400102

714        275 276 335 350 351 352 353 354 355 356 357 358 359 360 369 
714        370 381 382 383 384 386 387 422 431 602 681 682 683 684 685 
714        686 687 688 689 749 780 781 782 783 784 785 787 788 789 790 
714        791 792 793 794 795 796 797 798 799 820 822 823 824 825 829 
714        872 873 874 875 876 877 880 881 882 883 884 885 886 887 888 
714        889 

number of exchanges : 76

----------------------------------------------------------------------

Outdial Site: D/CASAN
300  bps: 311071400023
1200 bps: 311071400024
2400 bps: 311071400021

714        220 228 229 236 239 241 250 251 253 255 256 258 259 261 262 
714        265 282 283 285 289 321 322 323 324 325 326 327 328 329 332 
714        367 372 373 374 380 385 414 415 418 432 433 441 447 449 455 
714        458 472 474 475 476 490 491 494 497 499 502 503 509 513 515 
714        516 517 519 520 521 522 523 524 525 526 527 528 529 530 531 
714        532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 
714        547 548 549 550 551 552 553 554 556 557 558 559 565 566 567 
714        568 569 572 579 581 582 583 586 587 588 589 630 631 632 633 
714        634 635 636 637 638 639 640 641 642 643 644 645 646 647 648 
714        649 650 651 660 662 663 664 665 666 667 668 669 670 671 673 
714        675 680 691 692 693 707 708 712 720 721 722 723 724 725 726 
714        727 729 730 731 732 733 738 739 740 741 742 743 744 745 746 
714        747 748 750 751 752 754 755 756 757 758 759 760 761 762 764 
714        768 770 771 772 773 774 775 776 777 778 779 786 821 826 827 
714        828 830 831 832 833 834 835 836 837 838 839 840 841 842 843 
714        846 847 848 850 851 852 854 855 856 857 858 859 863 870 871 
714        879 890 891 892 893 894 895 896 897 898 921 937 938 939 951 
714        952 953 954 955 956 957 960 961 962 963 964 965 966 968 969 
714        970 971 972 973 974 975 977 978 979 990 991 992 993 994 995 
714        996 997 998 999 

Number of exchanges: 289

----------------------------------------------------------------------

Outdial Site: D/NYNYO
(dial 1+718)
300  bps: 311021200315
1200 bps: 311021200316
2400 bps: 311021200412
other   : 311021200028

718        200 204 209 217 221 224 225 229 230 232 233 234 235 236 237 
718        238 240 241 244 247 248 251 252 253 256 257 258 259 260 261 
718        262 263 265 266 267 268 270 271 272 273 274 275 276 277 278 
718        279 282 284 287 291 296 297 317 318 321 322 326 327 330 331 
718        332 335 336 337 338 339 341 342 343 345 346 347 349 351 352 
718        353 354 356 357 358 359 360 361 363 366 370 372 373 375 376 
718        377 380 381 383 384 385 386 387 388 389 390 392 395 397 398 
718        403 417 421 423 424 426 428 429 434 435 436 438 439 441 442 
718        443 444 445 446 447 448 449 451 452 453 454 455 456 457 458 
718        459 461 462 463 464 465 467 468 469 470 471 474 476 478 479 
718        480 481 482 485 486 489 492 493 494 495 497 498 499 507 520 
718        522 523 525 526 527 528 529 531 533 539 541 544 545 552 557 
718        565 571 574 575 591 592 596 599 604 615 622 624 625 626 627 
718        628 629 630 631 632 633 634 636 638 639 641 642 643 644 645 
718        646 647 648 649 651 656 657 658 659 667 670 672 680 692 693 
718        694 698 699 706 712 720 721 723 726 727 728 729 735 738 739 
718        740 743 745 746 748 754 755 756 760 761 762 763 764 767 768 
718        769 771 773 774 776 778 779 780 782 783 784 786 788 789 793 
718        797 802 803 805 816 821 826 827 830 831 832 833 834 835 836 
718        837 843 845 846 847 848 849 851 852 853 854 855 856 857 858 
718        859 868 871 875 876 883 886 891 894 895 896 897 898 899 917 
718        919 921 922 927 932 934 935 937 938 939 941 942 945 946 948 
718        949 951 953 955 956 961 962 963 965 966 967 968 969 972 977 
718        978 979 981 983 984 987 990 995 996 997 998 999 

Number of exchanges: 357




----------------------------------------------------------------------

Outdial Site: D/UTSLC
300  bps: 311080100020
1200 bps: 311080100021
2400 bps: 311080100012

801        220 237 240 250 251 252 254 255 261 262 263 264 265 266 268 
801        269 272 273 277 278 287 292 295 298 299 321 322 328 350 355 
801        359 363 364 366 451 460 461 466 467 468 480 481 482 483 484 
801        485 486 487 488 521 522 524 526 530 531 532 533 534 535 536 
801        537 538 539 543 544 546 547 549 561 562 565 566 569 570 571 
801        572 573 575 576 578 579 580 581 582 583 584 585 588 594 595 
801        596 633 799 933 942 943 944 947 964 965 966 967 968 969 972 
801        973 974 975 977 

Number of exchanges: 109



----------------------------------------------------------------------

Outdial Site: D/FLTAM
300  bps: 311081300020
1200 bps: 311081300021
2400 bps: 311081300124

813        221 222 223 224 225 226 227 228 229 231 232 234 236 237 238 
813        239 240 241 242 247 248 251 253 254 258 259 264 265 272 273 
813        276 281 286 287 289 620 621 622 623 626 628 633 634 641 645 
813        653 654 661 662 664 671 677 681 684 685 689 690 830 831 832 
813        835 837 839 840 854 855 870 871 872 873 874 875 876 877 878 
813        879 880 881 882 883 884 885 886 887 888 889 920 931 932 933 
813        935 948 949 960 961 962 963 968 969 971 972 973 974 977 978 
813        979 980 985 986 987 988 989 990 996 

Number of exchanges: 114

----------------------------------------------------------------------

Outdial Site: D/ILCHI
(dial 1+815)
300  bps: 311031200410
1200 bps: 311031200411
2400 bps: 311031200024

815        254 372 423 424 436 439 469 474 478 485 722 723 725 726 727 
815        729 740 741 744 773 774 834 838 886 

Number of exchanges: 24

----------------------------------------------------------------------

Outdial Site: D/MOKCI
300  bps: 311081600104
1200 bps: 311081600221
2400 bps: 311081600113

816        221 223 224 225 228 229 231 234 241 242 243 245 246 247 251 
816        252 254 257 274 275 276 283 292 322 331 333 346 348 353 356 
816        358 361 363 373 374 391 395 421 426 435 436 444 452 453 454 
816        455 459 461 464 466 468 471 472 474 478 483 497 521 523 524 
816        525 531 532 537 556 561 572 576 578 587 589 591 654 698 734 
816        737 741 743 751 753 756 757 759 761 763 765 767 781 792 795 
816        796 821 822 833 836 842 844 854 861 871 881 891 921 922 923 
816        924 926 931 932 941 942 943 966 968 995 997 

Number of exchanges: 116


----------------------------------------------------------------------

Outdial Site: D/TXDAL
300  bps: 311021400117
1200 bps: 311021400118
2400 bps: 311021400022

817        261 265 267 268 273 329 355 356 366 379 421 424 425 429 430 
817        432 449 450 461 467 469 475 477 481 498 530 540 543 572 577 
817        588 589 640 654 667 671 679 695 784 792 832 856 884 890 922 
817        925 929 930 961 962 963 967 

Number of exchanges: 52


----------------------------------------------------------------------
Outdial Site : D/CAGLE
300  bps: none listed
1200 bps: 311021300412
2400 bps: 311021300413

818        200 240 241 242 243 244 246 247 248 249 301 303 304 350 351 
818        352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 
818        367 368 370 371 372 373 374 375 376 377 378 379 381 382 393 
818        397 398 399 400 401 402 403 404 405 406 409 440 441 442 443 
818        444 445 446 447 448 449 450 459 500 501 502 503 504 505 506 
818        507 508 509 528 542 545 546 547 548 560 564 565 566 567 568 
818        569 574 575 577 578 579 580 584 753 754 760 761 762 763 764 
818        765 766 767 768 769 777 780 781 782 783 784 785 786 787 788 
818        789 790 791 792 793 794 795 796 797 798 799 818 821 831 840 
818        841 842 843 845 846 847 848 890 891 892 893 894 895 896 897 
818        898 899 901 902 903 904 905 906 907 908 909 951 952 953 954 
818        955 956 957 972 980 981 982 983 984 985 986 987 988 989 990 
818        994 995 997 

Number of exchanges: 183

----------------------------------------------------------------------
Outdial Site : D/CALAN
300  bps: none listed
1200 bps: 311021300412
2400 bps: 311021300413

818        200 240 241 242 243 244 246 247 280 281 282 284 285 286 287 
818        288 289 300 301 302 303 307 308 309 350 357 358 359 401 402 
818        409 442 443 444 445 446 447 448 450 451 457 458 459 500 502 
818        507 529 545 546 547 548 570 571 572 573 574 575 576 579 580 
818        805 821 956 

Number of exchanges: 63


----------------------------------------------------------------------

Outdial Site: D/TNMEM
300  bps: none accessable

901        227 272 274 276 278 320 323 324 325 327 332 344 345 346 348 
901        353 357 358 360 362 363 365 366 367 368 369 371 372 373 375 
901        377 382 385 386 387 388 395 396 397 398 452 454 458 465 475 
901        476 483 484 485 486 521 522 523 524 525 526 527 528 529 531 
901        532 533 535 543 544 572 575 576 577 578 579 597 654 678 681 
901        682 683 684 685 721 722 725 726 728 729 743 744 745 747 748 
901        752 753 754 755 756 757 758 761 762 763 765 766 767 774 775 
901        785 789 794 795 797 829 853 854 867 872 873 876 877 922 942 
901        946 947 948 976 

Number of exchanges: 124


----------------------------------------------------------------------

Outdial Site: D/MOKCI
(dial 1+913)
300  bps: 311021200315
1200 bps: 311021200316
2400 bps: 311021200412
other   : 311021200028

913        236 262 268 281 287 299 321 334 339 341 342 345 362 371 375 
913        381 383 384 422 432 441 451 469 491 492 541 551 573 574 576 
913        588 596 599 621 631 642 648 649 661 676 677 681 721 722 724 
913        764 780 782 787 788 791 829 831 888 894 897 962 967 

Number of exchanges: 58

----------------------------------------------------------------------

Outdial Site: D/CASAC
300  bps: 311091600011
1200 bps: 311091600012
2400 bps: 311091600007

916        227 228 255 262 263 264 277 278 321 322 323 324 325 326 327 
916        328 329 331 332 334 338 339 344 348 349 351 353 355 360 361 
916        362 363 364 366 368 369 371 372 373 374 381 382 383 386 387 
916        388 391 392 393 394 395 399 421 422 423 424 425 427 428 429 
916        433 440 441 442 443 444 445 446 447 448 449 451 452 453 454 
916        455 456 457 464 481 482 483 484 485 486 487 488 489 531 535 
916        537 539 551 552 553 557 566 567 568 593 631 635 636 638 641 
916        643 646 648 649 653 654 657 665 682 683 684 685 686 687 688 
916        689 731 732 733 734 736 737 739 747 761 762 763 764 765 766 
916        767 768 769 852 854 855 863 867 920 921 922 923 924 925 927 
916        928 929 933 939 942 944 951 952 955 956 957 961 962 965 966 
916        967 969 971 972 973 974 978 983 985 987 988 989 991 992 

Number of exchanges: 179

(Exchanges listed below require the 1+ phone number dialing)

916        721 722 723 725 726 727 728 729 745 785 752 753 754 756 757 
916        758 

Number of exchanges: 16 


----------------------------------------------------------------------

Outdial Site: D/NCRTP
300  bps: 311091900020
1200 bps: 311091900021
2400 bps: 311091900124

919        248 254 266 269 280 286 361 362 365 382 383 387 460 467 469 
919        470 471 477 479 481 489 490 493 528 530 541 543 544 546 549 
919        560 575 596 598 620 660 662 664 677 681 682 683 684 687 688 
919        733 737 740 755 772 779 781 782 783 787 790 821 828 829 831 
919        832 833 834 836 839 840 846 847 848 850 851 856 859 860 870 
919        872 876 878 880 881 890 899 929 932 933 941 942 956 962 966 
919        967 968 976 990 991 992 

Number of exchanges: 96

----------------------------------------------------------------------

Outdial Site: D/NJNBR
(dial 1+908)
300  bps: 311020100001
1200 bps: 311020100301
2400 bps: 311020100022

908        202 205 214 218 220 225 231 238 246 247 248 249 251 254 257 
908        271 274 283 287 297 302 306 321 324 329 356 360 390 406 407 
908        412 417 418 422 424 442 457 463 469 494 510 519 524 525 526 
908        545 548 549 560 561 562 563 572 602 603 607 613 632 634 636 
908        658 668 679 685 699 704 707 715 721 722 723 725 727 738 745 
908        750 752 753 754 755 756 757 769 805 819 821 826 828 844 846 
908        855 873 878 880 883 885 906 932 937 954 968 980 981 985 

Number of exchanges: 104
----------------------------------------------------------------------

Outdial Site: D/NJNEW
300  bps: 311020100001
1200 bps: 311020100301
2400 bps: 311020100022

908        200 232 233 241 245 272 273 276 277 289 298 317 322 351 352 
908        353 354 355 381 382 388 396 419 464 474 486 499 522 527 541 
908        558 574 582 594 602 634 636 654 665 686 687 688 709 737 750 
908        760 771 789 815 820 851 855 862 889 913 925 931 964 965 969 

Number of exchanges: 60

----------------------------------------------------------------------

Outdial Site: D/NYNYO
300  bps: 311021200315
1200 bps: 311021200316
2400 bps: 311021200412
other   : 311021200028

914        235 237 251 253 270 282 285 286 287 288 289 321 328 332 333 
914        335 337 345 347 375 376 378 381 390 391 395 397 422 423 428 
914        472 476 478 523 524 576 591 592 631 632 633 636 641 642 644 
914        654 662 664 665 667 668 674 681 682 683 684 686 693 694 696 
914        697 698 699 721 723 725 738 761 768 771 776 779 784 789 792 
914        793 833 834 835 899 921 925 933 934 935 937 939 946 948 949 
914        961 963 964 965 967 968 969 993 997 

Number of exchanges: 99

----------------------------------------------------------------------

                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     
                                                                                                                                                                                                                                                                                                                                                                           
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>
<*>                                                                        <*>
<*>                                                                        <*>                                                                                                                                             
<*>   THIS HAS BEEN A MODERNZ PRESENTATION                                 <*>                                                                                                                                                                                                                                                                                
<*>                                                                        <*>                                                                                                                                                                                                               
<*>                             SEE YOU ALL AT MATRIX BBS (908)905-6691    <*>                                                                                                                                                                                                         
<*>                                                                        <*>
<*>                NON-PURSUITABLE WIHTOUT A GLOBAL                        <*>                                                                                                                                                                                                                               
<*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*><*>                                                                                                                         
                                                                                                                                                             
                                    
                                                                                                                                                                               
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      
                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                

                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        
                                                                                                                                                                                                                                                                                                                 
                                                                                                                                                                                                                                                               