



                                    Page 162




                        The Official Phreaker's Manual

                TOWARD UNIVERSAL INFORMATION SERVICES VIA ISDN

Phase one, the present. The local network of today, although still largely
voice oriented, is already on the path to Universal Information Services.
Lightguide fiber is dramatically expanding the capacity of local networks,
helping to lower the costs and increase the demand for high-bandwidth,
Information Age services. And public networks are increasingly digital and
geared for data and special services.  For example:

   *  The AT&T Network Systems 5ESS switch, designed by Bell Laboratories, can
serve as the hub of a local digital network through deployment of remote
modules at locations up to 100 miles from a host central office.

   *  The Integrated Special Services Network (ISSN) is a channel networks that
provides special services, customer control options and digital private lines
rearrangeable under software control. The ISSN incorporates digital carrier
terminating equipment such as the D4 Channel Bank, D5 Digital Terminal System
and Digital Access and Cross-connect Systems (DACS).

   *  The New Centrex is bringing greater levels of customer control, improved
services and a broad range of data capabilities to the business customer.

 Todays public networks consist of multiple or overlay networks.  The public
switched network, or circuit network, is the base network.  Two kinds of
overlay networks provide special services.  Channel networks carry private
lines leased by large customers and transmit much of today's data and image
traffic; they also handle traffic for network operations support.  Packet
networks carry data communications, while packet switching is used internal to
public networks for common channel signaling to set up, route and take down
calls, or to give customers information.
   "Overlay networks help telecommunications companies efficiently meet growing
demand for digital transmission and special services," says Stan Johnston,
Market Planning Manager, Network Systems Evolution, in AT&T Network Systems.
"Their integration into a signal network, however, would be still
more effective."
   Phase two, the Integrated Services Digital Network (ISDN).  The ISDN is a
concept to which AT&T is commited--and it's the foundation for Universal
Information Services.  The central idea of ISDN, as AT&T Network Systems sees
it, is to provide an individual user a link to the local central office of
generous bandwidth--a digital subscriber line that can carry 144,000 bits per
second.  The bandwidth is subdivided into two 64,000-bit channels, which may
carry voice or data or both, and one 16,000-bit channel for packetized
signaling information or data transport.  Such a link provides convenient
"integrated" network access by accommodating voice, data and signaling over a
single line.
   The ISDN will make it easier for a customer to get varied services from
public and private networks.  More bandwidth for big customers will be
available through another ISDN access standard, the extended digital subscriber
line, which provides 1.5 million bit per second as 24 channels of 64,000 bits
each.
   In 1986, new software from Bell Labs will enable the 5ESS switch to
accommodate ISDN-sized 144,000-bit channels that standardize and simplify
subscribers' use of local networks.  AT&T is committed to future products that
will also be ISDN-compatible.  Other vendors, too, some of whom already plan to
build premises, terminal and other equipment to ISDN standards, will make ISDN
a cooperative effort.
   By providing integrated digital access to networks, ISDN  will make
important progress toward the goal of Universal Information Services.  But

                                    Page 163




                        The Official Phreaker's Manual

overlay networks will continue to divvy up the transport job.  And messages
needing less than 144,000 bits per second will not fill their allotted
bandwidth, leaving capacity underutilized.
   Phase three, Universal Information Services.  Rooted in the fertile ground
of 5ESS switches, ISDN equipment and technologies such as wideband packet
transport, Universal Information Services will bear fruit during the 1990s.
From a single kind of network will hang services as different as apples,
oranges and pears.  Just as network access was integrated in ISDN, transport
functions will increasingly be integrated by powerful new equipment evolved
from equipment developed for the ISDN.  Where customers once got standard-
sized ISDN channels, they'll get big bandwidth for large jobs, little bandwidth
for small jobs.

*** retyped from PROTO, AT&T Bell Laboratories report to executives on new
technologies, without written permission from the editors.  (heh, heh.)

Subscriptions:  $15.00 per year, published bi-monthly.  Send check payable to
"Bell Laboratories PROTO," to PROTO Circulation Manager, Room 3E-230, 150 John
F. Kennedy Parkway, Short Hills, N.J.  07078.

:LIQUID:CRYSTAL:
wisdom is safety





































                                    Page 164




                        The Official Phreaker's Manual

==Phrack Inc.==
Volume One, Issue Two, Phile #7 of 9

         @@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@
         @                                                          @
         @                   _  _        _______                    @
         @                  | \/ |      / _____/                    @
         @                  |_||_|etal / /hop                       @
         @                  __________/ /                           @
         @                 /___________/                            @
         @            Headquarters of Phrack Newsletter             @
         @                     (314) 432-0756                       @
         @                    Proudly Presents                      @
         @                      MCI Overview                        @
         @                   Written on 11/16/85                    @
         @                           by                             @
         @                                                          @
         @              Knight Lightning & Taran King               @
         @                                                          @
         @@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@

MCI Communications Corporation, headquartered in Washington, D.C., provides a
full range of domestic and international telecommunications services, including
voice and data, telex and cable, paging and mobile telephone, and time
sensitive message delivery.

Since its founding in 1968, MCI has grown to more than $1.6 billion in annual
sales and serves more than 1.9 million business, residential and government
customers through its four major business units:

MCI Telecommunications

MCI Airsignal

MCI International

MCI Digital Information Services


MCI TELECOMMUNICATIONS

   MCI Telecommunications provides domestic interstate long distance service
throughout all 50 states, plus Puerto Rico, the U.S. Virgin Islands, and major
calling areas of Canada.  It is also authorized to provide varying degrees of
intrastate long distance service in some states.

MCI also is the first long distance carrier other than AT&T to offer direct
dial service overseas.  International telephone service is available to all
residential and commercial customers (with the exception of Private Line
customers).  In October, 1984 the first international service agreements were
announced with the following countries:  Argentina, Belgium, Brazil, East
Germany, Greece, United Arab Emirates, and the United Kingdom.

Total capital investment in MCI's long distance network is approximately $2
billion.  MCI's network, the second largest in the U.S., employs microwave
optical fiber, satellite and various digital transmission technologies.

Subscribers - Domestic Long Distance (as of 10/84)

                                    Page 165




                        The Official Phreaker's Manual

-----------   ----------------------
Residential              1.4 million
Commercial                .3 million
     Total               1.7 million

Operations - (as of 10/84)
Network Miles...20,543 (microwave, optical fiber, satellite)
Circuits.......238,000
Employees........9,500 (full-time, approx.)

MCI AIRSIGNAL

MCI Airsignal provides personal message delivery and car telephone services.
MCI Message Service is offered in more than 50 metropolitan areas.  In 1984,
service will commence in New York City, Baltimore-Washington, Los Angeles, and
Chicago.  MCI car telephone service is offered in 20 markets.

Personal Message Delivery Service

ALPHANUMERIC MESSAGE SERVICE

Displays up to 40-character message using letters and/or numbers. Memory and
recall ability.  Alerts subscriber with a silent visual alert or a soft tone.

DISPLAY MESSAGE SERVICE

Displays up to 24-digit message (e.g., phone number, stock quotes, sales
figures, coded messages).  Memory and recall capability.  Alerts customer to
message with a silent visual alert or a soft tone.

TONE MESSAGE SERVICE

Notifies customer of a message with a soft tone.

VOICE MESSAGE SERVICE

Receives message in actual voice of caller.

EXPRESS MESSAGE SERVICE

Receives and stores messages.  Instantly alerts subscriber via pager when a
message is received.

Car Telephone Service

Enables customers to place calls to or receive calls from anywhere in the
world, 24 hours a day, as they travel in their cars.  With the advent of new
cellular technology, both the quality and the accessibility of car telephone
service will vastly improve.

MCI has thus far obtained franchises to operate a new kind of mobile phone
service,  cellular telephone, in Minneapolis and Pittsburgh, and has received
favorable decisions from FCC administration law judges authorizing service in
Los Angeles, Denver-Boulder, and Kansas City. MCI has applied for licenses to
provide cellular service in 81 metropolitan areas.

MCI Airsignal Branch Sales Offices


                                    Page 166




                        The Official Phreaker's Manual

Personal Message Service/Conventional Mobile Phone Service

Birmingham                             (205)  942-2924
Sacramento                             (916)  444-2350
Memphis                                (901)  682-9658
Cleveland                              (216)  464-7311
Dallas                                 (214)  788-5111
Fresno                                 (209)  486-7410
Las Vegas                              (702)  382-7461
Denver                                 (303)  778-7878
Portland                               (503)  227-2556
Philadelphia                           (215)  677-9845
Atlanta                                (404)  252-2114
West Florida                           (813)  875-3404
Minneapolis                            (612)  544-8175
Kansas City                            (913)  648-8090
Miami                                  (305)  491-0122
Pittsburgh                             (412)  343-1611
Houston                                (713)  464-2516
Bakersfield                            (805)  832-2346

Cellular Telephone Offices

            Minneapolis-St. Paul                   (612)  544-3312
            Los Angeles                            (714)  527-0385
            Elsewhere in California                (800)  344-3455
            Headquarters - Washington, D.C.        (202)  429-9660


MCI INTERNATIONAL

MCI International provides private-line voice service to several overseas
countries, and data and message services, including telex, cablegram, leased
channel, and packet switching communications, to more than 200 overseas points.
MCI has moved into two new areas of service:  International direct-dial
telephone service and international electronic mail and hard-copy delivery
services.

International Record Services

TELEX SERVICE   (domestic and international) permits instantaneous, two-way,
written communications with other subscribers worldwide.  Customers can send
messages at any time, even though the receiving terminal may be unattended. MCI
International offers access to its telex service from a variety of terminals
and networks; not only subscribers with telex terminals but also those with
communicating word processors, data terminals or computers that communicate
over telephone lines can take advantage of MCI International telex service.  To
subscribers connected to its own telex network, MCI International offers World
Message Services--a package of communications offerings including telex,
cablegram and MCI Mail services.  Various service enhancements are available to
save time, improve operating efficiency and simplify records keeping for telex
users.

CABLEGRAM SERVICE, the traditional means of international written
communications, offers flexibility in delivery and economical rates for shorter
messages.  Cablegrams can be delivered to virtually any overseas
point.Subscribers with telex terminals or various other types of equipment can
access and TELUS cablegram switch and take advantage of such service

                                    Page 167




                        The Official Phreaker's Manual

enhancements as abbreviated addressing and departmental billing.

LEASED
CHANNEL SERVICE  provides an exclusive line between a U.S. firm and it's
overseas office for private communications 24 hours a day.  Each MCI
International leased channel is tailored to meet the needs of a specific
customer for teleprinter, facsimile, voice and/or data traffic. For subscribers
with several offices requiring private communications with each other, MCI
International offers a versatile message-switching service. Voice/data leases
can be configured to meet a whole array of communicating needs; for example,
one channel might carry data traffic from a computer at night, voice
communications during office hours, and simultaneous teleprinter messages at
any time.  Data channels can handle requirements for traffic at any speed from
1200 bits per second to 1.544 megabits per second.

IMPACS SERVICE   uses packet-switching technology to provide international
communications service between data terminals and computers.  Impacs offers
on-line, real-time connections and enables many types of incompatible systems
to communicate.  Impacs service offers virtually error-free transmission
because of the error-detection and retransmission capability of the network.

INSTALINK SERVICE allows businesses overseas to use regular telex equipment to
access remote computing systems and databases in the U.S.  Subscribers can
retrieve data from a computer-based information service or use a computing
system connecting to a packet-switching network in the U.S.

INTERNATIONAL
FACSIMILE SERVICE enables subscribers to send duplicates of original documents
overseas quickly and efficiently, even when neither the sender or the receiver
has facsimile transmission equipment, or when the sender and receiver have
incompatible equipment.

DATEL SERVICE  provides automatic or voice-coordinated data transmission at
speeds up to 2400 bits per second. Either digital or analog facsimile traffic
can be transmitted via Datel.  Datel facilities are conditioned to ensure
high-quality transmission.  The MCI International switching center allows
communications between incompatible terminals.

MARITIME SERVICES   provide instant, high--quality contact between ships at sea
or offshore rigs, and between these vessels and land-based subscribers
worldwide.

International Voice Services

PRIVATE
LINE SERVICE   provides, fast, easy access to a single overseas location at an
economical monthly rate.  This technically efficient system maximizes the use
of line capacity by recognizing idle time and assigning a speaker to a
transmission path only when the path is needed.  Users can dial a four-digit
extension from a regular business phone to reach a key overseas location.

International Mail Services

WORLD
MESSAGE SERVICE   subscribers can access the domestic electronic mail and
hard-copy delivery offerings of MCI Mail.  In addition, MCI International is
developing fast, low-cost services that will deliver electronic messages and
high-quality printed documents worldwide.

                                    Page 168




                        The Official Phreaker's Manual


Customer Service

THE CUSTOMER TROUBLE REPORTING ASSISTANCE CENTER at MCI International addresses
customer concerns such as equipment maintenance and service performance
questions.  Customer service specialists, on duty 24 hours a day on business
days, answer questions and electronically route service requests to technicians
nationwide.

MCI DIGITAL INFORMATION SERVICES CORP.

MCI Digital Information Services, MCI's newest unit, provides high-speed,
low-cost, time-sensitive message delivery (MCI Mail), either electronically or
via hard copy.

MCI Mail   provides time-sensitive document delivery to anyone, anywhere vial
MCI's long-distance telephone network.  MCI Mail can reach a recipient
instantly, in four hours or less, or overnight by noon the next day.  Prices
are as much as 90 percent lower than comparable time-sensitive mail delivery
services.  MCI Mail can be delivered electronically, terminal to terminal, or
laser printed on letterhead stationery with the customer's signature.

MCI Mail customers can even order gifts and services direct through MCI Mail,
ranging from software and paper for personal computers to investment advisory
services to travel specials.

There are no sign-up, monthly service charges or "connect time" charges for MCI
Mail.  MCI Mail can be used by virtually any personal computer, word processor,
electronic typewriter, data terminal, telex, or other digital communications
device.  The service is accessed by a local telephone call or 800 number.

MCI Mail

INSTANT delivery to an "electronic" mailbox.

FOUR-HOUR paper delivery by courier to 17 major metropolitan areas regardless
of point of origin.

OVERNIGHT paper delivery by courier by noon the next day in 20,000 continental
U.S. cities.

MCI LETTER transmitted electronically to the MCI digital postal center nearest
its destination, then delivered locally by the U.S. Postal Service.

TELEX DISPATCH enables MCI Mail subscribers to transmit messages to the more
than 1.6 million telex subscribers worldwide.

VOLUME MAIL enables customers to send large mailings in a variety of letter
formats, at substantial savings in delivery time and expense.

         ============================================================
              Look for more MCI Files coming to Metal Shop soon!

                 This has been a Knight Lightning Presentation
         ============================================================




                                    Page 169




                        The Official Phreaker's Manual

                               Reference Tables

   Just some notes that you will always try to find but can never!
























































                                    Page 170




                        The Official Phreaker's Manual

==Phrack Inc.==
Volume One, Issue One, Phile #5 of 8

                            Using MCI Calling Cards
                                      by
                               Knight Lightning
                                    of the
                                  2600 Club!

How to dial international calls on MCI:

               "Its easy to use MCI for international calling."

1.  Dial your MCI access number and authorization code (code = 14 digit number,
however the first 10 digits are the card holders NPA+PRE+SUFF).

2.  Dial 011

3.  Dial the country code

4.  Dial the city code and the PRE+SUFF that you want.

Countries served by MCI:

Country                          code|Country                     code
-------------------------------------|--------------------------------
Algeria..........................213 |New Zealand..................064
Argentina........................054 |Northern Ireland.............044
Australia........................061 |Oman.........................968
Belgium..........................032 |Papua New Guinea.............675
Brazil...........................055 |Qatar........................974
Canada................Use Area Codes |Saudi Arabia.................966
Cyprus...........................357 |Scotland.....................044
Denmark..........................045 |Senegal......................221
Egypt............................020 |South Africa.................027
England..........................044 |Sri Lanka....................094
German Democratic Republic           |Sweden.......................046
(East Germany)...................037 |Taiwan.......................886
Greece...........................030 |Tanzania.....................255
Jordan...........................962 |Tunisa.......................216
Kenya............................254 |United Arab Emirates.........971
Kuwait...........................965 |Wales........................044
Malawi...........................265 |
======================================================================

Thats 33 countries in all. To get the extender for these calls dial 950-1022 or
1-800-624-1022.

For local calling:

1.  Dial 950-10222 or 1-800-624-1022

2.  Wait for tone

3.  Dial "0", the area code, the phone number, and the 14 digit authorization
code. You will hear 2 more tones that let you know you are connected.

  - Knight Lightning -->  The 2600 Club!

                                    Page 171




                        The Official Phreaker's Manual

=====================================================================


























































                                    Page 172




                        The Official Phreaker's Manual

            AT&T INTERNATIONAL DIALING COUNTRY CODES AS OF 2-17-85

                             FILE BY:  Lock Lifter
                          +=========================+

*UNITED KINGDOM/IRELAND
------------------------------------
IRELAND.........................353
UNITED KINGDOM...................44

*EUROPE
------------------------------------
ANDORRA..........................33
AUSTRIA..........................43
BELGIUM..........................32
CYPRUS..........................357
CZECHOLSLOVAKIA..................42
DENMARK..........................45
FINLAND.........................358
FRANCE...........................33
GERMAN DEMOCRATIC REPUBLIC.......37
GERMANY, FEDERAL REPUBLIC OF.....49
GIBRALTAR.......................350
GREECE...........................30
HUNGARY..........................36
ICELAND.........................354
ITALY............................39
LIECHTENSTEIN....................41
LUXEMBOURG......................352
MONACO...........................33
NETHERLANDS......................31
NORWAY...........................47
POLAND...........................48
PORTUGAL........................351
ROMANIA..........................40
SAN MARINO.......................39
SPAIN............................34
SWEDEN...........................46
SWITZERLAND......................41
TURKEY...........................90
VATICAN CITY.....................39
YUGOSLAVIA.......................38

*CENTRAL AMERICA
------------------------------------
BELIZE..........................501
COSTA RICA......................506
EL SALVADOR.....................503
GUATEMALA.......................502
HONDURAS........................504
NICARAGUA.......................505
PANAMA..........................507

*AFRICA
------------------------------------
ALGERIA.........................213
CAMEROON........................237
EGYPT............................20

                                    Page 173




                        The Official Phreaker's Manual

ETHIOPIA........................251
GABON...........................241
IVORY COAST.....................225
KENYA...........................254
LESOTHO.........................266
LIBERIA.........................231
LIBYA...........................218
MALAWI..........................265
MOROCCO.........................212
NAMIBIA.........................264
NIGERIA.........................234
SENEGAL.........................221
SOUTH AFRICA.....................27
SWAZILAND.......................268
TANZANIA........................255
TUNISIA.........................216
UGANDA..........................256
ZAMBIA..........................260
ZIMBABWE........................263

*PACIFIC
------------------------------------
AMERICAN SAMOA..................684
AUSTRAILIA.......................61
BRUNEI..........................673
FIJI............................679
FRENCH POLYNESIA................689
GUAM............................671
HONG KONG.......................852
INDONESIA........................62
JAPAN............................81
KOREA, REPUBLIC OF...............82
MALAYSIA.........................60
NEW CALEDONIA...................687
NEW ZEALAND......................64
PAPUA NEW GUINEA................675
PHILIPPINES......................63
SAIPAN..........................670
SINGAPORE........................65
TAIWAN..........................886
THAILAND.........................66

*INDIAN OCEAN
------------------------------------
PAKISTAN.........................92
SRI LANKA........................94

*SOUTH AMERICA
------------------------------------
ARGENTINA........................54
BOLIVIA.........................591
BRAZIL...........................55
CHILE............................56
COLOMBIA.........................57
ECUADOR.........................593
GUYANA..........................592
PARAGUAY........................595
PERU.............................51

                                    Page 174




                        The Official Phreaker's Manual

SURINAME........................597
URUGUAY.........................598
VENEZUELA........................58

*NEAR EAST
------------------------------------
BAHRAIN.........................973
IRAN.............................98
IRAQ............................964
ISRAEL..........................972
JORDAN..........................962
KUWAIT..........................965
OMAN............................968
QATAR...........................974
SAUDI ARABIA....................966
UNITED ARAB EMIRATES............971
YEMEN ARAB REPUBLIC.............967

*CARIBBEAN/ATLANTIC
------------------------------------
FRENCH ANTILLES.................596
GUANTANAMO BAY (US NAVY BASE)....53
HAITI...........................509
NETHERLANDS ANTILLES............599
ST. PIERRE AND MIQUELON.........508

*INDIA
------------------------------------
INDIA............................91

*CANADA
------------------------------------
TO CALL CANADA, DIAL 1 + AREA CODE +
LOCAL NUMBER.

*MEXICO
------------------------------------
TO CALL MEXICO, DIAL 011 + 52 + CITY CODE+ LOCAL NUMBER.

***NOTES :DO NOT FORGET ABOUT THE TIME DIFFERENCE WHEN CALLING OUTSIDE OF YOUR
TIME ZONE. CALLING CARDS CAN BE USED OVER SEAS TO CALL BACK INTO THE U.S. FOR
FURTHER INFORMATION CALL TOLL-FREE 1-800-874-0000. DIAL '#' AFTER THE COMPLETE
NUMBER TO MAKE THE CALL GO THROUGH FASTER.
















                                    Page 175




                        The Official Phreaker's Manual

                    **************************************
                    *                                    *
                    *    International Dialing Codes     *
                    *         Country + Routing          *
                    *                                    *
                    *      (Typed by The Dagda Mor)      *
                    *       (Edited by The Jammer)       *
                    *                                    *
                    **************************************

To dial international calls:

International Access Code + Country code + Routing code

Example :

To call Frankfurt, Germany, you would do the following:

011 + 49 + 611 + (# wanted) + # sign(octothrope)

The # sign at the end is to tell Bell that you are done entering in all the
needed info.

Here is the list of Country Codes, listed next to the country, and the routing
codes listed next to the city.

Andorra- 33          Argentina- 54
-------              ---------
all points- 078      Buenos Aires- 1


Australia- 61        Austria- 43
---------            -------
Melbourne- 3         Innsbruck- 5222
Sydney- 2            Vienna- 222


Bahrain- 973         Belgium- 32
-------              -------
no routing needed    Antwerp- 31
                     Brussels- 2


Belize- 501          Bolivia- 591
------               -------
no routing needed    La Paz- 2


Brazil- 591          Chile- 56
------               -----
Brasilia-61          Santiago- 2
Rio de Janeiro- 21   Valparaiso- 31
Sao Paulo- 11


China- 86            Colombia- 56
-----                --------
Tainan- 62           none needed

                                    Page 176




                        The Official Phreaker's Manual

Taipei- 2


Costa Rica- 506      Cyprus- 357
----- ----           ------
no routing needed    Nicosia- 21


Denmark- 45          Ecuador- 593
-------              -------
Aalborg- 8           Cuenca- 4
Copenhagen 1 or 2    Quito- 2


El Salvador- 503     Fiji- 679
----------           ----
no routing needed    none needed


France- 33           Germany- 49
------               -------
Bordeaux- 56         Berlin- 30
Marseille- 91        Bonn- 228
Nice- 93             Frankfurt- 661
Paris- 1             Munich- 89


German. Rep- 37      Greece- 30
------- ---          ------
Berlin- 2            Athens- 1
                     Rhodes- 241


Guam- 671            Guatamala- 502
----                 ---------
no routing needed    Guatemala City- 2


Guyana- 592          Haiti- 509
------               -----
Georgetown- 02       Port Au Prince- 1


Hoduras- 504         Hong Kong- 852
-------              ---- ----
no routing needed    Hong Kong- 5
                     Kowloon- 3


Indonesia- 62        Iran- 98
---------            ----
Jakarta- 21          Teheran- 21


Iraq- 964            Ireland- 353
----                 -------
Baghdad- 1           Dublin- 1
                     Galway- 91

                                    Page 177




                        The Official Phreaker's Manual



Israel- 978          Italy- 39
------               -----
Haifa- 4             Florence- 55
Jerusalem- 2         Naples- 81
Tel Aviv- 3          Rome- 6
                     Venice- 41


Ivory Coast- 225     Japan- 81
----- -----          -----
no routing needed    Hiroshima- 822
                     Tokyo- 3
                     Yokohama- 45


Kenya- 254           Korea- 82
-----                -----
Nairobi- 2           Pusan- 51
                     Seoul- 2


Kuwait- 965          Liberia- 231
------               -------
no routing needed    none needed


Libya- 218           Lechtenstein- 4
-----                ------------
Tripoli- 21          All points- 75


Luxembourg- 352      Malaysia- 60
----------           --------
no routing needed    Kuala Lumpur- 3


Monaco- 33           Netherlands- 31
------               -----------
All points- 93       Amsterdam- 20
                     Rotterdam- 10
                     The Hague- 70


New Caledonia- 687   New Zealand- 64
--- ---------        --- -------
no routing needed    Auckland- 9
                     Wellinton- 4


Nicaragua- 505       Nigeria- 234
---------            -------
Managua- 2           Lagos- 1


Norway- 47           Panama- 507
------               ------

                                    Page 178




                        The Official Phreaker's Manual

Bergen- 5            none needed
Oslo- 2


Papua New Guinea-675 Paraguay- 595
----- --- ------     --------
no routing needed    Asuncion- 21


Peru- 51             Phillippines- 63
----                 ------------
Arequipa- 542        Manila- 2
Lima- 14

Portugal- 351        Romania- 40
--------             -------
Lisbon- 19           Bucuresti- 0


San Marino- 39       Saudi Arabia- 966
--- ------           ----- ------
All points- 541      Riyadh- 1


Senegal- 221         South Africa- 27
-------              ----- ------
no routing needed    Cape Town- 21
                     Pretoria- 12


Spain- 34            Sri Lanka- 94
-----                --- -----
Barcelona- 3         Colombo- 1
Canary Is.- 28
Madrid- 1
Seville- 54


Suriname- 597        Sweden- 46
--------             ------
no routing needed    Goteborg- 31
                     Stockholm- 8


Switzerland- 41      Tahiti- 689
-----------          ------
Berne- 31            none needed
Geneva- 22
Lucerne- 41
Zurich- 1


Thailand- 66         Tunisia- 216
--------             -------
Bangkok- 2           Tunis- 1


Turkey- 90           United Arab

                                    Page 179




                        The Official Phreaker's Manual

------               Emirates- 971
Istanbul- 11         --------
                     Abu Dhabi- 2
                     Ajman- 6
                     Al Ain- 3
                     Aweir- 49
                     Dubai- 4
                     Fujairah- 91
                     Jebel Dhana- 5
                     Sharjah- 6
                     Umm-Al-Quwain- 6


United Kingdom- 44   USSR- 7
------ -------       ----
Belfast- 232         Kiev- 044
Cardiff- 222         Leningrad- 812
Edinburgh- 31        Minsk- 017
Glasgow- 41          Moscow- 095
Liverpool- 51        Tallinn- 0142
London- 1

Vatican City- 39     Venezuela- 58
------- ----         ---------
All points- 6        Caracas- 2
                     Maracaibo- 61

Yugoslavia- 38
----------
Belgrade- 11
Zagreb- 41




























                                    Page 180




                        The Official Phreaker's Manual

                    **************************************
                    *                                    *
                    *           MAX ACCESS PORTS         *
                    *                                    *
                    *        (LEXITEL CORPORATION)       *
                    *                                    *
                    *   WORD PROCESSED BY THE DAGDA MOR  *
                    *                                    *
                    **************************************

ADRIAN,MI............313-263-0191  LIVONIA, MI..........313-261-6970
AKRON,OH.............216-275-9814  LOS ANGELES, CA......213-624-9041
ANN ARBOR, MI........313-451-2121  LOUISVILLE, KY.......502-568-6204
ATLANTA, GA..........404-525-1769  MARION, OH...........614-387-1011
AVON LAKE, OH........216-933-2823  MCKEESPORT, PA.......412-664-4870
BADEN, PA............412-869-1360  MENTOR, OH...........216-255-1645
BALTIMORE, MD........301-444-7280  MIDDLETOWN, OH.......513-423-1066
BEAVER FALLS, PA.....412-847-3640  MILWAUKEE, WI........414-933-1880
BIRMINGHAM, MI.......313-649-0730  MINNEAPOLIS, MN......612-375-0280
BOSTON, MA...........617-267-9134  MONESSEN, PA.........412-684-8710
BUFFALO, NY..........716-854-0802  MORTON GROVE,IL......312-950-1066
BUTLER, PA...........412-285-9081  NEWARK, NJ...........201-624-5040
CANTON, OH...........216-455-1425  NEWARK, OH...........614-349-8754
CHICAGO, IL..........312-950-1066  NEW CASTLE, PA.......412-656-9420
CHILLICOTHE, OH......614-772-1066  NEW YORK, NY.........212-950-1066
CINCINNATI, OH.......513-421-1880  OAK LAWN, IL.........312-950-1066
CLEVELAND, OH........216-771-6614  PHILADELPHIA, PA.....215-751-9711
COLUMBUS, OH.........614-950-1066  PITTSBURG, PA........412-391-9532
DALLAS, TX...........214-653-1047  PLYMOUTH, MI.........313-451-2121
DAYTON, OH...........513-223-0366  PONTIAC, MI..........313-332-0500
DETROIT, MI..........313-950-1066  PORT HURON, MI.......313-982-7115
ELK GROVE, IL........312-950-1066  PHOENIX, AZ..........602-242-0252
ELYRIA, OH...........419-323-4431  QUEENS, NY...........718-204-7330
FINDLAY, OH..........419-424-5934  SANDUSKY, OH.........419-625-1289
GLEENSHAW, PA........412-486-7394  SHARON, PA...........412-983-0100
GRAND RAPIDS, MI.....616-456-7925  SPRINGFIELD, OH......513-950-1066
GREENSBURG, PA.......412-836-8110  STEUBENVILLE, OH.....614-283-1756
HACKENSACK, NJ.......201-342-2815  ST. LOUIS, MO........314-289-9100
HOUSTON, TX..........713-224-0982  ST. PAUL, WI.........612-375-0280
INDIANA, PA..........412-349-8760  TOLEDO, OH...........419-255-1316
INDIANAPOLIS, IN.....317-638-4442  TROY, OH.............513-335-2303
KALAMAZOO, MI........616-342-0266  TURTLE CREEK, PA.....412-823-1500
KANSAS CITY, MO......816-474-6193  WASHINGTON, DC.......202-479-4411
KOKOMO, IN...........317-453-9932  WASHINGTON, PA.......412-225-1800
LA GRANGE, IL........312-950-1066  WARREN, MI...........313-268-9120
LANCASTER, OH........614-687-0159  XENIA, OH............513-376-2991
LANSING, MI..........517-950-1066  YOUNGSTOWN, OH.......216-746-2021
LAFAYETTE, IN........317-423-5492  ZANESVILLE, OH.......614-454-6815











                                    Page 181




                        The Official Phreaker's Manual

      ******************** METROFONE ACCESS NUMBERS ********************

ANAHEIM, CA          (714)527-7055  LOS ANGELES, CA      (213)992-8282
ATLANTA, GA          (404)223-1000  LOS ANGELES, CA      (213)202-6117
AUSTIN, TX           (512)474-6057  MIAMI, FL            (305)326-3300
BALTIMORE, MD        (301)659-7700  MILWAUKEE, WI        (414)277-1805
BEAUMONT, TX         (713)833-9331  MINNEAPOLIS, MN      (612)370-9000
BOSTON, MA           (617)482-3222  NEW ORLEANS, LA      (504)566-8500
BUFFALO, NY          (716)852-9200  NEW YORK, NY         (212)732-7430
CHICAGO, IL          (312)853-4700  NEWARK, NJ           (201)645-9220
CINCINNATI, OH       (513)241-1747  OAKLAND, CA          (415)836-6900
CLEVELAND, OH        (216)861-5163  OKLAHOMA CITY, OK    (405)232-9011
COLUMBUS, OH         (614)224-0577  OMAHA, NE            (402)422-1120
CULVER CITY, CA      (213)410-0078  PHILADELPHIA, PA     (215)351-0100
DALLAS, TX           (214)742-4500  PITTSBURGH, PA       (412)261-5720
DAYTON, OH           (513)228-1576  RENO, NV             (702)329-1025
DENVER, CO           (303)623-5326  RICHMOND, VA         (804)225-1920
DETROIT, MI          (313)963-4847  ST. LOUIS, MO        (314)342-1130
EL MONTE, CA         (213)350-1028  SACRAMENTO, CA       (916)443-6921
ELK GROVE, IL        (312)981-8870  SAN ANTONIO, TX      (512)224-9600
FT. LAUDERDALE, FL   (305)462-3530  SAN DIEGO, CA        (714)233-0327
FT. WORTH, TX        (817)338-1639  SAN FRANCISCO, CA    (415)956-0162
HACKENSACK, NJ       (201)487-3155  SAN JOSE, CA         (408)947-7606
HARTFORD, CT         (203)522-0003  SAN MATEO, CA        (415)579-6001
HAWTHORNE, NJ        (201)427-1100  SANTA ANA, CA        (714)972-9515
HINSDALE, IL         (312)986-0566  SEATTLE, WA          (206)382-0910
HOUSTON, TX          (713)224-9417  SKOKIE, IL           (312)679-8120
HUNTINGTON BEACH, CA (714)972-8515  SYRACUSE, NY         (315)474-3911
INDIANAPOLIS, IN     (317)635-6284  TOLEDO, OH           (419)243-1046
KANSAS CITY, KS      (913)621-3186  WASHINGTON, DC       (202)737-2051
LONG ISLAND, NY      (516)443-5402
LOS ANGELES, CA      (213)629-1026



























                                    Page 182




                        The Official Phreaker's Manual

                 Area Codes In Numerical Order, by The Jammer
______________________________________________________________________

201 Newark           New Jersey    519 London           Ontario
202 Washington D.C   (all)         601 Mississippi      (all)
203 Connecticut      (all)         602 Arizona          (all)
205 Alabama          (all)         603 New Hampshire    (all)
206 Seattle          Washington    605 South Dakota     (all)
207 Maine            (all)         606 Winchester       Kentucky
208 Idaho            (all)         607 Binghamton       New York
212 Bronx            Nyc, New York 608 Madison          Wisconsin
212 Manhattan        Nyc, New York 609 Trenton          New Jersey
213 Los Angeles      California    612 St. Paul         Minnesota
214 Dallas           Texas         613 Ottawa           Ontario
215 Philadelphia     Pennsylvania  614 Columbus         Ohio
216 Cleveland        Ohio          615 Nashville        Tennessee
217 Springfield      Illinois      616 Grand Rapids     Michigan
218 Duluth           Minnesota     617 Boston           Massachusetts
219 Gary             Indiana       618 Alton            Illinois
301 Maryland         (all)         619 San Diego        California
303 Colorado         (all)         700 Teleconference   (all)
304 West Virginia    (all)         701 North Dakota     (all)
305 Miami            Florida       702 Nevada           (all)
305 Orlando          Florida       703 Alexandria       Virginia
307 Wyoming          (all)         704 Charlotte        North Carolina
308 Abott            Nebraska      705 North Bay        Ontario
309 Peoria           Illinois      712 Councilbluffs    Iowa
312 Chicago          Illinois      713 Houston          Texas
313 Detroit          Michigan      714 Anaheim          California
314 St. Louis        Missouri      715 Bay City         Wisconsin
315 Syracuse         New York      716 Buffalo          New York
316 Wichita          Kansas        716 Rochester        New York
317 Indinapolis      Illinois      717 Harrisburg       Pennsylvania
318 Lake charles     Lousiana      800 Toll Free        (all)
319 Davenport        Iowa          801 Utah             (all)
401 Rhode Island     (all)         802 Vermont          (all)
402 Omaha            Nebraska      803 South Carolina   (all)
404 Atlanta          Georgia       804 Richmond         Virgina
405 Oklahoma City    Oklahoma      805 Bakersfield      California
406 Montana          (all)         806 Amarillo         Texas
408 San Jose         California    807 Thunder Bay      Ontario
412 Pittsburg        Pennsylvania  808 Hawaii           (all)
413 Springfield      Massachusetts 809 Bermuda          (all)
414 Milwaukee        Wisconsin     809 Bahamas          (all)
415 San Francisco    California    809 Puerto Rico      (all)
416 Toronto          Onterio       809 Virgin Islands   (all)
417 Joplin           Missouri      812 Evansville       Indiana
418 Quebec           Quebec        812 Dade park        Kentucky
419 Toledo           Ohio          814 Johnston         Pennsylvania
501 Arkansas         (all)         815 Rockford         Illinois
502 Frankfort        Kentucky      816 Independence     Missouri
503 Oregon           (all)         817 Fort Worth       Texas
504 New Orleans      Louisiana     818 Burbank          California
504 Baton Rouge      Louisiana     819 Trois Riv.       Quebec
505 New Mexico       (all)         900 Dial-it          (all)
507 Rochester        Minnesota     901 Memphis          Tennessee
509 Pullman          Washington    904 Talahassee       Florida
512 Austin           Texas         906 Escanaba         Michigan

                                    Page 183




                        The Official Phreaker's Manual

513 Cincinnati       Ohio          907 Alaska           (all)
514 Montreal         Quebec        912 Savannah         Georgia
515 Des Moines       Iowa          913 Kansas  City     Kansas
516 Hempstead        New York      915 El Paso          Texas
517 Lansing          Michigan      916 Sacramento       California
518 Albany           New York      918 Tulsa            Oklahoma
                                   919 Raleigh          North Carolina




















































                                    Page 184




                        The Official Phreaker's Manual

==Phrack Inc.==
Volume One, Issue Two, Phile #5 of 9

Updated from November 26, 1985
Tac Dialups taken from Arpanet
by Phantom Phreaker

                   TAC DIALUPS SORTED BY LOCATION 26-NOV-85

State/Country         300 Baud             1200 Baud              1200 Type
-------------      ---------------       -----------------        ---------

  ALABAMA
   Anniston Army Depot [M]
   (ANNIS-MIL-TAC)   (205) 235-6285 (R4)    (205) 235-7650               B/V
                     (205) 237-5731 (R8)    (205) 237-5731 (R8)          B/V
                     (205) 237-5770 (R8)    (205) 237-5779 (R8)          B/V
                     (205) 237-5805 (R8)    (205) 237-5805 (R8)          B/V

   *Please note:  When accessing the Anniston TAC you must first enter a
   <RETURN>, then enter DDN <RETURN>.  After you receive CLASS DDN START,
   proceed as normal.

   Gunter AFS [M]

   (GUNTER-TAC)      (205) 279-3576
                     (205) 279-4682

   Redstone Arsenal [M]
   (MICOM-TAC)       [none known]

  ARIZONA
   Ft. Huachuca [M]
   (HUAC-MIL-TAC)    [none known]

   Yuma [M]
   (YUMA-TAC)        (602) 328-2186         (602) 328-2186               B/V
                     (602) 328-2187         (602) 328-2187               B/V
                     (602) 328-2188         (602) 328-2188               B/V

  CALIFORNIA (NORTHERN)
   Alameda [M]
   (ALAMEDA-MIL-TAC)     [none known]

   Menlo Park [M]
   (SRI-MIL-TAC)     (415) 327-5440 (R3)    (415) 327-5440 (R3)          B

   (USGS3-TAC) [M]   [no dialups]

   Moffett Field [M]
   (AMES-TAC)        [no dialups; contact NSC for access]
                     William Jones - (415) 694-6482
                                     (FTS) 494-6482
                                      (AV) 359-6482

   Monterey [M]
   (NPS-TAC)         [none known]


                                    Page 185




                        The Official Phreaker's Manual

   Sacsamento [M]
   (MCCLELLAN1-MIL-TAC)   [none known]
   (MCCLELLAN2-MIL-TAC)   [none known]

   Stanford [A]
   (SU-TAC)          (415) 327-5220

  CALIFORNIA (SOUTHERN)
   China Lake [M]
   (NWC-TAC)         [none known]


   Edwards AFB [M]
   (EDWARD-MIL-TAC)  [none known]

   El Segundo [M]
   (AFSC-SD-TAC)     (213) 643-9204     (213) 643-9204                  B/V

   Los Angeles [A]
   (USC-TAC)         (213) 749-5436

   Los Angeles [A]
   (USC-ARPA-TAC)    [none known]

   San Diego [M]
   (ACCAT-TAC)   (619) 225-1641 (R4)    (619) 225-6903                  V
                 (619) 225-6946 (R3)
                                        (619) 223-2148                  V
                 (619) 226-7884 (R2)

   Santa Monica
   (RAND-ARPA-TAC) [A]
                 (213) 393-9230
                 (213) 393-9237
                 (213) 393-9238
                 (213) 393-9239

   (RAND2-MIL-TAC) [M]   [none known]

  COLORADO
   Denver Fed Ctr [M]
   (USGS2-TAC)       (303) 232-0206         (303) 232-0206              B/V

   Lowry Air Force Base [M]
   (LOWRY-MIL-TAC)   [none known]

  D.C.
   Washington
    [Andrews AFB] [M]
   (AFSC-HQ-TAC)  (301) 967-7930 (R16)     (301) 967-7930 (R16)         B
                  (301) 736-2990 (R4)      (301) 736-2990 (R4)          B
                  (301) 736-2998 (R2)      (301) 736-2998 (R2)          B

   (PENTAGON-TAC) (202) 553-0229 (R14)  (202) 553-0229 (R14)            B

  FLORIDA
   Eglin AFB [M]
   (AFSC-AD-TAC)     (904) 882-8202         (904) 882-8202              B/V

                                    Page 186




                        The Official Phreaker's Manual

                     (904) 882-8201         (904) 882-8201              V

   MacDill AFB [M]
   (MACDILL-MIL-TAC)  [none known]

   Naval Air Station - Jacksonville [M]
    (JAX1-MIL-TAC)    [none known]

   Naval Air Station - Orlando [M]
    (ORLANDO-MIL-TAC) [none known]

  GEORGIA
   Robins AFB [M]
   (ROBINS-TAC)      (912) 926-2725         (912) 926-2725              B/V
                     (912) 926-2726
                     (912) 926-3231
                     (912) 926-3232
                     (912) 926-2204         (912) 926-2204              B/V
   HAWAII
   Camp H.M. Smith [M]
   (HAWAII2-TAC)     (808) 487-5545         (808) 487-5545              B

  ILLINOIS
   Scott AFB [M]
   (SCOTT-TAC)       [none known]

   (SCOTT2-MIL-TAC)  [none known]

  KANSAS
   Ft. Leavenworth [M]
   (LVN-MIL-TAC)     (913) 651-7041 (R8)  (913) 651-7041 (R8)           B

  LOUISIANA
   Navy Regional Data Automation Center [M]
   (NORL-MIL-TAC)    (504) 944-7940       (504) 944-7940                B
                     (504) 944-7948 (R2)  (504) 944-7948 (R2)           B
                     (504) 944-7951 (R5)  (504) 944-7951 (R5)           B
                     (504) 944-8702 (R8)  (504) 944-8702 (R8)           B

  MARYLAND
   Aberdeen Proving Ground [M]
   (BRL-TAC)      (301) 278-6916 (R4)   (301) 278-6916 (R4)             B/V

   Bethesda [M]
   (DAVID-TAC)    (202) 227-3526 (R16)  (202) 227-3526 (R16)            B/V

   Patuxent River [M]
   (PAX-RV-TAC)      (301) 863-4815        (301) 863-4815               B/V
                     (301) 863-4816        (301) 863-4816               B/V
                     (301) 863-5750 (R6)   (301) 863-5750 (R6)          B/V

   Silver Spring [M]
   (WHITEOAK-MIL-TAC)   (301) 572-5960 (R10)   (301) 572-5960 (R10)     B
                        (301) 572-5970 (R10)   (301) 572-5970 (R10)     B

  MASSACHUSETTS
   Hanscom AFB [M]
   (AFGL-TAC)     (617) 861-3000 (R8)   (617) 861-3000 (R8)             B

                                    Page 187




                        The Official Phreaker's Manual

                  (617) 861-4965 (R8)   (617) 861-4965 (R8)

   Cambridge
   (BBN-MIL-TAC) [M]   [none known]

   (BBN-ARPA-TAC) [A]  [no dialup capability]

   (CCA-ARP-TAC) [A]   [none known]

   (MIT-TAC) [A]
                        (617) 491-5669        (617) 258-6224            V
                        (617) 491-5708        (617) 258-6225            V
                        (617) 491-5734        (617) 258-6227            V
                        (617) 491-5819        (617) 258-6248            V
                        (617) 491-5826
                        (617) 491-5841
                        (617) 491-5849
                        (617) 491-6769
                        (617) 491-6772
                        (617) 491-6937
                        (617) 258-6241
                        (617) 258-6242
                        (617) 258-6243

  MICHIGAN
   U.S. Army Tank Automotive Command (TACOM) - Warren [M]
   (TACOM-TAC)       [none known]

  MISSOURI
   St. Louis [M]
   (STLA-TAC)        [none known]

  NEBRASKA
   Offutt AFB [M]
   (SAC1-MIL-TAC)    [none known]

   (SAC2-MIL-TAC)    (402) 292-4638 (R10)   (402) 292-4638 (R10)         B

   (SAC-ARPA-TAC) [A]
                     (402) 294-2398         (402) 294-2398               B
                     (402) 291-2018         (402) 291-2018               B
                     (402) 292-7054         (402) 292-7054               B

  NEW JERSEY
   Dover [M]
   (ARDC-TAC)        (201) 724-6731         (201) 724-6731               B/V
                     (201) 724-6732         (201) 724-6732               B/V
                     (201) 724-6733         (201) 724-6733               B/V
                     (201) 724-6734         (201) 724-6734               B/V

   Fort Monmouth [M]
   (FTMONMOUTH1-MIL-TAC)   (201) 544-2052         (201) 544-2052         B/V
                           (201) 544-2062         (201) 544-2062         B/V
                           (201) 544-2072         (201) 544-2072         B/V
                           (201) 544-2396         (201) 544-2396         B/V
                           (201) 544-2430         (201) 544-2430         B/V

   (FTMONMOUTH2-MIL-TAC)   (201) 544-4254 (R3)    (201) 544-2430         B

                                    Page 188




                        The Official Phreaker's Manual

                                                  (201) 544-2636         B
                                                  (201) 544-2638         B
          (201) 544-2777         B

  NEW MEXICO
   Albuquerque [M]
   (AFWL-TAC)        [none known]

  White Sands [M]
   (WSMR-TAC)       [no dialups; contact NSC for access]
                    Claude (Skeet) Steffey - (505) 678-1271
                                             (FTS) 898-1271
                                              (AV) 258-1271

  NEW YORK
   Griffiss AFB
   (RADC-ARPA-TAC) [A] [no dialup capability]

   (RADC-TAC) [M]
                     (315) 339-4913 (R5)
                     (315) 337-2004           (315) 337-2004              B/V
                     (315) 337-2005           (315) 337-2005              B/V

                     (315) 330-2294           (315) 330-2294  (FTS) 952   B/V

                     (315) 330-3587           (315) 330-3587  (FTS) 952   B/V

  NORTH CAROLINA
   Ft. Bragg [A]
   (BRAGG-ARPA-TAC)  (919) 396-1131 (R10)     (919) 396-1426  (R5)        B/V
                                              (919) 396-1491  (R8)        B/V
   Ft. Bragg [M]
   (BRAGG-MIL-TAC)   [none known]

  OHIO
   Wright-Patterson AFB [M]
   (WPAFB-TAC)       (513) 258-4218
                     (513) 258-4219
                     (513) 258-4987
                     (513) 258-4988
                     (513) 258-4989
                     (513) 258-4990

   (WPAFB2-MIL-TAC)  (513) 257-2172 (R8)     (513) 257-2172 (R8)        B
                     (513) 257-2690 (R8)     (513) 257-2690 (R8)        B
                     (513) 257-3625 (R8)     (513) 257-3625 (R8)        B

  OKLAHOMA
   Tinker AFB [M]
   (TINKER-MIL-TAC)  [none known]


  PENNSYLVANIA
   New Cumberland Army Depot [M]
   (NCAD-MIL-TAC)    [none known]

   (NCAD2-MIL-TAC)   [none known]


                                    Page 189




                        The Official Phreaker's Manual

  TEXAS
   Brooks AFB [M]
   (BROOKS-AFB-TAC)  (512) 536-3081 (R6)  (512) 536-3081 (R6)              B/V

   Richardson [A]
   (COLLINS-TAC)     (214) 235-2131       (214) 235-2131                   B
                     (214) 235-2143       (214) 235-2143                   B
                     (214) 235-2178       (214) 235-2178                   B
                     (214) 235-2204       (214) 235-2204                   B
                     (214) 235-2251       (214) 235-2251                   B
                     (214) 235-2278       (214) 235-2278                   B

  UTAH
   Dugway Proving Ground [M]
   (DUGWAY-MIL-TAC)  [none known]

   Salt Lake City (University of Utah) [A]
   (UTAH-TAC)        (801) 581-3486       (801) 581-3486                   B/V

  VIRGINIA
   Alexandria [M]
   (DARCOM-TAC)      (202) 274-5300       (202) 274-5300                   B
                     (202) 274-5320 (R6)  (202) 274-5320 (R6)              B

   Arlington
   (ARPA1-MIL-TAC) [M]   [none known]

   (ARPA2-MIL-TAC) [M]   [none known]

   (ARPA3-TAC) [A]   [no dialup capability]

   Dahlgren [M]
   (NSWC-TAC)        (703) 663-2162 (R8)     (703) 663-2162 (R8)          B

   Langley Air Force Base [M]
   (LANGLEY-MIL-TAC) [none known]

   McLean [M]
   (DDN-PMO-MIL-TAC) [none known]


   (MITRE-TAC) [M]
                     (703) 442-8020 (R15)
                     (703) 893-0330 (R10)    (703) 893-0330 (R10)         B/V

   Norfolk [M]
   (NORFOLK-MILTAC)  (804) 423-0241 (R2)     (804) 423-0241 (R2)          B
                     (804) 423-0247 (R2)     (804) 423-0247 (R2)          B
                     (804) 423-0346 (R4)     (804) 423-0346 (R4)          B
                     (804) 423-0480          (804) 423-0480               B
                     (804) 423-0486 (R2)     (804) 423-0486 (R2)          B
                     (804) 423-0489          (804) 423-0489               B
                     (804) 423-0570          (804) 423-0570               B
                     (804) 423-0572 (R2)     (804) 423-0572 (R2)          B
                     (804) 423-0577 (R2)     (804) 423-0577 (R2)          B
                     (804) 423-0651          (804) 423-0651               B
                     (804) 423-0654 (R3)     (804) 423-0654 (R3)          B
                     (804) 423-0841 (R2)     (804) 423-0841 (R2)          B

                                    Page 190




                        The Official Phreaker's Manual

                     (804) 423-0845          (804) 423-0845               B
                     (804) 423-0849          (804) 423-0849               B
                     (804) 423-0858          (804) 423-0858               B
                     (804) 423-0950          (804) 423-0950               B
                     (804) 423-0952          (804) 423-0952               B
                     (804) 423-0955 (R3)     (804) 423-0955 (R3)          B
                     (804) 423-0959          (804) 423-0959               B

   Reston
   (DCEC-ARPA-TAC) [A]   [no dialups available]

   (DCEC-MIL-TAC) [M]
                     (703) 437-2892 (R5)     (703) 437-2928               B
                     (703) 437-2925          (703) 437-2929               B
                     (703) 437-2926
                     (703) 437-2927

  WASHINGTON
   Seattle [A]
   (WASHINGTON-TAC)  [no dialup capability]

  ENGLAND [M]
   (CROUGHTON-MIL-TAC)   [none known]

  GERMANY [M]
   (FRANKFURT-MIL-TAC)
                     (M) 2311-5641 (R8)                                   B

   (RAMSTEIN2-MIL-TAC) [none known]

  ITALY [M]
   (AGNANO-MIL-TAC)

  JAPAN [M]
   (BUCKNER-MIL-TAC)

   (ZAMA-MIL-TAC)

  KOREA [M]
   (KOREA-TAC)       (M) 264-4951 (R8)                                    B

  PHILIPPINES [M]
   (CLARK-MIL-TAC)

  SPAIN [M]
   (MILNET-TJN-TAC)  [none known]

   (ROTA-MIL-TAC)    [none known]

  Notes:

  1.  "(R10)" following phone number indicates a rotary with 10 lines.

  2.  For alternate phone numbers, FTS=Federal Telephone System.
  3.  (M)=Military DoD Telephone System.

  4.  [M] denotes a MILNET TAC and [A] denotes an ARPANET TAC.


                                    Page 191




                        The Official Phreaker's Manual

  5.  "1200 Type" refers to the modem compatibility for 1200 baud only:
       B/V =  Bell and Vadic
       B   =  Bell 212A only
       V   =  Vadic 3400 only

  6.  This list is contained in the file NETINFO:TAC-PHONES.LIST at
      SRI-NIC.




















































                                    Page 192




                        The Official Phreaker's Manual

                        >>==========================<<
                        >>==> TELCO TEST NUMBERS <==<<
                        >>====> as of 5/16/85 <=====<<
                        >>=> compiled and updated <=<<
                        >>====> by Shadow 2600 <====<<
                        >>==========================<<

011-44-61-2468011 : US dial tone then "When this system changes, this is the
new dial tone you hear" (UK is changing dialtone)

201-226-0709 : alternating tones, then "warble"
201-267-9922 : sweep tone
201-267-9966 : 600 ohm termination
201-232-9924 : (tone 1,2,5-beep, bleep; 9,#- 1200 baud static, beep, bleep;
6-tone, higher tone, bleep)
201-232-9959 : tone 11 sec. silence, repeats...
201-233-9972 : multitude of clicks
201-233-9974 : busy 15 sec. then tone w/ clicks
201-241-9916 : hissing with clicks
201-328-9971 : 1000 hrtz tone
201-376-9907 : "is being checked for trouble.  Please try again later"
201-464-9915 : low tone 15 sec, silence
201-464-9916 : low tone 2 sec, silence
201-464-9963 : buzz
201-464-9974 : busy 15 sec, low tone
201-543-9902 : "If you'd like to make a call, hang up and try it again."
201-543-9903 : "We're sorry, your call did not go through."
201-543-9904 : "the number you have dialed requires a .20 cents deposit."
201-655-9900 : "cannot be completed as dialed from the phone you are using"
201-769-0205 : People's Express Reservation system
203-771-4920 : telephone company employee newsline
207-866-4411 : 1000 hrtz tone
212-233-9980 : (tone 1,2,3,*-tone, higher tone, bloop; 5-tone, bloop; 9,#-
static,beep,bloop)
212-369-7003 : "you have reached 212-369-7003 in zone 3" (?)
212-799-5017 : ABC New York feed line
213-621-4141 : telephone employee newsline
213-935-1111 : sweep tone with echo at top of range (?)
215-489-0036 : tone, bloop (1,2,5-tone bloop, 3,6,9-tone, higher tone,tone)
215-489-0040 : "please check your instruction manual or call repair service for
assistance"
215-489-0042 : "if you like to make a call please hang up and try again"
215-489-0043 : "We're sorry, your call did not go through."
215-489-0044 : "The call you have made requires a 25 cent deposit"
215-489-0045 : "You must first dial a 1 when dialing this number."
215-489-0074 : LOUD tone, stops, repeats
215-489-0075 : 600 ohm termination (silence)
215-489-0078 : tone, silence
215-489-0080 : 600 ohm termination
215-489-0097 : tone, (lower pitched than -0078) silence (also at -0098)
215-489-0104 : 1000 hrtz tone
216-861-8300 : tone, then higher tone
301-256-9987 : 1000 hertz
301-546-7777 : "Due to Telephone Company facility trouble your call cannot be
completed at this time"
301-725-9904 : "deposit .20"
305-263-0000 : repeating bloop (keypress 2 : slow reorder w/ bloops, clicks)
305-994-9963 : pay fone instructions

                                    Page 193




                        The Official Phreaker's Manual

305-994-9966 : "telephone you are calling from is not in service"
312-222-9948 : tone (keypress 1,2,3,6,7,*-tone, high tone, bleep,
4-tone,bloop,9, #-static,beep,bloop)
312-222-9954 : "Test Center"
312-222-9990 : clicks, ticking like
312-222-9996 : LOUD tone, repeats
312-368-8000 : Illinois Bell Communicator (employee newsline)
312-592-0000 : tone (keypress 2222, then other digits, at re-order type * to
restart) (?)
313-223-7223 : telephone employee newsline
313-333-9981 : LOUD tone, silence
313-333-9989 : high tone (enter touchtones for a while, eventually get
"metallic" echo, then 5-high pitched tone, random re-orders)
313-333-9990 : beep, click repeats, with "winks"
313-333-9994 : tone bloop (keypress in 2-tone,bloop, 3-tone, higher tone,tone,
9-static, beep,bloop)
313-333-9995 : 600 ohm termination (silence)
313-333-9996 : weird siren/sweep tone, multi-frequency
313-430-4300 : beep, beep, beep, then reorder
313-698-9998 : sweep tone
314-247-5511 : Southwestern Bell Telenews (employee newsline)
315-471-9934 : "deposit 5 cents for next five minutes"
408-255-0081 : (any two 2,4,8,0-tone)
408-294-6969 : beep, click, computer voice repeats number
408-395-1110 : (tone 2-bleep,glitch; 3-beep,higher beep;#then number-loud
tone,bleep)
408-738-8190 : (tone 1,3,6,7,*-tone, high tone, tone;2-beep,cluck;9,#-
static,tone,beep)
408-745-6060 : high pitched tone, low tone then repeats
408-994-0044 : tone end of loop
412-633-3333 : telephone company employee newsline
414-628-0001 : continuous tone
414-628-0002 : continuous tone (higher pitched, sounds like muted dial)
414-628-0004 : high pitched tone, bloop, silence
414-628-0006 : brief very high tone (also -0007) (multiple keypresses of
2,5,8,0 tone repeats)
414-628-0010 : loud tone, stops, repeats...
414-628-0011 : loud tone, stops
414-628-0013 : 600 ohm termination (silence) (also -0017, two in an exchange?)
414-628-0014 : continuous tone (sounds like weird dial), eventually stops
414-628-0015 : LOUD tone, repeats
414-628-0028 : "Your call cannot be completed as dialed
414-678-3511 : Wisconsin Bell Newsline
414-781-0004 : high tone, silence (keypress 2,5-beep,bleep, 3,6-beep,longbeep,
bloop, 9-static,bloop)
415-284-1111 : one sweep, then silence
415-327-0046 : sweep tone
415-388-0037 : tone,bloop (keypress 2-tone,bloop, 3-tone,high tone,tone,
9-static,beep,bloop)
415-472-0046 : sweep w/ glitch at top
415-545-8800 : Pacific Bell Newsline
415-467-0097 : fast DTMF tones, keypress to repeat
415-777-0020 : 1000 hrtz tone
415-777-0037 : tone, bloop (keypress 2-beep,bloop, 3,6-tone,higher tone,
9-static,beep,bloop)
415-777-0046 : sweep tone with echo
415-777-0105 : tone,bloop (keypress 2-beep,bleep, 3,6-tone, higher tone,
tone,9-static,beep,bloop

                                    Page 194




                        The Official Phreaker's Manual

415-826-0022 : tone, click, tone (sounds like a busy)
415-994-0710 : multitude of clicks
512-472-2181 : "if you would like to make a call, please hang up and try
again"
512-472-4263 : garbled recording (?)
512-472-9833 : "you must first dial a 1 or 0 before calling this number"
512-472-9936 : "please check your instructions or call your business office for
assistance"
512-472-9941 : "insert 25 cents"
516-222-3825 : LOUD tone
516-234-9914 : New York Telephone Newsline
518-471-2272 : New York Telephone Newsline
518-789-3299 : weird busy, multitude of clicks
609-267-9966 : busy with clicks in background
609-267-9967 : 600 ohm termination (silence)
609-267-9968 : 1000 hrtz tone
609-267-9971 : LOUD tone, stops, repeats
609-267-9972 : rings with clicks in background (also -9973 and -9974)
609-877-9924 : high tone (tone in 1,2,5-tone, bloop; 3,6,*-tone, higher tone,
bleep; #-static, beep, bleep)
609-877-9929 : 1000 hrz tone
617-553-9953 : tone end of loop
617-890-9900 : sweep tone
617-955-1111 : telephone company employee newsline
619-748-0002 : tone increases in pitch, silence, repeats in monotone
619-748-0003 : sweep, repeat, hangs up
702-789-6711 : Nevada Bell Newsline
713-354-0000 : touch tone in #, then new #, then 5 - listed, 9 - unlisted)
713-482-3199 : "We're sorry, all circuit are busy now."
713-652-5111 : touch tones echo back "metallic", something about "drivers
licence number" replys in a female recorded voice
717-255-5555 : Bell of Pennsylvania "Inside Line" (employee newsline)
718-429-9900 : "Please slide a valid credit card through the slot now"
800-221-5959 : tone (# makes it ring)
800-228-8466 : Sensaphone (tm) demo (time etc. (EST) (wait 7+ rings))
800-321-3048 : non-connecting loop with 800-321-3049
800-321-3052 : loop (don't know where other end is)
800-321-6366 : Centagram's Voice Memo System (extension 100 for demo)
800-323-6321 : tone, stops, bloop repeats
800-327-0000 : "Announcement three, Dallas" (changes sometimes)
800-344-4001 : non-connecting loop with 800-344-4002
800-524-0000 : "Announcement 1 Atlanta"
800-554-5924 : Cable News Network audio feed
800-824-8274 : "Enter your password service code"
802-955-1111 : telephone company newsline
808-533-4426 : Hawaiian Telephone Newsline
816-391-1122 : recorder (keypress 1-toggle on/off, 3-rewind, 4-stop, 7-play)
907-269-0955 : tone (sounds like extender, doesn't take touch tone (?))
914-232-9901 : "Daytona, New York DMS-100 verification"
914-268-9901 : "Congers DMS 100 Verification"
914-268-9903 : "your call cannot be completed as dialed"
914-268-9968 : (keypress 2-high tone, 3-high, higher tone, 6,0-click, 7- hangs
up, sometimes 0,#,*-harmony)
914-359-9901 : repeats the number dialed ("914-359-9901")
914-359-9960 : weird tone, stops, clicks, repeats
914-623-9968 : (keypress 2,5-beep glitch, 3,6-tone highertone)
916-480-8000 : Pacific Bell Newsline


                                    Page 195




                        The Official Phreaker's Manual

                        WHAT A TSPS CONSOLE LOOKS LIKE

--- NON/COIN ---- ------------- COIN ------------- --------- HOTEL ---------

 ----   ----   ----   ----   ----    ----   -----   ---       ---    ----
!VFY ! !OVER! !SCRN! !INWD! !EMER!  !STA ! ! 0+ ! !DIAL!     !STA ! ! 0+ !
!DIAL! !POST! !TONE! !STA ! ! 0+ !  !DIAL! !QST ! !    !     !    ! !    !
 ----   ----   ----   ----   ----    ----   ----   ----       ----   ----

----- OUTGOING TRUNKS -----    RING RELEASE

 ----   ----   ----   ----   ----   -----   ----   ----   ----   ----
! DA ! !R&R ! !SWB ! !OGT ! !BACK! ! FWD ! !CALL! !T&C ! !NFY ! !CHG !
 ----   ----   ----   ----   ----   -----   ----   ----   ----  ! DUE!
                                                                 ----
 ---    ----   ----   ----   ----   ----   ----   ----   ----   ----
!KEY ! !BACK! !FWD ! ! SR ! !MAKE! !MTCE! !POS ! !BACK! !    ! !    !
!CLG ! !    ! !    ! !    ! !BUSY! !TRFR!  ----   ----   ----   ----
 ----   ----   ----   ----   ----   ----

              ----------------- AMA -----------------
              ----   ----   ----   ----   ----   ----
STATION -----!PAID! !COL ! !SPL ! !SPL ! !AUTO! !DDD !
             !    ! !    ! !CLG ! !CLD ! !COL ! !    !
              ----   ----   ----   ----   ----   ----

              ----   ----   ----   ----          ----
PERSON ----- !PAID! !COL ! !SPL ! !SPL !        ! NO !
             !    ! !    ! !CLG ! !CLD !        !AMA !
              ----   ----   ----   ----          ----

               ----         ----         ----
              !CLG !       !CLG !       !CLG !
              !    !       !    !       !    !
               ----         ----         ----
























                                    Page 196




                        The Official Phreaker's Manual

                                   Box Plans

   Hmm...  I wonder!  This is still under construction (Ha Ha).
























































                                    Page 197




                        The Official Phreaker's Manual

                           THE INFINITY TRANSMITTER

                            TYPED BY THE GHOST WIND

                         FROM THE BOOK BUILD YOUR OWN
         LASER, PHASER, ION RAY GUN & OTHER WORKING SPACE-AGE PROJECTS
                       BY ROBERT IANNINI (TAB BOOKS INC)

Description:  Briefly, the Infinity Transmitter is a device which activates a
microphone via a phone call.  It is plugged into the phone line, and when the
phone rings, it  will immediately intercept the ring and broadcast into the
phone any sound that is in the room. This device was originally made by
Information Unlimited, and had a touch tone decoder to prevent all who did not
know the code from being able to use the phone in its normal way.  This
version, however, will activate the microphone for anyone who calls while it is
in operation.
NOTE:  It is illegal to use this device to try to bug someone. It is also
pretty stupid because they are fairly noticeable.
Parts List:
Pretend that uF means micro Farad, cap= capacitor

Part           #          Description
----           -          -----------
R1,4,8         3         390 k 1/4 watt resistor
R2             1         5.6 M 1/4 watt resistor
R3,5,6         3         6.8 k 1/4 watt resistor
R7/S1          1         5 k pot/switch
R9,16          2         100 k 1/4 watt resistor
R10            1         2.2 k 1/4 watt resistor
R13,18         2         1 k 1/4 watt resistor
R14            1         470 ohm 1/4 watt resistor
R15            1         10 k 1/4 watt resistor
R17            1         1 M 1/4 watt resistor
C1             1         .05 uF/25 V disc cap
C2,3,5,6,7     5         1 uF 50 V electrolytic cap or tant
                          (preferably non-polarized)
C4,11,12       3         .01 uF/50 V disc cap
C8,10          2         100 uF @ 25 V electrolytic cap
C9             1         5 uF @ 150 V electrolytic cap
C13            1         10 uF @ 25 V electrolytic cap
TM1            1         555 timer dip
A1             1         CA3018 amp array in can
Q1,2           2         PN2222 npn sil transistor
Q3             1         D4OD5 npn pwr tab transistor
D1,2           2         50 V 1 amp react. 1N4002
T1             1         1.5 k/500 matching transformer
M1             1         large crystal microphone
J1             1         Phono jack optional for sense output
WR3            (24")     #24 red and black hook up wire
WR4            (24")     #24 black hook up wire
CL3,4          2         Alligator clips
CL1,2          2         6" battery snap clips
PB1            1         1 3/4x4 1/2x.1 perfboard
CA1            1         5 1/4x3x2 1/8 grey enclosure fab
WR15           (12")     #24 buss wire
KN1            1         small plastic knob
BU1            1         small clamp bushing
B1,2           2         9 volt transistor battery or 9V ni-cad

                                    Page 198




                        The Official Phreaker's Manual


Circuit Operation: Not being the most technical guy in the world, and not being
very good at electronics (yet),  I'm just repeating what Mr. Iannini's said
about the circuit operation.  The Transmitter consists of a high grain
amplifier fed into the telephone lines via transformer.  The circuit is
initiated by the action  of  a voltage transient pulse occurring across  the
phone line  at the instant the telephone circuit is made (the ring,  in other
words).  This transient immediately triggers a timer  whose output  pin  3 goes
positive, turning on transistors Q2 and  Q3. Timer TM1 now remains in this
state for a period depending on the values  of R17 and C13 (usually about 10
seconds for  the  values shown). When Q3 is turned on by the timer, a simulated
"off hook" condition is created by the switching action of Q3 connecting the
500  ohm  winding  of the transformer directly across  the  phone lines.
Simultaneously, Q2 clamps the ground of A1, amplifier, and Q1, output
transistor, to the negative return of B1,B2, therefore enabling this amplifier
section.  Note that B2 is always required by  supplying  quiescent power to TM1
during  normal conditions. System is off/on controlled by S1 (switch).
  A  crystal mike picks up the sounds that are fed to  the  first two
transistors of the A1 array connected as an emitter follower driving the
remaining  two  transistors  as  cascaded   common emitters. Output of the
array now drives Q1 capacitively coupled to  the  1500 ohm  winding of  T1.
R7  controls  the  pick  up sensitivity of the system.
  Diode  D1  is  forward biased at the instant of  connection  and essentially
applies a negative pulse at pin 2 of TM1,  initiating the cycle.   D2 clamps
any high positive pulses.   C9 dc-isolates and desensitizes the circuit. The
system described should operate when any incoming call is made without ringing
the phone.

Schematic Diagram:  Because this is text,  this doesn't look  too hot. Please
use  a little imagination!  I will hopefully get  a graphics drawing  of  this
out as soon as I  can  on  a  Fontrix graffile.

To be able to see what everything is, this character: | should appear as a
horizontal bar. I did this on a ][e using a ][e 80 column card, so I'm sorry if
it looks kinda weird to you.

Symbols:
 resistor: -/\/\/-            switch: _/ _
 battery:  -|!|!-             capacitor (electrolytic): -|(-
 capacitor (disc): -||-                   _    _
 transistor:(c)  > (e)        Transformer: )||(
              \_/                          )||(
               |(b)                       _)||(_
 diode: |<
 chip: ._____.
       !_____! (chips are easy to recognize!)

 Dots imply a connection between wires. NO DOT, NO CONNECTION.
ie.:  _!_ means a connection while _|_ means no connection.
----------------------------------------------------------------------------

.________________________to GREEN wire phone line
|
| .______________________to RED wire phone line
| |
| |     ._________(M1)______________.
| |     |                           |
| |     |           R1              |

                                    Page 199




                        The Official Phreaker's Manual

| |     !__________/\/\/____________!
| |     |                          _!_ C1
| |     |this wire is the amp      ___
| |     |<=ground                   |                     R2
| |     |                           !___________________/\/\/_____________.
| |     |                   ._______!_______.                             |
| |     !___________________!4      9     11!_____________________________!
| |     |                   |               |                             |
| |     !___________________!7            12._____________________________!
| |     |                   |     A1        |              R3             |
| |     !___________________!10       ____*8!_______.____/\/\/____________! ^
| |     |                   |        /      |       |                     | |
| |     |    C4             |       /       |       \                     |2ma
| |     !____||______.      |      /        |       /R4                B1 +
| |     |    ||      |      |     /         |       \                    |!|!
| |     |     R7     |  C2  |    /          |       /                     |
| |     !____/\/\/___!__)|__!8*_/           |       |                 S1  |
| |     |     ^             |              6!_______!           neg<__/.__!
| |     |     |     C3      |               |       | C5       return     |
| |     |     !_____|(___.__!3              |       '-|(-|                |
| |     |                |  |       5      1!____________!                |
| |     |                \  !_______._______!            |             B2|!|!
| |     !________.    R8 /          |                    |                +
| |              |       \          |                    |      R6        |3ma
| |              |       !__________!____________________|_____/\/\/______! |
| |              |    R5            |                    |                | v
| |              !__/\/\/___________|____________________!                |
| |              |                  |                                     |
| |              |                  |                                     |
| |              |               C6 |                                     |
| |              |             |-)|-'             R9                      |
| |              |             !_________________/\/\/_______.            |
| |              |             |                             |            |
| |              |         Q1 _!_                            |   R10      |
| |              !____________/ \____________________________!__/\/\/_____!
| |              |                                           |            |
| |              |                                           |            |
| |              |          C8                               |            |
| |              !__________)|_______________________________|____________!
| |              !                                           |            |
| |             /                                            |            |
| |       -----|                                             |            |
| |       |     \                                            |            |
| |       |      >                                           |            |
| |       |      |                                           |            |
| |       |      |                                           |            |
| |       |      !_____________.                             |            |
| |       |                    |                             |            |
| |       !__________.         |                             |            |
| |                  |         |                             |            |
| !________.         |         |                       ._____!            |
|          |         |         |                       |                  |
|          |         |         |                       |                  |
|          |         |         |                       | C7               |
|          |         |         |                       '-|(-|             |
|          |_________|_________!_______.T1._________________|             |
|                    |         |  1500 )||( 500                           |
|                    |         |   ohm )||( ohm                           |

                                    Page 200




                        The Official Phreaker's Manual

|                    |         !______.)||(.__.                           |
|                    |         |              |                           |
|                    |         |              |                           |
|                    |         |              >                           |
|                    |         |            |/                            |
|                    |         |       +----|   Q3                        |
|                    |         |       |    |\                            |
!____________________|_________|_______|______!__. D1   C9                |
                     |         |       |         '-|<---|(------|         |
      .______________!         |       |                        |         |
      |                        |       |                        |         |
      |       .________________!       |                        |         |
      |       |                        |                        |         |
      \       |       .________________!             C11        |         |
      /       |       |                       .___||____________!         |
  R13 \       |       |                       |   ||            |         |
      /       |       |                       |                 |         |
      \       !___.___|_______________________!                 |         |
      |       |   |   |                       |     R16         |    R15  |
      |       v   |   |                       !___/\/\/\________!___/\/\/_!
      |      neg  |   |                       |    D2           |         |
      |    return |   |                       !_____|<__________!         |
      |     B1,B2 |   \                       |                 |         |
      |           |   /                       |    .____________!_.       |
      |           |   \R14                    |C12 |   TM1      2 |       |
      |           |   /                       !_||_!5            4!_______!
      |           |   \                       | || |              |       |
      |           |   |                       !____!1            8!_______!
      |           |   |                       |    |     7 6   3  |       |
      |           |   |                       |    !_____._.____._!       |
      |           |   |                       |          | |    |         |
      |           |   |                       |   C13    | |    |   R17   |
      |           |   |                       !___)|_____!_!____|__/\/\/__!
      |           |   |                       |                 |         |
      !___________|___!_______________________|_________________!         |
                  |   |                       |                           |
                  |   \                       |          C10              |
                  |   /R18                    !__________)|_______________!
                  |   \
                  |   /
                  |   |
                  !___O J1
                    sense output

Construction notes: Because the d***!ed book just gave a picture instead of step
by step instructions, and I'll try to give you as much help as possible. Note
that all the parts that you will be using are clearly labeled in the schematic.
The perfboard, knobs, 'gator clips, etc are optional. I do strongly suggest
that you do use the board!!! It will make wiring the components up much much
easier than if you don't use it.
 The knob you can use to control the pot (R7). R7 is used to tune the IT so
that is sounds ok over the phone. (You get to determine what sounds good) By
changing the value of C13, you can change the amount of time that the circuit
will stay open (it cannot detect a hang up, so it works on a timer.) A value of
100 micro Farads will increase the time by about 10 times.
 The switch (S1) determines whether or not the unit is operational. Closed is
on. Open is off. The negative return is the negative terminals of the battery!!
The batteries will look something like this when hooked up:

                                    Page 201




                        The Official Phreaker's Manual

  <-v_____.   .______.    ._____.   .____->
          |   |      |    |     |   |
        __!___!__    |    |   __!___!__
        | +   - |    !_/ _!   | +   - |
        |       |  switch ^   |       |
        | 9volts|         |   | 9volts|
        !_______! neg return  !_______!

 To hook this up to the phone line, there are three ways, depending upon what
type of jack you have. If it is the old type (non modular) then you can just
open up the wall plate and connect the wires from the transmitter directly to
the terminals of the phone.
 If you have a modular jack with four prongs, attach the red to the negative
prong (don't ask me which is which! I don't have that type of jack... I've only
seen them in stores), and the green to the positive prong, and plug in. Try not
to shock yourself...
 If you have the clip-in type jack, get double male extension cord (one with a
clip on each end), and chop off one clip. Get a sharp knife and splice off the
grey protective material. You should see four wires, including one green and
one red. You attach the appropriate wires from the IT to these two, and plug
the other end into the wall.

Getting the IT to work: If you happen to have a problem, you should attempt to
do the following (these are common sense rules!!) Make sure that you have the
polarity of all the capacitors right (if you used polarized capacitors, that
is). Make sure that all the soldering is done well and has not short circuited
something accidently (like if you have a glob touching two wires which should
not be touching.) Check for other short circuits. Check to see if the battery
is in right. Check to make sure the switch is closed.
 If it still doesn't work, drop me a line on one of the Maryland or Virginia
BBSs and I'll try to help you out.

The sense output: Somehow or other, it is possible to hook something else up to
this and activate it by phone (like an alarm, flashing lights, etc.)

As of this writing, I have not tried to make one of these, but I will. If you
actually get it working, leave me a note somewhere.

I sure hope all you people appreciate this.


<<< the Ghost Wind >>>

















                                    Page 202




                        The Official Phreaker's Manual

    ::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
    :                                                                    :
    :            SILVER BOX:  AN ALTERNATE METHOD OF CONSTRUCTION        :
    :                                                                    :
    :                  BY:  THE LOCK LIFTER--1/25/85                     :
    :                                                                    :
    ::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::

PARTS & EQUIPMENT:
(1) POCKET TONE DIALER  (RADIO SHACK CAT. NO. 43-138)
(2) SINGLE POLE DOUBLE THROW SWITCH  (TOGGLE, THE SMALLER THE BETTER)
(3) SOLDERING IRON

     THIS MODIFICATION WILL ALLOW THE PRODUCTION OF A,B,C,&D TONES. WHEN YOU
FLIP THE SWITCH THE 3,6,9,&# KEYS WILL BECOME A,B,C,&D RESPECTIVELY.  THE IC
INSIDE THE DIALER IS CAPABLE OF MAKING THESE TONES ALREADY, ALL WE MUST DO IS
CONNECT IT FULLY.  THIS MOD CAN ALSO BE MADE TO MANY ELECTRONIC FONES THAT
CONTAIN A DTMF TONE ENCODING IC. THIS CHIP CAN BE IDENTIFIED BY THE NUMBER 5089
OR S2559 OR MK5380 OR TCM5087N.  PIN 9 OF THESE CHIPS IS THE FOURTH COLUMN
KEYPAD INPUT WHILE PIN 5 IS THE THIRD COLUMN.  NOW ON WITH THE CONSTRUCTION.

1)    REMOVE THE BATTERY COVER, BATTERIES, AND THE SMALL SCREW. THE CASE SHOULD
NOW POP OPEN WITH A LITTLE PRESSURE.
2)    OPEN THE CASE SO THAT THE HALF CONTAINING THE SPEAKER AND THE BATTERIES
IS ON YOUR LEFT WITH THE BATTERIES ON THE BOTTOM. YOU SHOULD NOW BE LOOKING AT
THE BACK OF 2 PRINTED CIRCUIT BOARDS.
3)  FIND THE TWO ROWS OF SOLDER BEADS WHERE THE IC IS CONNECTED.  THE UPPER
LEFT PIN OF THE 2 ROWS SHOULD HAVE NO SOLDER ON IT. THIS IS PIN 9 OF THE IC.
4)  ATTACH A SHORT WIRE TO PIN 9.
5)  SEE THE 8 GOLD WIRES GOING TO THE KEY PAD?  UNSOLDER THE ONE 4TH FROM THE
LEFT AND CONNECT IT TO A SHORT WIRE.
6)  SOLDER A SHORT WIRE INTO THE NOW VACANT HOLE IN THE KEYPAD PCB.
7)  MELT OR DRILL A ROUND HOLE IN THE PLASTIC CASE FOR THE SWITCH. THE BEST
PLACE FOR THIS IS OPPOSITE THE SMALL PCB CONTAINING THE L.E.D.
8)  INSERT THE SWITCH AND SCREW IT IN PLACE.
9)  ATTACH THE WIRE FROM THE KEYPAD PCB TO THE CENTER OF THE SWITCH. ATTACH THE
OTHER TWO WIRES TO THE OTHER TWO POLES OF THE SWITCH. JUST CLOSE THE CASE, PUT
BACK IN THE SCREW AND BATTERIES.

THE SWITCH WILL NOW ALLOW THE  3RD COLUMN KEYS TO PRODUCE BOTH 3RD AND FOURTH
COLUMN TONES.  HAVE PHUN


















                                    Page 203




                        The Official Phreaker's Manual


































             Well, this is just a page to protect the other pages.
                         I hope you enjoyed the book!
























                                    Page 204



Downloaded From P-80 International Information Systems 304-744-2253
