
	   	       | Basic NAM Programming |


By: The Clone
Date: Sunday March 26, 2000


1) This is test mode NAM Programming:

- Turn phone on
- FCN,0,0,*,*,8,3,7,8,6,6,3,3,RCL
- # to get to main test screen
- 55# to get to nam programming
- After done # to main screen and 01# to reset phone     


2) Normal NAM Programming if factory system code is the default:

- Turn phone on
- FCN,0,0,0,0,0,0,0,0,0,0,0,0,0,STO (13 zeros)
- * to move through NAM programming menu.
- To exit go back to the first NAM programming stage and hit SND 

END


http://nettwerk.hypermart.net
webmaster@nettwerk.hypermart.net
